System Report

Date | Mo 24 Feb 2020 17:16:36 CET
--- | ---
OS Version | 10.11.3
OS Build | 15D21
Model Name | iMac
Model Identifier | iMac14,2
Processor | Intel(R) Core(TM) i7-5820K CPU @ 3.30GHz
Total Number of Cores | 6
Memory | 32 GB
Graphics Card(s) | AMD Radeon RX480
Bootloader | Clover - UEFI r4097
| AppleHDA | is loaded

AppleALC | 1.1.2
--- | ---
FakeSMC | 685
GenericUSBXHCI | 1.2.7
Lilu | 1.1.4
USBInjectAll | 0.6.1
VoodooTSCSync | 1.1

AppleALC | EFI/CLOVER/kexts/Other
--- | ---
Apowersoft_AudioDevice | /Library/Extensions
CPUSensors | EFI/CLOVER/kexts/Other/FakeSMC.kext/Contents/PlugIns
FakeSMC | EFI/CLOVER/kexts/Other
GPUSensors | EFI/CLOVER/kexts/Other/FakeSMC.kext/Contents/PlugIns
GenericUSBXHCI | EFI/CLOVER/kexts/Other
Lilu | EFI/CLOVER/kexts/Other
LittleSnitch | /Library/Extensions
NullCPUPowerManagement | EFI/CLOVER/kexts/Other
TACC | /Library/Extensions
USBInjectAll | EFI/CLOVER/kexts/Other
VoodooTSCSync | EFI/CLOVER/kexts/Other
YamahaSteinbergUSBAudio | EFI/CLOVER/kexts/Other
fabio | /System/Library/Extensions
rtprotection |

Currently in use: |
--- | ---
standby | 0
Sleep On Power Button | 1
womp | 0
autorestart | 0
hibernatefile | /var/vm/sleepimage
powernap | 0
networkoversleep | 0
disksleep | 0
sleep | 0
autopoweroffdelay | 14400
hibernatemode | 0
autopoweroff | 1
ttyskeepawake | 1
displaysleep | 0
standbydelay | 10800

Vendor | Device | Sub Ven | Sub Dev | Device Information
--- | --- | --- | --- | ---
8086 | 2F81 | 1462 | 7885 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 R3 QPI Link 0 !LSPCI! 1 Monitoring
8086 | 2F81 | 1462 | 7885 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 R3 QPI Link 0 !LSPCI! 1 Monitoring
8086 | 2F36 | 1462 | 7885 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 R3 QPI Link 0 !LSPCI! 1 Monitoring
8086 | 2F36 | 1462 | 7885 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 R3 QPI Link 0 !LSPCI! 1 Monitoring
8086 | 2F37 | 1462 | 7885 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 R3 QPI Link 0 !LSPCI! 1 Monitoring
8086 | 2F37 | 1462 | 7885 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 R3 QPI Link 0 !LSPCI! 1 Monitoring
8086 | 2FE0 | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Unicast Registers
8086 | 2FE0 | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Unicast Registers
8086 | 2FE1 | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Unicast Registers
8086 | 2FE1 | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Unicast Registers
8086 | 2FE2 | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Unicast Registers
8086 | 2FE2 | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Unicast Registers
8086 | 2FE3 | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Unicast Registers
8086 | 2FE3 | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Unicast Registers
8086 | 2FE4 | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Unicast Registers
8086 | 2FE4 | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Unicast Registers
8086 | 2FE5 | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Unicast Registers
8086 | 2FE5 | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Unicast Registers
8086 | 2FF8 | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Buffered Ring Agent
8086 | 2FF8 | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Buffered Ring Agent
8086 | 2FF9 | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Buffered Ring Agent
8086 | 2FF9 | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Buffered Ring Agent
8086 | 2FFC | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 System Address Decoder !LSPCI! Broadcast Registers
8086 | 2FFC | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 System Address Decoder !LSPCI! Broadcast Registers
8086 | 2FFD | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 System Address Decoder !LSPCI! Broadcast Registers
8086 | 2FFD | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 System Address Decoder !LSPCI! Broadcast Registers
8086 | 2FFE | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 System Address Decoder !LSPCI! Broadcast Registers
8086 | 2FFE | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 System Address Decoder !LSPCI! Broadcast Registers
8086 | 2F1D | 8086 | 2F1D | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 PCIe Ring Interface
8086 | 2F1D | 8086 | 2F1D | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 PCIe Ring Interface
8086 | 2F34 | 8086 | 2F34 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 PCIe Ring Interface
8086 | 2F34 | 8086 | 2F34 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 PCIe Ring Interface
8086 | 2F1E | 8086 | 2F1E | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Scratchpad !LSPCI! Semaphore Registers
8086 | 2F1E | 8086 | 2F1E | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Scratchpad !LSPCI! Semaphore Registers
8086 | 2F7D | 8086 | 2F7D | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Scratchpad !LSPCI! Semaphore Registers
8086 | 2F7D | 8086 | 2F7D | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Scratchpad !LSPCI! Semaphore Registers
8086 | 2F1F | 8086 | 2F1F | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Scratchpad !LSPCI! Semaphore Registers
8086 | 2F1F | 8086 | 2F1F | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Scratchpad !LSPCI! Semaphore Registers
8086 | 2FA0 | 8086 | 2FA0 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Home Agent 0
8086 | 2FA0 | 8086 | 2FA0 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Home Agent 0
8086 | 2F30 | 8086 | 2F30 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Home Agent 0
8086 | 2F30 | 8086 | 2F30 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Home Agent 0
8086 | 2FA8 | 8086 | 2FA8 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Target Address, Thermal !LSPCI! RAS Registers
8086 | 2FA8 | 8086 | 2FA8 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Target Address, Thermal !LSPCI! RAS Registers
8086 | 2F71 | 8086 | 2F71 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Target Address, Thermal !LSPCI! RAS Registers
8086 | 2F71 | 8086 | 2F71 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Target Address, Thermal !LSPCI! RAS Registers
8086 | 2FAA | 8086 | 2FAA | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Channel Target Address Decoder
8086 | 2FAA | 8086 | 2FAA | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Channel Target Address Decoder
8086 | 2FAB | 8086 | 2FAB | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Channel Target Address Decoder
8086 | 2FAB | 8086 | 2FAB | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Channel Target Address Decoder
8086 | 2FAC | 8086 | 2FAC | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Channel Target Address Decoder
8086 | 2FAC | 8086 | 2FAC | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Channel Target Address Decoder
8086 | 2FAD | 8086 | 2FAD | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Channel Target Address Decoder
8086 | 2FAD | 8086 | 2FAD | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Channel Target Address Decoder
8086 | 2FAE | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 DDRIO Channel 0/1 Broadcast
8086 | 2FAE | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 DDRIO Channel 0/1 Broadcast
8086 | 2FAF | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 DDRIO Global Broadcast
8086 | 2FAF | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 DDRIO Global Broadcast
8086 | 2FB0 | 8086 | 2FB0 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Channel 0 Thermal Control
8086 | 2FB0 | 8086 | 2FB0 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Channel 0 Thermal Control
8086 | 2FB1 | 8086 | 2FB1 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Channel 1 Thermal Control
8086 | 2FB1 | 8086 | 2FB1 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Channel 1 Thermal Control
8086 | 2FB2 | 8086 | 2FB2 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Channel 0 ERROR Registers
8086 | 2FB2 | 8086 | 2FB2 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Channel 0 ERROR Registers
8086 | 2FB3 | 8086 | 2FB3 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Channel 1 ERROR Registers
8086 | 2FB3 | 8086 | 2FB3 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Channel 1 ERROR Registers
8086 | 2FBC | 02 | 02 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 DDRIO (VMSE) 0 !LSPCI! 1
8086 | 2FBC | 02 | 02 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 DDRIO (VMSE) 0 !LSPCI! 1
8086 | 2FBD | 02 | 02 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 DDRIO (VMSE) 0 !LSPCI! 1
8086 | 2FBD | 02 | 02 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 DDRIO (VMSE) 0 !LSPCI! 1
8086 | 2FBE | 02 | 02 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 DDRIO (VMSE) 0 !LSPCI! 1
8086 | 2FBE | 02 | 02 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 DDRIO (VMSE) 0 !LSPCI! 1
8086 | 2FBF | 02 | 02 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 DDRIO (VMSE) 0 !LSPCI! 1
8086 | 2FBF | 02 | 02 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 DDRIO (VMSE) 0 !LSPCI! 1
8086 | 2FB4 | 8086 | 2FB4 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Channel 2 Thermal Control
8086 | 2FB4 | 8086 | 2FB4 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Channel 2 Thermal Control
8086 | 2FB5 | 8086 | 2FB5 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Channel 3 Thermal Control
8086 | 2FB5 | 8086 | 2FB5 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Channel 3 Thermal Control
8086 | 2FB6 | 8086 | 2FB6 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Channel 2 ERROR Registers
8086 | 2FB6 | 8086 | 2FB6 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Channel 2 ERROR Registers
8086 | 2FB7 | 8086 | 2FB7 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Channel 3 ERROR Registers
8086 | 2FB7 | 8086 | 2FB7 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 0 Channel 3 ERROR Registers
8086 | 2F68 | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 1 Target Address, Thermal !LSPCI! RAS Registers
8086 | 2F68 | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 1 Target Address, Thermal !LSPCI! RAS Registers
8086 | 2F6E | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 DDRIO Channel 2/3 Broadcast
8086 | 2F6E | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 DDRIO Channel 2/3 Broadcast
8086 | 2F6F | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 DDRIO Global Broadcast
8086 | 2F6F | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 DDRIO Global Broadcast
8086 | 2FD0 | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 1 Channel 0 Thermal Control
8086 | 2FD0 | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Integrated Memory Controller 1 Channel 0 Thermal Control
8086 | 2FB8 | 02 | 02 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 DDRIO (VMSE) 2 !LSPCI! 3
8086 | 2FB8 | 02 | 02 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 DDRIO (VMSE) 2 !LSPCI! 3
8086 | 2FB9 | 02 | 02 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 DDRIO (VMSE) 2 !LSPCI! 3
8086 | 2FB9 | 02 | 02 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 DDRIO (VMSE) 2 !LSPCI! 3
8086 | 2FBA | 02 | 02 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 DDRIO (VMSE) 2 !LSPCI! 3
8086 | 2FBA | 02 | 02 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 DDRIO (VMSE) 2 !LSPCI! 3
8086 | 2FBB | 02 | 02 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 DDRIO (VMSE) 2 !LSPCI! 3
8086 | 2FBB | 02 | 02 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 DDRIO (VMSE) 2 !LSPCI! 3
8086 | 2F98 | 8086 | 2F98 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Power Control Unit
8086 | 2F98 | 8086 | 2F98 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Power Control Unit
8086 | 2F99 | 8086 | 2F99 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Power Control Unit
8086 | 2F99 | 8086 | 2F99 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Power Control Unit
8086 | 2F9A | 8086 | 2F9A | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Power Control Unit
8086 | 2F9A | 8086 | 2F9A | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Power Control Unit
8086 | 2FC0 | 8086 | 2FC0 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Power Control Unit
8086 | 2FC0 | 8086 | 2FC0 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Power Control Unit
8086 | 2F9C | 8086 | 2F9C | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Power Control Unit
8086 | 2F9C | 8086 | 2F9C | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Power Control Unit
8086 | 2F88 | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 VCU
8086 | 2F88 | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 VCU
8086 | 2F8A | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 VCU
8086 | 2F8A | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 VCU
8086 | 2F00 | 1462 | 7885 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 DMI2
8086 | 2F02 | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 PCI Express Root Port 1
8086 | 2F03 | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 PCI Express Root Port 1
8086 | 2F04 | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 PCI Express Root Port 2
8086 | 2F08 | 0000 | 0000 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 PCI Express Root Port 3
8086 | 2F28 | 1462 | 7885 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Address Map, VTd_Misc, System Management
8086 | 2F29 | 1462 | 7885 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 Hot Plug
8086 | 2F2A | 1462 | 7885 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 RAS, Control Status and Global Errors
8086 | 2F2C | 1462 | 7885 | Intel Corporation Xeon E7 v3/Xeon E5 v3/Core i7 I/O APIC
8086 | 8D7C | 05 | 05 | Intel Corporation C610/X99 series chipset SPSR
8086 | 8D62 | 05 | 05 | Intel Corporation C610/X99 series chipset sSATA Controller (AHCI mode)
8086 | 8D31 | 1462 | 7885 | Intel Corporation C610/X99 series chipset USB xHCI Host Controller
8086 | 8D3A | 1462 | 7885 | Intel Corporation C610/X99 series chipset MEI Controller #1
8086 | 8D2D | 1462 | 7885 | Intel Corporation C610/X99 series chipset USB Enhanced Host Controller #2
8086 | 8D20 | 1462 | D885 | Intel Corporation C610/X99 series chipset HD Audio Controller
8086 | 8D10 | 0000 | 0000 | Intel Corporation C610/X99 series chipset PCI Express Root Port #1
8086 | 8D14 | 0000 | 0000 | Intel Corporation C610/X99 series chipset PCI Express Root Port #3
8086 | 8D16 | 0000 | 0000 | Intel Corporation C610/X99 series chipset PCI Express Root Port #4
8086 | 8D18 | 0000 | 0000 | Intel Corporation C610/X99 series chipset PCI Express Root Port #5
8086 | 8D26 | 1462 | 7885 | Intel Corporation C610/X99 series chipset USB Enhanced Host Controller #1
8086 | 8D47 | 1462 | 7885 | Intel Corporation C610/X99 series chipset LPC Controller
8086 | 8D02 | 05 | 05 | Intel Corporation C610/X99 series chipset 6-Port SATA Controller (AHCI mode)
8086 | 8D22 | 1462 | 7885 | Intel Corporation C610/X99 series chipset SMBus Controller
1002 | 67DF | 0000 | 0000 | Advanced Micro Devices, Inc. (AMD/ATI) Ellesmere (Radeon RX 470/480/570/570X/580/580X/590)
1002 | AAF0 | 0000 | 0000 | Advanced Micro Devices, Inc. (AMD/ATI) Ellesmere HDMI Audio (Radeon RX 470/480 / 570/580/590)
8086 | 1533 | 1462 | 7885 | Intel Corporation I210 Gigabit Network Connection
1106 | 3483 | 1462 | 7885 | VIA Technologies, Inc. VL805 USB 3.0 Host Controller
1B21 | 1242 | 0000 | 0000 | ASMedia Technology Inc. ASM1142 USB 3.1 Host Controller