[2020/01/27 09:30:35]
Ai Overclock Tuner (Ai-Übertaktungstuner) [XMP]
XMP [XMP DDR4-3597 18-19-19-39-1.35V]
BCLK Frequency (BCLK-Frequenz) [100.0000]
ASUS Multicore Enhancement (ASUS Multicore-Erweiterung) [Auto]
SVID Behavior [Auto]
AVX Instruction Core Ratio Negative Offset [Auto]
CPU Core Ratio [Per Core]
1-Core Ratio Limit [50]
2-Core Ratio Limit [50]
3-Core Ratio Limit [50]
4-Core Ratio Limit [50]
5-Core Ratio Limit [50]
6-Core Ratio Limit [50]
CPU-Bus-Geschwindigkeit: DRAM-Geschwindigkeits-Ratio-Modus [Auto]
DRAM Odd Ratio Mode (Modus eigentümliches DRAM-Verhältnis) [Enabled]
Speicherfrequenz [DDR4-3600MHz]
OC Tuner [Keep Current Settings]
Power-saving & Performance Mode [Auto]
CPU SVID Support (CPU-SVID-Unterstützung) [Auto]
CPU Core/Cache Current Limit Max. (CPU-Kern-/Cache-Stromgrenze max.) [Auto]
CPU Graphics Current Limit [Auto]
Ring Down Bin [Auto]
Min CPU Cache Ratio (Minimales CPU-Cache-Verhältnis) [Auto]
Max CPU Cache Ratio [Auto]
Maximale iGPU-Frequenz [Auto]
Extreme Überspannung [Disabled]
BCLK Aware Adaptive Voltage [Auto]
CPU Core/Cache Voltage [Manual Mode]
- CPU-Kernspannungsübergehung [1.385]
DRAM-Spannung [1.3530]
CPU VCCIO Voltage [Auto]
CPU System Agent Voltage [Auto]
CPU Graphics Voltage Mode [Auto]
PCH-Kernspannung [Auto]
CPU Standby Voltage [Auto]
DRAM CTRL REF Voltage [Auto]
DRAM DATA REF Voltage on CHB [Auto]
DRAM DATA REF Voltage on CHA DIMM0 Rank0 BL0 [Auto]
DRAM DATA REF Voltage on CHA DIMM0 Rank0 BL1 [Auto]
DRAM DATA REF Voltage on CHA DIMM0 Rank0 BL2 [Auto]
DRAM DATA REF Voltage on CHA DIMM0 Rank0 BL3 [Auto]
DRAM DATA REF Voltage on CHA DIMM0 Rank0 BL4 [Auto]
DRAM DATA REF Voltage on CHA DIMM0 Rank0 BL5 [Auto]
DRAM DATA REF Voltage on CHA DIMM0 Rank0 BL6 [Auto]
DRAM DATA REF Voltage on CHA DIMM0 Rank0 BL7 [Auto]
DRAM DATA REF Voltage on CHA DIMM0 Rank1 BL0 [Auto]
DRAM DATA REF Voltage on CHA DIMM0 Rank1 BL1 [Auto]
DRAM DATA REF Voltage on CHA DIMM0 Rank1 BL2 [Auto]
DRAM DATA REF Voltage on CHA DIMM0 Rank1 BL3 [Auto]
DRAM DATA REF Voltage on CHA DIMM0 Rank1 BL4 [Auto]
DRAM DATA REF Voltage on CHA DIMM0 Rank1 BL5 [Auto]
DRAM DATA REF Voltage on CHA DIMM0 Rank1 BL6 [Auto]
DRAM DATA REF Voltage on CHA DIMM0 Rank1 BL7 [Auto]
DRAM DATA REF Voltage on CHA DIMM1 Rank0 BL0 [Auto]
DRAM DATA REF Voltage on CHA DIMM1 Rank0 BL1 [Auto]
DRAM DATA REF Voltage on CHA DIMM1 Rank0 BL2 [Auto]
DRAM DATA REF Voltage on CHA DIMM1 Rank0 BL3 [Auto]
DRAM DATA REF Voltage on CHA DIMM1 Rank0 BL4 [Auto]
DRAM DATA REF Voltage on CHA DIMM1 Rank0 BL5 [Auto]
DRAM DATA REF Voltage on CHA DIMM1 Rank0 BL6 [Auto]
DRAM DATA REF Voltage on CHA DIMM1 Rank0 BL7 [Auto]
DRAM DATA REF Voltage on CHA DIMM1 Rank1 BL0 [Auto]
DRAM DATA REF Voltage on CHA DIMM1 Rank1 BL1 [Auto]
DRAM DATA REF Voltage on CHA DIMM1 Rank1 BL2 [Auto]
DRAM DATA REF Voltage on CHA DIMM1 Rank1 BL3 [Auto]
DRAM DATA REF Voltage on CHA DIMM1 Rank1 BL4 [Auto]
DRAM DATA REF Voltage on CHA DIMM1 Rank1 BL5 [Auto]
DRAM DATA REF Voltage on CHA DIMM1 Rank1 BL6 [Auto]
DRAM DATA REF Voltage on CHA DIMM1 Rank1 BL7 [Auto]
DRAM DATA REF Voltage on CHB DIMM0 Rank0 BL0 [Auto]
DRAM DATA REF Voltage on CHB DIMM0 Rank0 BL1 [Auto]
DRAM DATA REF Voltage on CHB DIMM0 Rank0 BL2 [Auto]
DRAM DATA REF Voltage on CHB DIMM0 Rank0 BL3 [Auto]
DRAM DATA REF Voltage on CHB DIMM0 Rank0 BL4 [Auto]
DRAM DATA REF Voltage on CHB DIMM0 Rank0 BL5 [Auto]
DRAM DATA REF Voltage on CHB DIMM0 Rank0 BL6 [Auto]
DRAM DATA REF Voltage on CHB DIMM0 Rank0 BL7 [Auto]
DRAM DATA REF Voltage on CHB DIMM0 Rank1 BL0 [Auto]
DRAM DATA REF Voltage on CHB DIMM0 Rank1 BL1 [Auto]
DRAM DATA REF Voltage on CHB DIMM0 Rank1 BL2 [Auto]
DRAM DATA REF Voltage on CHB DIMM0 Rank1 BL3 [Auto]
DRAM DATA REF Voltage on CHB DIMM0 Rank1 BL4 [Auto]
DRAM DATA REF Voltage on CHB DIMM0 Rank1 BL5 [Auto]
DRAM DATA REF Voltage on CHB DIMM0 Rank1 BL6 [Auto]
DRAM DATA REF Voltage on CHB DIMM0 Rank1 BL7 [Auto]
DRAM DATA REF Voltage on CHB DIMM1 Rank0 BL0 [Auto]
DRAM DATA REF Voltage on CHB DIMM1 Rank0 BL1 [Auto]
DRAM DATA REF Voltage on CHB DIMM1 Rank0 BL2 [Auto]
DRAM DATA REF Voltage on CHB DIMM1 Rank0 BL3 [Auto]
DRAM DATA REF Voltage on CHB DIMM1 Rank0 BL4 [Auto]
DRAM DATA REF Voltage on CHB DIMM1 Rank0 BL5 [Auto]
DRAM DATA REF Voltage on CHB DIMM1 Rank0 BL6 [Auto]
DRAM DATA REF Voltage on CHB DIMM1 Rank0 BL7 [Auto]
DRAM DATA REF Voltage on CHB DIMM1 Rank1 BL0 [Auto]
DRAM DATA REF Voltage on CHB DIMM1 Rank1 BL1 [Auto]
DRAM DATA REF Voltage on CHB DIMM1 Rank1 BL2 [Auto]
DRAM DATA REF Voltage on CHB DIMM1 Rank1 BL3 [Auto]
DRAM DATA REF Voltage on CHB DIMM1 Rank1 BL4 [Auto]
DRAM DATA REF Voltage on CHB DIMM1 Rank1 BL5 [Auto]
DRAM DATA REF Voltage on CHB DIMM1 Rank1 BL6 [Auto]
DRAM DATA REF Voltage on CHB DIMM1 Rank1 BL7 [Auto]
DRAM CAS# Latency [18]
DRAM RAS# to CAS# Delay [19]
DRAM RAS# ACT Time [39]
DRAM Command Rate [Auto]
DRAM RAS# to RAS# Delay L [Auto]
DRAM RAS# to RAS# Delay S [Auto]
DRAM REF Cycle Time [Auto]
DRAM Refresh Interval [Auto]
DRAM WRITE Recovery Time [Auto]
DRAM READ to PRE Time [Auto]
DRAM FOUR ACT WIN Time [Auto]
DRAM WRITE to READ Delay [Auto]
DRAM WRITE to READ Delay L [Auto]
DRAM WRITE to READ Delay S [Auto]
DRAM CKE Minimum Pulse Width [Auto]
DRAM Write Latency [Auto]
tRDRD_sg [Auto]
tRDRD_dg [Auto]
tRDWR_sg [Auto]
tRDWR_dg [Auto]
tWRWR_sg [Auto]
tWRWR_dg [Auto]
tWRRD_sg [Auto]
tWRRD_dg [Auto]
tRDRD_dr [Auto]
tRDRD_dd [Auto]
tRDWR_dr [Auto]
tRDWR_dd [Auto]
tWRWR_dr [Auto]
tWRWR_dd [Auto]
tWRRD_dr [Auto]
tWRRD_dd [Auto]
TWRPRE [Auto]
TRDPRE [Auto]
tREFIX9 [Auto]
OREF_RI [Auto]
MRC-Systemschnellstart [Auto]
DRAM CLK Period [Auto]
Speicher-Scrambler [Aktiviert]
Kanal A DIMM-Steuerung [Enable both DIMMs]
Kanal B DIMM-Steuerung [Enable both DIMMs]
MCH Full Check [Auto]
Training Profile [Auto]
DLLBwEn [Auto]
DRAM SPD Write [Disabled]
DRAM RTL INIT value [Auto]
DRAM RTL (CHA DIMM0 Rank0) [Auto]
DRAM RTL (CHA DIMM0 Rank1) [Auto]
DRAM RTL (CHA DIMM1 Rank0) [Auto]
DRAM RTL (CHA DIMM1 Rank1) [Auto]
DRAM RTL (CHB DIMM0 Rank0) [Auto]
DRAM RTL (CHB DIMM0 Rank1) [Auto]
DRAM RTL (CHB DIMM1 Rank0) [Auto]
DRAM RTL (CHB DIMM1 Rank1) [Auto]
DRAM IOL (CHA DIMM0 Rank0) [Auto]
DRAM IOL (CHA DIMM0 Rank1) [Auto]
DRAM IOL (CHA DIMM1 Rank0) [Auto]
DRAM IOL (CHA DIMM1 Rank1) [Auto]
DRAM IOL (CHB DIMM0 Rank0) [Auto]
DRAM IOL (CHB DIMM0 Rank1) [Auto]
DRAM IOL (CHB DIMM1 Rank0) [Auto]
DRAM IOL (CHB DIMM1 Rank1) [Auto]
CHA IO_Latency_offset [Auto]
CHB IO_Latency_offset [Auto]
CHA RFR delay [Auto]
CHB RFR delay [Auto]
ODT RTT WR (CHA) [Auto]
ODT RTT PARK (CHA) [Auto]
ODT RTT NOM (CHA) [Auto]
ODT RTT WR (CHB) [Auto]
ODT RTT PARK (CHB) [Auto]
ODT RTT NOM (CHB) [Auto]
ODT_READ_DURATION [Auto]
ODT_READ_DELAY [Auto]
ODT_WRITE_DURATION [Auto]
ODT_WRITE_DELAY [Auto]
Data Rising Slope [Auto]
Data Rising Slope Offset [Auto]
Cmd Rising Slope [Auto]
Cmd Rising Slope Offset [Auto]
Ctl Rising Slope [Auto]
Ctl Rising Slope Offset [Auto]
Clk Rising Slope [Auto]
Clk Rising Slope Offset [Auto]
Data Falling Slope [Auto]
Data Falling Slope Offset [Auto]
Cmd Falling Slope [Auto]
Cmd Falling Slope Offset [Auto]
Ctl Falling Slope [Auto]
Ctl Falling Slope Offset [Auto]
Clk Falling Slope [Auto]
Clk Falling Slope Offset [Auto]
CPU Load-Line Calibration (CPU-Belastungslinie-Kalibrierung) [Level 6]
CPU Current Capability (CPU-Stromfähigkeit) [140%]
CPU VRM Switching Frequency (CPU-VRM-Schaltfrequenz) [Auto]
VRM Spread Spectrum (VRM-Streuspektrum) [Auto]
CPU Power Duty Control (CPU-Leistungszyklusregelung) [T.Probe]
CPU Power Phase Control (CPU-Leistungsphasensteuerung) [Auto]
CPU VRM Thermal Control [Auto]
CPU Graphics Load-line Calibration [Auto]
CPU Graphics Current Capability [Auto]
CPU Graphics VRM Switching Frequency [Auto]
CPU Graphics Power Phase Control [Auto]
Intel(R) SpeedStep(tm) [Auto]
Turbo-Modus [Aktiviert]
Long Duration Package Power Limit (Langzeit-Paket-Leistungslimit) [4095]
Package Power Time Window (Paket-Leistungszeitfenster) [Auto]
Short Duration Package Power Limit (Kurzzeit-Paket-Leistungslimit) [4095]
IA AC Load Line [Auto]
IA DC Load Line [Auto]
TVB Voltage Optimizations [Auto]
PCI Express Native Power Management [Disabled]
DMI-Link-ASPM-Steuerung [Deaktiviert]
ASPM [Deaktiviert]
L1 Substates [Deaktiviert]
PCI Express Clock Gating [Aktiviert]
DMI Link ASPM Control [Deaktiviert]
PEG - ASPM [Deaktiviert]
Hyper-Threading [Aktiviert]
Aktive Prozessorkerne [Alle]
Intel Virtualization Technology [Deaktiviert]
Hardware Prefetcher [Aktiviert]
Adjacent Cache Line Prefetch [Aktiviert]
SW Guard Extensions (SGX) [Software Controlled]
Tcc Offset Time Window [Auto]
Intel(R) SpeedStep(tm) [Auto]
Turbo-Modus [Aktiviert]
CPU C-states [Auto]
CFG Lock [Deaktiviert]
Intel(R) Speed Shift Technology [Aktiviert]
VT-d [Deaktiviert]
Above 4G Decoding [Deaktiviert]
Primäre Anzeige [PCIE]
iGPU-Initialisierung [Aktiviert]
RC6(Render Standby) [Auto]
DVMT Pre-Allocated [64M]
DMI Max Link Speed [Auto]
PCIEX16/X8_1-Verbindungsgeschwindigkeit [Auto]
PCIEX8_2-Verbindungsgeschwindigkeit [Auto]
IOAPIC 24-119 Entries [Aktiviert]
PCIe Speed [Auto]
SATA Controller [Aktiviert]
SATA-Modusauswahl [AHCI]
Aggressive-LPM-Unterstützung [Deaktiviert]
S.M.A.R.T.-Statusprüfung [Enabled]
SATA6G_1(Charcoal Black) [Aktiviert]
Hot Plug [Deaktiviert]
SATA6G_2(Charcoal Black) [Aktiviert]
Hot Plug [Deaktiviert]
SATA6G_3(Charcoal Black) [Aktiviert]
Hot Plug [Deaktiviert]
SATA6G_4(Charcoal Black) [Aktiviert]
Hot Plug [Deaktiviert]
SATA6G_5(Charcoal Black) [Aktiviert]
Hot Plug [Deaktiviert]
SATA6G_6(Charcoal Black) [Aktiviert]
Hot Plug [Deaktiviert]
Intel Platform Trust Technology [Disabled ]
VccCore Override Enable [Deaktiviert]
VccST Override Enable [Deaktiviert]
VccSA Override Enable [Deaktiviert]
VccSFR_OC Override Enable [Deaktiviert]
VccSFR Override Enable [Deaktiviert]
VccIO Override Enable [Deaktiviert]
Core PLL Voltage Offset [0]
GT PLL Voltage Offset [0]
Ring PLL Voltage Offset [0]
System Agent PLL Voltage Offset [0]
Memory Controller PLL Voltage Offset [0]
Security Device Support [Enable]
Pending operation [None]
Platform Hierarchy [Enabled]
Storage Hierarchy [Enabled]
Endorsement Hierarchy [Enabled]
TPM2.0 UEFI Spec Version [TCG_2]
Physical Presence Spec Version [1.3]
ErP-Bereit [Deaktiviert]
Nach Stromausfall wiederherstellen [Ausgeschaltet]
Einschalten durch PCI-E [Deaktiviert]
Einschalten durch RTC [Deaktiviert]
Hyper M.2X16 [Disabled]
Azalia HD Audio-Controller [Aktiviert]
Depop [Aktiviert]
M.2_1 Configuration [Auto]
Asmedia USB 3.1-Controller [Aktiviert]
When system is in working state [Ein]
When system is in sleep, hibernate or soft off states [Ein]
Wi-Fi Controller [Aktiviert]
Bluetooth Controller [Aktiviert]
Intel-LAN-Controller [Aktivieren]
Intel PXE Option ROM [Disabled]
Netzwerk-Stack [Deaktiviert]
Antiquierte USB-Unterstützung [Enabled]
USB Keyboard and Mouse Simulator [Disabled]
Intenso Ultra Line 1.00 [Auto]
U31G1_1 [Aktiviert]
U31G1_2 [Aktiviert]
U31G1_3 [Aktiviert]
U31G1_4 [Aktiviert]
U31G1_5 [Aktiviert]
U31G1_6 [Aktiviert]
USB9 [Aktiviert]
USB10 [Aktiviert]
USB11 [Aktiviert]
USB12 [Aktiviert]
USB13 [Aktiviert]
USB14 [Aktiviert]
CPU-Temperatur(PECI) [Verwaltung]
MB-Temperatur [Verwaltung]
PCH Temperature [Verwaltung]
T_Sensor Temperature [Verwaltung]
CPU-Lüftergeschwindigkeit [Verwaltung]
CPU Optionale Lüftergeschwindigkeit [Verwaltung]
Gehäuselüfter-1-Drehzahl [Verwaltung]
Gehäuselüfter-2-Drehzahl [Verwaltung]
W_PUMP+ Geschwindigkeit [Verwaltung]
CPU-Kern-Spannung [Verwaltung]
CPU Graphics Voltage [Verwaltung]
3.3V-Spannung [Verwaltung]
5V-Spannung [Verwaltung]
12V-Spannung [Verwaltung]
PCH Core Voltage [Verwaltung]
CPU System Agent Voltage [Verwaltung]
CPU VCCIO Voltage [Verwaltung]
DRAM Voltage [Verwaltung]
CPU Standby Voltage [Verwaltung]
DMI Voltage [Verwaltung]
CPU Q-Fan-Kontrolle [Auto]
CPU Fan Speed Lower Limit [200 RPM]
CPU-Lüfterprofil [Standard]
Wasserpumpensteuerung [Deaktiviert]
Gehäuselüfter 1 Q-Fan-Steuerung [Auto]
Chassis Fan 1 Q-Fan Source [CPU]
Unterer Grenzwert der Gehäuselüftergeschwindigkeit [200 RPM]
Gehäuselüfter-1-Profil [Standard]
Gehäuselüfter 2 Q-Fan-Steuerung [Auto]
Chassis Fan 2 Q-Fan Source [CPU]
Unterer Grenzwert der Gehäuselüftergeschwindigkeit [200 RPM]
Gehäuselüfter-2-Profil [Standard]
Schnelles Boot [Enabled]
Nächster Systemstart nach Ausfall der Stromversorgung [Normal-Boot]
Boot-Logo-Anzeige [Auto]
POST-Verzögerungszeit [2 Sek]
NUM-Zustand beim Bootup [An]
Bei Fehler auf 'F1' warten [Aktiviert]
Option-ROM-Meldungen [Force BIOS]
Interrupt 19 abfangen [Deaktiviert]
Einrichtungsmodus [EZ-Modus]
CSM starten [Aktiviert]
Bootgerätekontrolle [UEFI und Legacy OPROM]
Von Netzwerkgeräten booten [Legacy only]
Von externen Datenträger booten [UEFI-Treiber zuerst]
PCI-E Erweiterungskarten booten [Legacy only]
Art des Betriebssystems [Anderes Betriebssystem]
Setup Animator [Deaktiviert]
Vom Profil laden [1]
Profilname [OC 5Ghz SAVE]
Im Profil speichern [1]
Bus Interface (Busschnittstelle) [PCIe_x16_1/PCIex8_1]
