#Maintained by: RehabMan for: Laptop Patches
#misc_Skylake-LPC.txt

# inject "compatible" with recognized series-100 LPC device-id
into method label _DSM parent_adr 0x001F0000 remove_entry;
into device name_adr 0x001F0000 insert
begin
Method (_DSM, 4, NotSerialized)\n
{\n
    If (LEqual (Arg2, Zero)) { Return (Buffer() { 0x03 } ) }\n
    Return (Package()\n
    {\n
        "compatible", "pci8086,9cc1",\n
    })\n
}\n
end;
