Extracted contents:
header:          00 ff ff ff ff ff ff 00
serial number:   06 10 f2 9c 00 00 00 00 1a 15
version:         01 04
basic params:    95 1a 0e 78 02
chroma info:     ef 05 97 57 54 92 27 22 50 54
established:     00 00 00
standard:        01 01 01 01 01 01 01 01 01 01 01 01 01 01 01 01
descriptor 1:    1a 36 80 a0 70 38 1f 40 30 20 35 00 db 0b 11 00 00 1a
descriptor 2:    8d 0e c0 a0 30 1c 10 20 30 20 35 00 db 0b 11 00 00 1a
descriptor 3:    00 00 00 fc 00 43 6f 6c 6f 72 20 4c 43 44 0a 20 20 20
descriptor 4:    00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
extensions:      01
checksum:        bf

Manufacturer: APP Model 9cf2 Serial Number 0
Made week 26 of 2011
EDID version: 1.4
Digital display
6 bits per primary color channel
DisplayPort interface
Maximum image size: 26 cm x 14 cm
Gamma: 2.20
Supported color formats: RGB 4:4:4
First detailed timing is preferred timing
Chroma Info:
Red X: 0.592773 Y: 0.341797
Green X: 0.331055 Y: 0.573242
Blue X: 0.152344 Y: 0.132812
White X: 0.313477 Y: 0.329102
Established timings supported:
Standard timings supported:
Detailed mode: Clock 138.500 MHz, 475 mm x 267 mm
               1920 1968 2000 2080 hborder 0
               1080 1083 1088 1111 vborder 0
               +hsync -vsync 
Detailed mode: Clock 37.250 MHz, 475 mm x 267 mm
                960 1008 1040 1120 hborder 0
                540  543  548  556 vborder 0
               +hsync -vsync 
Monitor name: Color
Manufacturer-specified data, tag 0
Has 1 extension blocks
Checksum: 0xbf (valid)

Manufacturer-specific extension block
Unknown extension block

EDID block does NOT conform to EDID 1.3!
	Missing monitor ranges
	Detailed block string not properly terminated
EDID block does not conform at all!
	Has 3495383 nonconformant extension block(s)
