Device path: PciRoot(0x0)/Pci(0x1F,0x3)/VenMsg(A9003FEB-D806-41DB-A491-5405FEEF46C3,00000000)
Address: 0x0

Codec: Realtek ALC257
AFG Function Id: 0x1 (unsol 1)
Vendor Id: 0x10EC0257
Revision Id: 0x100001
Default PCM:
    rates [0x560]: 44100 48000 96000 192000
    bits [0xE]: 16 20 24
    formats [0x1]: PCM
Default Amp-In caps: N/A
Default Amp-Out caps: N/A
Node 0x02 (2) [Audio Output] wcaps 0x41D: Stereo Amp-Out
  Amp-Out caps: ofs=0x57, nsteps=0x57, stepsize=0x02, mute=0
  Amp-Out vals: [0x57 0x57]
  Converter: stream=0, channel=0
  PCM:
    rates [0x60]: 44100 48000
    bits [0xE]: 16 20 24
    formats [0x1]: PCM
Node 0x03 (3) [Audio Output] wcaps 0x41D: Stereo Amp-Out
  Amp-Out caps: ofs=0x57, nsteps=0x57, stepsize=0x02, mute=0
  Amp-Out vals: [0x57 0x57]
  Converter: stream=0, channel=0
  PCM:
    rates [0x60]: 44100 48000
    bits [0xE]: 16 20 24
    formats [0x1]: PCM
Node 0x04 (4) [Vendor Defined Widget] wcaps 0xF00000: Mono
Node 0x05 (5) [Vendor Defined Widget] wcaps 0xF00000: Mono
Node 0x06 (6) [Audio Output] wcaps 0x611: Stereo Digital
  Converter: stream=0, channel=0
  PCM:
    rates [0x5E0]: 44100 48000 88200 96000 192000
    bits [0xE]: 16 20 24
    formats [0x1]: PCM
Node 0x07 (7) [Audio Input] wcaps 0x10051B: Stereo Amp-In
  Amp-In caps: ofs=0x17, nsteps=0x3F, stepsize=0x02, mute=1
  Amp-In vals: [0x97 0x97]
  Converter: stream=0, channel=0
  PCM:
    rates [0x560]: 44100 48000 96000 192000
    bits [0xE]: 16 20 24
    formats [0x1]: PCM
  Connection: 1
     0x24
Node 0x08 (8) [Audio Input] wcaps 0x10051B: Stereo Amp-In
  Amp-In caps: ofs=0x17, nsteps=0x3F, stepsize=0x02, mute=1
  Amp-In vals: [0x97 0x97]
  Converter: stream=0, channel=0
  PCM:
    rates [0x560]: 44100 48000 96000 192000
    bits [0xE]: 16 20 24
    formats [0x1]: PCM
  Connection: 1
     0x23
Node 0x09 (9) [Audio Input] wcaps 0x10051B: Stereo Amp-In
  Amp-In caps: ofs=0x17, nsteps=0x3F, stepsize=0x02, mute=1
  Amp-In vals: [0x97 0x97]
  Converter: stream=0, channel=0
  PCM:
    rates [0x560]: 44100 48000 96000 192000
    bits [0xE]: 16 20 24
    formats [0x1]: PCM
  Connection: 1
     0x22
Node 0x0A (10) [Vendor Defined Widget] wcaps 0xF00000: Mono
Node 0x0B (11) [Vendor Defined Widget] wcaps 0xF00000: Mono
Node 0x0C (12) [Vendor Defined Widget] wcaps 0xF00000: Mono
Node 0x0D (13) [Vendor Defined Widget] wcaps 0xF00000: Mono
Node 0x0E (14) [Vendor Defined Widget] wcaps 0xF00000: Mono
Node 0x0F (15) [Vendor Defined Widget] wcaps 0xF00000: Mono
Node 0x10 (16) [Vendor Defined Widget] wcaps 0xF00000: Mono
Node 0x11 (17) [Vendor Defined Widget] wcaps 0xF00000: Mono
Node 0x12 (18) [Pin Complex] wcaps 0x40040B: Stereo Amp-In
  Amp-In caps: ofs=0x00, nsteps=0x03, stepsize=0x27, mute=0
  Amp-In vals:
  Pincap 0x00000020: IN
  Pin Default 0x411111F0: [None] Speaker at Ext Rear
    Conn = 1/8, Color = Black
    DefAssociation = 0xF, Sequence = 0x0
Pin-ctls: 0x00: VREF_HIZ
Node 0x13 (19) [Pin Complex] wcaps 0x40040B: Stereo Amp-In
  Amp-In caps: ofs=0x00, nsteps=0x03, stepsize=0x27, mute=0
  Amp-In vals:
  Pincap 0x00000020: IN
  Pin Default 0x411111F0: [None] Speaker at Ext Rear
    Conn = 1/8, Color = Black
    DefAssociation = 0xF, Sequence = 0x0
Pin-ctls: 0x00: VREF_HIZ
Node 0x14 (20) [Pin Complex] wcaps 0x40058D: Stereo Amp-Out
  Amp-Out caps: ofs=0x00, nsteps=0x00, stepsize=0x00, mute=1
  Amp-Out vals: [0x80 0x80]
  Pincap 0x00010014: OUT EAPD Detect
  EAPD 0x2: EAPD
  Pin Default 0x90170110: [Fixed] Speaker at Int N/A
    Conn = Analog, Color = Unknown
    DefAssociation = 0x1, Sequence = 0x0
Pin-ctls: 0x00: VREF_HIZ
  Connection: 1
     0x02
Node 0x15 (21) [Vendor Defined Widget] wcaps 0xF00000: Mono
Node 0x16 (22) [Vendor Defined Widget] wcaps 0xF00000: Mono
Node 0x17 (23) [Vendor Defined Widget] wcaps 0xF00000: Mono
Node 0x18 (24) [Pin Complex] wcaps 0x40048B: Stereo Amp-In
  Amp-In caps: ofs=0x00, nsteps=0x03, stepsize=0x27, mute=0
  Amp-In vals:
  Pincap 0x00003724: IN Detect VREF_HIZ VREF_GRD VREF_50 VREF_80 VREF_100
  Pin Default 0x411111F0: [None] Speaker at Ext Rear
    Conn = 1/8, Color = Black
    DefAssociation = 0xF, Sequence = 0x0
Pin-ctls: 0x20: IN VREF_HIZ
Node 0x19 (25) [Pin Complex] wcaps 0x40048B: Stereo Amp-In
  Amp-In caps: ofs=0x00, nsteps=0x03, stepsize=0x27, mute=0
  Amp-In vals:
  Pincap 0x00003724: IN Detect VREF_HIZ VREF_GRD VREF_50 VREF_80 VREF_100
  Pin Default 0x04A11030: [Jack] Mic at Ext Right
    Conn = 1/8, Color = Black
    DefAssociation = 0x3, Sequence = 0x0
Pin-ctls: 0x20: IN VREF_HIZ
Node 0x1A (26) [Pin Complex] wcaps 0x40048B: Stereo Amp-In
  Amp-In caps: ofs=0x00, nsteps=0x03, stepsize=0x27, mute=0
  Amp-In vals:
  Pincap 0x00003724: IN Detect VREF_HIZ VREF_GRD VREF_50 VREF_80 VREF_100
  Pin Default 0x411111F0: [None] Speaker at Ext Rear
    Conn = 1/8, Color = Black
    DefAssociation = 0xF, Sequence = 0x0
Pin-ctls: 0x00: VREF_HIZ
Node 0x1B (27) [Pin Complex] wcaps 0x40058F: Stereo Amp-In Amp-Out
  Amp-In caps: ofs=0x00, nsteps=0x03, stepsize=0x27, mute=0
  Amp-In vals: [0x00 0x00] [0x00 0x00]
  Amp-Out caps: ofs=0x00, nsteps=0x00, stepsize=0x00, mute=1
  Amp-Out vals: [0x80 0x80]
  Pincap 0x00013734: IN OUT EAPD Detect VREF_HIZ VREF_GRD VREF_50 VREF_80 VREF_100
  EAPD 0x2: EAPD
  Pin Default 0x411111F0: [None] Speaker at Ext Rear
    Conn = 1/8, Color = Black
    DefAssociation = 0xF, Sequence = 0x0
Pin-ctls: 0x20: IN VREF_HIZ
  Connection: 2
     0x02 0x03
Node 0x1C (28) [Vendor Defined Widget] wcaps 0xF00000: Mono
Node 0x1D (29) [Pin Complex] wcaps 0x400400: Mono
  Pincap 0x00000020: IN
  Pin Default 0x411111F0: [None] Speaker at Ext Rear
    Conn = 1/8, Color = Black
    DefAssociation = 0xF, Sequence = 0x0
Pin-ctls: 0x20: IN VREF_HIZ
Node 0x1E (30) [Pin Complex] wcaps 0x400781: Stereo Digital
  Pincap 0x00000014: OUT Detect
  Pin Default 0x411111F0: [None] Speaker at Ext Rear
    Conn = 1/8, Color = Black
    DefAssociation = 0xF, Sequence = 0x0
Pin-ctls: 0x40: OUT VREF_HIZ
  Connection: 1
     0x06
Node 0x1F (31) [Vendor Defined Widget] wcaps 0xF00000: Mono
Node 0x20 (32) [Vendor Defined Widget] wcaps 0xF00040: Mono
Node 0x21 (33) [Pin Complex] wcaps 0x40058D: Stereo Amp-Out
  Amp-Out caps: ofs=0x00, nsteps=0x00, stepsize=0x00, mute=1
  Amp-Out vals: [0x80 0x80]
  Pincap 0x0001001C: OUT HP EAPD Detect
  EAPD 0x2: EAPD
  Pin Default 0x04211020: [Jack] HP Out at Ext Right
    Conn = 1/8, Color = Black
    DefAssociation = 0x2, Sequence = 0x0
Pin-ctls: 0x00: VREF_HIZ
  Connection: 2
     0x02 0x03
Node 0x22 (34) [Audio Mixer] wcaps 0x20010B: Stereo Amp-In
  Amp-In caps: ofs=0x00, nsteps=0x00, stepsize=0x00, mute=1
  Amp-In vals: [0x80 0x80] [0x80 0x80] [0x80 0x80] [0x80 0x80] [0x80 0x80] [0x80 0x80]
  Connection: 6
     0x18 0x19 0x1A 0x1B 0x1D 0x13
Node 0x23 (35) [Audio Mixer] wcaps 0x20010B: Stereo Amp-In
  Amp-In caps: ofs=0x00, nsteps=0x00, stepsize=0x00, mute=1
  Amp-In vals: [0x80 0x80] [0x80 0x80] [0x80 0x80] [0x80 0x80] [0x80 0x80] [0x80 0x80]
  Connection: 6
     0x18 0x19 0x1A 0x1B 0x1D 0x12
Node 0x24 (36) [Audio Selector] wcaps 0x300101: Stereo
  Connection: 2
     0x12 0x13
