[
{"data":{"title":"IOPowerManagement"},"attr":{"id":"9128","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"CurrentPowerState"},"attr":{"id":"9130","ColType":"Number","ColValue":"2"}},{"data":{"title":"DevicePowerState"},"attr":{"id":"9132","ColType":"Number","ColValue":"2"}},{"data":{"title":"MaxPowerState"},"attr":{"id":"9134","ColType":"Number","ColValue":"3"}},{"data":{"title":"DriverPowerState"},"attr":{"id":"9136","ColType":"Number","ColValue":"0"}},{"data":{"title":"CapabilityFlags"},"attr":{"id":"9138","ColType":"Number","ColValue":"65536"}}]},
{"data":{"title":"locationID"},"attr":{"id":"9140","ColType":"Number","ColValue":"1510998016"}},
{"data":{"title":"kUSBBusCurrentAllocation"},"attr":{"id":"9142","ColType":"Number","ColValue":"0"}},
{"data":{"title":"kUSBSleepPortCurrentLimit"},"attr":{"id":"9144","ColType":"Number","ColValue":"1000"}},
{"data":{"title":"port"},"attr":{"id":"9146","ColType":"Data","ColValue":"&lt;01000000&gt;"}},
{"data":{"title":"port-statistics"},"attr":{"id":"9148","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"kPortStatRemoteWakeCount"},"attr":{"id":"9150","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatEOF2ViolationCount"},"attr":{"id":"9152","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatEOF2ViolationDuringResetCount"},"attr":{"id":"9154","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatAddressFailureCount"},"attr":{"id":"9156","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatEOF2ViolationDuringResumeCount"},"attr":{"id":"9158","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatEOF2ViolationRecoveryDuringResetCount"},"attr":{"id":"9160","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatOverCurrentCount"},"attr":{"id":"9162","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatEnumerationFailureCount"},"attr":{"id":"9164","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatEOF2ViolationCurrentConnectCount"},"attr":{"id":"9166","ColType":"Number","ColValue":"0"}},{"data":{"title":"kPortStatPowerStateTime"},"attr":{"id":"9168","ColType":"Dictionary","ColValue":"0_values"},"children":[{"data":{"title":"kPowerStateSleep"},"attr":{"id":"9170","ColType":"String","ColValue":"0ms (0%)"}},{"data":{"title":"kPowerStateOn"},"attr":{"id":"9172","ColType":"String","ColValue":"0ms (0%)"}},{"data":{"title":"kPowerStateOff"},"attr":{"id":"9174","ColType":"String","ColValue":"0ms (0%)"}},{"data":{"title":"kPowerStateSuspended"},"attr":{"id":"9176","ColType":"String","ColValue":"1808169ms (100%)"}}]},{"data":{"title":"kPortStatConnectCount"},"attr":{"id":"9178","ColType":"Number","ColValue":"0"}}]},
{"data":{"title":"kUSBWakePortCurrentLimit"},"attr":{"id":"9180","ColType":"Number","ColValue":"1500"}},
{"data":{"title":"IOGeneralInterest"},"attr":{"id":"9182","ColType":"String","ColValue":"IOCommand is not serializable"}},
{"data":{"title":"port-status"},"attr":{"id":"9184","ColType":"Number","ColValue":"1"}},
{"data":{"title":"kUSBBusCurrentSleepAllocation"},"attr":{"id":"9186","ColType":"Number","ColValue":"0"}}
]
