00:00.0 Host bridge: Intel Corporation 4 Series Chipset DRAM Controller (rev 02)
00:06.0 PCI bridge: Intel Corporation 4 Series Chipset PCI Express Root Port (rev 02)
## 00.06:0 is a bridge from 00 to 01-01
00:1a.0 USB controller: Intel Corporation 82801JI (ICH10 Family) USB UHCI Controller #4
00:1a.1 USB controller: Intel Corporation 82801JI (ICH10 Family) USB UHCI Controller #5
00:1a.2 USB controller: Intel Corporation 82801JI (ICH10 Family) USB UHCI Controller #6
00:1a.7 USB controller: Intel Corporation 82801JI (ICH10 Family) USB2 EHCI Controller #2
00:1c.0 PCI bridge: Intel Corporation 82801JI (ICH10 Family) PCI Express Root Port 1
## 00.1c:0 is a bridge from 00 to 06-06
00:1c.1 PCI bridge: Intel Corporation 82801JI (ICH10 Family) PCI Express Port 2
## 00.1c:1 is a bridge from 00 to 05-05
00:1c.2 PCI bridge: Intel Corporation 82801JI (ICH10 Family) PCI Express Root Port 3
## 00.1c:2 is a bridge from 00 to 04-04
00:1c.3 PCI bridge: Intel Corporation 82801JI (ICH10 Family) PCI Express Root Port 4
## 00.1c:3 is a bridge from 00 to 03-03
00:1c.4 PCI bridge: Intel Corporation 82801JI (ICH10 Family) PCI Express Root Port 5
## 00.1c:4 is a bridge from 00 to 02-02
00:1d.0 USB controller: Intel Corporation 82801JI (ICH10 Family) USB UHCI Controller #1
00:1d.1 USB controller: Intel Corporation 82801JI (ICH10 Family) USB UHCI Controller #2
00:1d.2 USB controller: Intel Corporation 82801JI (ICH10 Family) USB UHCI Controller #3
00:1d.7 USB controller: Intel Corporation 82801JI (ICH10 Family) USB2 EHCI Controller #1
00:1e.0 PCI bridge: Intel Corporation 82801 PCI Bridge (rev 90)
## 00.1e:0 is a bridge from 00 to 07-07
00:1f.0 ISA bridge: Intel Corporation 82801JIR (ICH10R) LPC Interface Controller
00:1f.2 SATA controller: Intel Corporation 82801JI (ICH10 Family) SATA AHCI Controller
00:1f.3 SMBus: Intel Corporation 82801JI (ICH10 Family) SMBus Controller
01:00.0 VGA compatible controller: NVIDIA Corporation GK104 [GeForce GTX 670] (rev a1)
01:00.1 Audio device: NVIDIA Corporation GK104 HDMI Audio Controller (rev a1)
02:00.0 IDE interface: Marvell Technology Group Ltd. 88SE6111/6121 SATA II / PATA Controller (rev b1)
03:00.0 Ethernet controller: Marvell Technology Group Ltd. 88E8056 PCI-E Gigabit Ethernet Controller (rev 12)
04:00.0 Ethernet controller: Marvell Technology Group Ltd. 88E8056 PCI-E Gigabit Ethernet Controller (rev 12)
05:00.0 Audio device: Creative Labs Sound Core3D [Sound Blaster Recon3D / Z-Series] (rev 01)
07:00.0 Multimedia video controller: Conexant Systems, Inc. CX23880/1/2/3 PCI Video and Audio Decoder (rev 05)
07:00.1 Multimedia controller: Conexant Systems, Inc. CX23880/1/2/3 PCI Video and Audio Decoder [Audio Port] (rev 05)
07:00.2 Multimedia controller: Conexant Systems, Inc. CX23880/1/2/3 PCI Video and Audio Decoder [MPEG Port] (rev 05)
07:00.4 Multimedia controller: Conexant Systems, Inc. CX23880/1/2/3 PCI Video and Audio Decoder [IR Port] (rev 05)
07:03.0 FireWire (IEEE 1394): VIA Technologies, Inc. VT6306/7/8 [Fire II(M)] IEEE 1394 OHCI Controller (rev c0)

Summary of buses:

00: Primary host bus
	1e.0 Bridge to 07-07
	1c.4 Bridge to 02-02
	1c.3 Bridge to 03-03
	1c.2 Bridge to 04-04
	1c.1 Bridge to 05-05
	1c.0 Bridge to 06-06
	06.0 Bridge to 01-01
01: Entered via 00:06.0
02: Entered via 00:1c.4
03: Entered via 00:1c.3
04: Entered via 00:1c.2
05: Entered via 00:1c.1
07: Entered via 00:1e.0
