+-o Root  <class IORegistryEntry, id 0x100000100, retain 12>
  | {
  |   "IOKitBuildVersion" = "Darwin Kernel Version 15.6.0: Mon Nov 13 21:58:35 PST 2017; root:xnu-3248.72.11~1/RELEASE_X86_64"
  |   "OS Build Version" = "15G18013"
  |   "IONDRVFramebufferGeneration" = <0400000004000000>
  |   "OSKernelCPUSubtype" = 3
  |   "OSKernelCPUType" = 16777223
  |   "OSPrelinkKextCount" = 264
  |   "IOConsoleLocked" = No
  |   "IORegistryPlanes" = {"IOACPIPlane"="IOACPIPlane","IOPower"="IOPower","IODeviceTree"="IODeviceTree","IOService"="IOService","IOFireWire"="IOFireWire","IOUSB"="IOUSB"}
  |   "IOConsoleUsers" = ({"kCGSSessionOnConsoleKey"=Yes,"kCGSSessionLoginwindowSafeLogin"=No,"kSCSecuritySessionID"=100007,"kCGSessionLongUserNameKey"="Manuel","kCGSSessionUserIDKey"=501,"kCGSSessionSystemSafeBoot"=No,"kCGSessionLoginDoneKey"=Yes,"kCGSSessionIDKey"=257,"kCGSSessionGroupIDKey"=20,"kCGSSessionUserNameKey"="manuel","kCGSSessionAuditIDKey"=100007})
  |   "IOKitDiagnostics" = {"Container allocation"=3328293,"Instance allocation"=8036776,"Pageable allocation"=215687696,"Classes"={"CCIOReporterHub"=0,"IOHDIXCommand"=0,"AppleACPIButton"=1,"FakeSMCPlugin"=0,"_IOConfigThread"=0,"nvVirtualAddress"=1879,"IOInterleavedMemoryDescriptor"=0,"IOAGPDevice"=0,"IOHIDPointing"=1,"IOHIDEventRepairDriver"=0,"AppleUSB30HubPort"=0,"IOFWSyncer"=0,"AppleACPICPUInterruptController"=1,"IOUSBRootHubDevice"=0,"OSSerialize"=1,"IOBreaker"=0,"IOFWBusCommand"=1,"IOSMBusController"=1,"IOGraphicsAccelerator2"=1,"AppleUSBEHCIIsochronousRequest"=11,"IOSlowAdaptiveClockingDomain"=0,"AppleUSBHostControllerIsochListElement"=1,"AppleUSBUHCIPCI"=6,"ACPI_SMC_PlatformPlugin"=1,"hv_vmx_space_t"=0,"IOMemoryCursor"=2,"nvDevice"=20,"IOUserClient"=23,"AppleMCP89AHCIPort"=0,"nvCommandQueue"=0,"IOFireWireROMCache"=0,"IORegistryIterator"=0,"IOFWReceiveDCL"=0,"AppleSATAExpressPort"=0,"IOBluetoothHostController"=0,"IOServicePM"=144,"IOUSBLog"=1,"IOBluetoothObject"=0,"IOAccelResource2"=1,"AppleFWOHCI_IsocXmitHelper"=0,"nvTextureBuffer"=920,"AppleSMBusPCI"=1,"OSArray"=5184,"IODVDBlockStorageDevice"=1,"nvVidMemory"=670,"AppleUSBUHCIiTD"=1536,"IOSubMemoryDescriptor"=39,"AppleAHCIDiskPolledInterface"=3,"IOAccelMemory"=2,"OSObject"=112,"AppleUSBUHCIIsochronousEndpoint"=0,"com_apple_driver_pmtelemetry"=1,"IOApplePartitionScheme"=0,"PMHaltWorker"=0,"AppleUSBUHCIDMACommand"=110,"ACPI_SMC_PluginUserClient"=0,"AppleFWOHCI_DCLProgram_U"=0,"IOTimerEventSource"=1797,"IOPCIMessagedInterruptController"=1,"IOMemoryDescriptor"=2,"AppleMCP89AHCI"=0,"IOFWPhysicalAddressSpace"=0,"AppleUSBHostControllerListElement"=3,"AppleIntelPanelA"=1,"com_driver_G13UserClient"=0,"AppleFWOHCI_CallbackEventSource"=3,"AppleACPILid"=0,"__GLNVEvoBasePushBuf"=2,"IOFireWireUnitInfo"=0,"IODTPlatformExpert"=1,"com_apple_driver_pm_cstate_reporter"=1,"AppleMobileFileIntegrity"=1,"AppleUSBHubPolicyMaker"=4,"IOConditionLock"=0,"IOUSBInterfaceIterator"=0,"IOBluetoothMemoryDescriptorRetainer"=0,"AppleUSBController"=4,"IOFWAsyncStreamReceiver"=0,"IOUSBControllerV2"=1,"AppleEFIRuntime"=1,"IOAppleLabelScheme"=0,"IOFireWireDevice"=0,"IOUSBHostPipe"=2,"IOAHCIPort"=1,"IOBluetoothDevice"=0,"IOFWController"=1,"com_apple_driver_pm_reporter"=6,"CCStream"=0,"nvFermiGLContext"=2,"IOHIDWorkLoop"=1,"_IOFramebufferNotifier"=14,"AppleSATAExpress"=0,"AppleUSBHostResourcesClient"=1,"IOHIDUserClient"=1,"IOCommandPool"=8,"AppleUSBInterface"=8,"IOMultiMemoryDescriptor"=0,"nvFermiHAL"=1,"IOBluetoothRFCOMMConnectionUserClient"=0,"IOFWUserAsyncStreamCommand"=0,"IOHIDKeyboard"=2,"OSNumber"=6910,"IOHIDElement"=1,"IOPacketQueue"=0,"PMAssertionsTracker"=1,"AppleGraphicsDeviceControlClient"=1,"nvKeplerSharedPixels"=1,"FakeSMCKeyStoreUserClient"=0,"IOHIDResourceDeviceUserClient"=0,"IOPlatformExpert"=1,"IOServiceMessageUserNotification"=176,"AppleMCCSControlModule"=4,"IOHDACodecFunction"=0,"IODisplayConnect"=2,"IOHDIXHDDriveOutKernel"=0,"IOUSBControllerListElement"=0,"AppleBacklightDisplay"=0,"IOOutputQueue"=1,"IOAccelEventMachineFast2"=1,"IOEventSource"=15,"IORemoteConfigDirectory"=0,"AppleSMBusDevice"=1,"com_apple_AppleFSCompression_AppleFSCompressionTypeDataless"=1,"nvVirtualAddressSpace"=18,"IOUSBMassStorageDriverRequestTimer"=0,"AppleIntelSlowAdaptiveClockingManager"=1,"AppleGraphicsDeviceControl"=1,"IOFramebufferParameterHandler"=4,"AppleUSBEHCIQueueHead"=84,"IOPanicPlatform"=0,"IOSlowAdaptiveClockingManager"=1,"IOUSBControllerV3"=1,"IOBluetoothL2CAPSupervisoryFrameMemoryBlock"=0,"AppleSMC"=1,"OSKext"=112,"AppleFWOHCI_CallbackContainer"=1,"AppleSMBusControllerUserClient"=0,"IOCompactDiscServices"=0,"IOSCSIPeripheralDeviceType07"=0,"IOBluetoothHCIUserClient"=0,"AppleAHCIPortPolledAdapter"=3,"AppleHDAControllerUserClient"=0,"IOBootFramebuffer"=0,"FakeSMCDevice"=1,"IOUSBBus"=1,"AppleUSB30Hub"=0,"AppleEmbeddedKeyboard"=0,"IOBluetoothLocalUtilityEventSource"=0,"OverdriveService"=4,"AppleHDAWorkLoop"=0,"nvGpFifoChannel"=11,"IORootParent"=1,"IOBluetoothSerialClientModemStreamSync"=0,"yukon"=2,"IOAccelChannel2"=1,"nvHAL"=1,"AppleMobileFileIntegrityUserClient"=0,"IOAccelCommandBufferPool2"=0,"IOAccelContext2"=2,"AppleFWOHCI_IOMemoryBlock32"=5,"IOAccelCommandQueue"=0,"IOFireWireMagicMatchingNub"=0,"AppleUSBEHCISplitIsochronousRequestPool"=2,"nvSemaphoreManager"=3,"IOHIDResource"=1,"com_apple_driver_pm_ltr_reporter"=1,"IOAccelMemoryMap"=1,"OverdriveUserClient"=4,"IOMemoryMap"=1268,"IOAccelDeviceShmem"=0,"AppleUSB20InternalIntelHub"=0,"CCIOReporterLogStream"=0,"AppleUSBEHCIDMACommand"=40,"IOAudioDevice"=1,"IOI2CInterface"=1,"IOSCSIMultipathedLogicalUnit"=0,"IOPMPowerSourceList"=0,"IOAccelShared2"=1,"AppleUSBHostBusCurrentPool"=1,"IOUSBMassStorageUASDriver"=0,"IOAudioToggleControl"=4,"IOFWUserLocalIsochPort"=0,"IOAudioStream"=8,"FakeSMCKey"=23,"IOSCSILogicalUnitNub"=4,"IOFireWireBusAux"=1,"AppleUSBEHCIRequestPool"=2,"IOReportLegend"=0,"AppleUSBHostSynchronousRequestCompleter"=7,"nvGpFifoChannelInterface"=11,"IOFWAsyncStreamReceivePort"=0,"IOFWAsyncCommand"=1,"IOAccelDisplayMachine2"=1,"IOPowerConnection"=142,"IOUSBLowLatencyCommandLegacy"=0,"IOPMServiceInterestNotifier"=85,"IOBDServices"=0,"IOPCIBridge"=2,"AppleUSBUHCIRequest"=40,"AppleUSB20InternalSMSCHub"=0,"_IOServiceNotifier"=286,"AppleIntelCPUPowerManagement"=1,"nvSysMemory"=896,"IOFWInterface"=1,"IOHIDKeyboardDevice"=0,"OverdriveHIDPointer"=4,"IOHDAController"=1,"AppleEFINVRAM"=1,"IOPlatformStateSensor"=0,"IOSCSIMultimediaCommandsDevice"=1,"IOPCIDevice"=30,"IOGraphicsDevice"=1,"IOAudioPort"=0,"AppleUSBEHCIRequest"=10,"IOFWUserReadCommand"=0,"IOBluetoothDataQueue"=0,"IOInterruptEventSource"=73,"IOFWUserVectorCommand"=0,"nvVidmemPushBuffer"=0,"IOFireWireUnitAux"=0,"AppleACPIEventController"=1,"IOHDAStream"=0,"IOHIDevice"=2,"IOFWUserPseudoAddressSpace"=0,"IOPMRequest"=0,"IOPlatformPluginFamily"=1,"IOPlatformExpertDevice"=1,"IOHITabletPointer"=0,"IORegistryPlane"=6,"IOUSBInterface"=1,"AppleFWOHCI_ReceiveDCL_U"=0,"IOFireWireUnit"=0,"IOFWPseudoAddressSpaceAux"=2,"AppleAHCIPolledAdapter"=1,"AppleUSBRootHubDevice"=4,"AppleFWOHCI_AsyncTransmitResponse"=1,"AppleUSBHostDARTDMACommand"=0,"IOLittleMemoryCursor"=0,"AppleUSBLegacyRoot"=1,"IOFireWireIRM"=1,"IOFWWorkLoop"=1,"IOFWPHYPacketListener"=0,"AppleFWOHCI_DCLPool"=0,"IOHIDEventDriver"=4,"IOAHCIDiskQueueManager"=1,"IOAccelMemoryInfoUserClient"=3,"IOSurfaceRootUserClient"=30,"IOMbufMemoryCursor"=1,"IOBluetoothACLMemoryDescriptor"=0,"IOAudioControlUserClient"=20,"com_apple_driver_pm_msr_reporter"=1,"AppleFWOHCI_DCLProgram"=0,"BroadcomBluetoothHostController"=0,"IOAccelBlockFencePort2"=0,"IOFWUserWriteCommand"=0,"IOAccelSharedNamespace2"=19,"OSData"=3761,"IODVDMediaBSDClient"=0,"AppleUSBCDCControl"=0,"IOHIDDeviceShim"=0,"IODMACommand"=213,"IOMbufNaturalMemoryCursor"=4,"IOPlatformDevice"=4,"IOPCI2PCIBridge"=7,"IOSortableConfigurationDescriptor"=0,"IOUSBHubDevice"=0,"IOConfigurationDescriptorOrderedSet"=0,"IOBluetoothMemoryBlockQueue"=0,"IOPartitionScheme"=2,"AppleUSBEHCIsiTD"=0,"IOBDBlockStorageDriver"=0,"IOBufferMemoryDescriptor"=815,"IOBluetoothL2CAPChannel"=0,"IOUSBController"=1,"IOAccelDisplayPipeGammaTable2"=0,"IOWatchDogTimer"=2,"OSIterator"=2,"AppleUSBPipe"=5,"IOGeneralMemoryDescriptor"=480,"OSMetaClass"=0,"SCSITaskUserClient"=0,"IOFWLocalIsochPort"=0,"IOBluetoothDeviceUserClient"=0,"OSSymbol"=5493,"OSString"=7490,"IOPlatformControl"=1,"EFIData"=63,"IOFWUserCompareSwapCommand"=0,"IOHistogramReporter"=0,"hv_vcpu_t"=0,"IOKitDiagnosticsClient"=0,"IOHIDLibUserClient"=20,"_IOServiceInterestNotifier"=157,"IOMapper"=0,"IOPlatformSensor"=1,"AppleCredentialManager"=1,"IOUserIterator"=20,"IOAccelEventMachine2"=1,"AppleOSXWatchdog"=1,"IOHIKeyboardMapper"=8,"com_driver_LogJoystick"=1,"IOBluetoothL2CAPSignalChannel"=0,"IOFWSimpleContiguousPhysicalAddressSpace"=0,"AppleIntelPanel"=1,"IOSerialATARequestFIS"=206,"IOUSBMassStorageCBIDriver"=0,"IOFWQEventSource"=1,"IOHIDEventSource"=5,"com_apple_AppleFSCompression_AppleFSCompressionTypeZlib"=1,"AppleUSB20HubExpressCardPort"=0,"nvEvoChannel"=2,"AppleUSBUHCIQueueHeadPool"=6,"IOConfigDirectoryIterator"=0,"IOUSBHostHIDDevice"=1,"IOSCSIPeripheralDeviceType05"=1,"AppleUSBEHCIPipe"=5,"nv2DContext"=4,"IOAHCIPollerInterface"=1,"AppleUSBUHCIRequestPool"=6,"AppleUSB20Hub"=2,"AppleSMBusControllerMCP"=0,"IOCommandGate"=438,"IOHIDConsumer"=2,"AppleFWOHCI_CycleTimeRequest"=0,"IOPMRequestQueue"=2,"AppleUSB20HubPort"=6,"AppleSCSISubsystemGlobals"=1,"IOFWUserCommand"=0,"IOFireWireLocalNode"=1,"IOSerialBSDClient"=1,"IOMediaBSDClient"=8,"IOSCSIProtocolServices"=3,"IOBluetoothRFCOMMConnection"=0,"IOHIDPointingDevice"=0,"IOUSBPortInterruptEventSource"=30,"IONetworkController"=2,"nvHandleManager"=2,"AppleUSBEHCITTInfo"=0,"AppleCredentialManagerUserClient"=0,"IONDRVFramebuffer"=1,"SMCPolledInterface"=1,"CCPipeUserClient"=0,"IODTNVRAM"=1,"AppleUpstreamUserClientDriver"=4,"IOACPIPlatformExpert"=1,"IOUSBMassStorageUFIDriverNub"=0,"AppleUSBHostDMACommand"=2,"AppleUSBHostResources"=1,"com_apple_driver_pm_pch_reporter"=1,"nvChannelManager"=1,"AppleUSBInterfaceIterator"=0,"IOGraphicsWorkLoop"=2,"IOUSBMassStorageInterfaceNub"=1,"AppleUSBUHCIIsochronousRequestPool"=6,"IOHDIXController"=1,"IOSCSIPeripheralDeviceType00"=4,"IOKDP"=0,"IOBluetoothHCIPacketLogUserClient"=0,"nvTimerManager"=1,"IOHIDEventServiceQueue"=0,"nvAccelerator"=1,"IOInterruptController"=5,"IOBluetoothHCIController"=1,"IOAccelerationUserClient"=1,"AppleUSBHostControllerIsochEndpoint"=0,"AppleSMBusController"=1,"AppleMCCSControlCello"=0,"AppleFWOHCI_PM_x86"=1,"AppleUSB30GLHub"=0,"IOFWSimplePhysicalAddressSpace"=0,"FakeSMC"=1,"AppleFWOHCI_SkipCycleDCL"=0,"sk98osx_dnet"=1,"IOUSBCommand"=0,"IOHIDElementPrivate"=1652,"CCLogStream"=0,"AppleUSB20InternalIntelHubClient"=0,"VoodooHDADevice"=2,"IOFramebufferUserClient"=4,"IOStateReporter"=0,"IOFireWireIP"=1,"IOCDBlockStorageDevice"=1,"nvGeneralDisplayLayerBase"=2,"IOFireWireUserClientIniter"=2,"CSRBluetoothHostController"=0,"nvVideoContext"=0,"AppleAHCIRequestTimer"=3,"AppleUSBEHCIPI7C9X440SL"=0,"IOHIDSystem"=1,"IOFWPhysicalAddressSpaceAux"=0,"IOFWRingBufferQ"=0,"SCSITask"=0,"AppleMCP79AHCIPort"=0,"IOFilterScheme"=0,"IOUSBHostStream"=0,"IOCPU"=1,"IOFireWirePowerManager"=1,"AHCIRequest"=165,"RootDomainUserClient"=57,"IOLocalConfigDirectory"=3,"AppleIntelCPUPowerManagementClient"=1,"AppleACPIACAdapter"=0,"OSCollectionIterator"=36,"IOHIDDevice"=2,"IOFWWriteCommand"=0,"AppleKeyStore"=1,"AppleUSBUHCIPipe"=12,"OSSerializer"=78,"IOBlockStorageDevice"=3,"AppleSATLSMARTUserClient"=0,"IOUSBNotification"=0,"nvFermiSharedPixels"=1,"IOAccelSurface2"=1,"PMTraceWorker"=1,"IOAHCIBlockStorageDevice"=3,"AppleAHCIWorkLoop"=6,"nvEventLog"=1,"IOBluetoothL2CAPChannelUserClient"=0,"IOUserEthernetResourceUserClient"=0,"AppleUSBUHCI"=1,"OSDictionary"=9908,"IODVDMedia"=0,"AppleMCCSParameterHandler"=4,"AppleUSBNetworkingCommand"=0,"AppleUSBHostDescriptorCache"=7,"IOUSBHostInterface"=8,"IOReportHub"=1,"AppleICH8AHCI"=0,"AppleMCCSUserClient"=0,"IOHIDEventQueue"=0,"AppleUSBHostPort"=3,"PMSettingObject"=3,"com_apple_driver_pm_msr_limits_reporter"=1,"IOCDMediaBSDClient"=0,"FakeSMCKeyHandler"=0,"IOAudioLevelControl"=8,"IOAudioClientBufferSet"=0,"IOFWUserIsochChannel"=0,"IOHDIXCommandQueue"=0,"AppleSMCClient"=1,"IOEthernetInterface"=2,"IOAudioEngineUserClient"=8,"IOHDIXControllerUserClient"=0,"IOAudioTimeIntervalFilter"=0,"AppleUSBHostDescriptor"=29,"AppleFWOHCI_ReceiveDCL"=0,"AppleOSXWatchdogClient"=1,"IOHDIXHDDriveOutKernelUserClient"=0,"IOUSBMassStorageUASDriverCommand"=0,"IONetworkUserClient"=0,"AppleFWOHCI_AsyncReceiveResponse"=1,"IOHIDStackShotUserClient"=0,"AppleUSBHostRequestPool"=5,"IOFireWireIRMAllocation"=0,"IOSCSIPeripheralDeviceNub"=2,"AppleMCCSControlFamily"=1,"AppleUSBCDCCompositeDevice"=4,"IOFWDCLPool"=0,"IOPMinformeeList"=144,"IOAudioControl"=3,"IOBluetoothSerialClient"=1,"nvMemory"=1,"nvCudaContext"=0,"IOAudioTimeIntervalFilterIIR"=0,"IOAccelStatistics2"=1,"IOUSBMassStorageDriver"=1,"AppleUSBHostBusCurrentClient"=38,"AppleHVClient"=0,"IOBluetoothRFCOMMChannel"=0,"IOHIKeyboard"=3,"yukon2osx"=2,"IOFilterInterruptEventSource"=13,"AppleUSBUHCIIsochronousRequest"=30,"IOHITablet"=1,"IODCLProgram"=0,"IOAccelRangeAllocator"=0,"VoodooHDAUserClient"=0,"AppleACPICPU"=4,"IOSurfaceRoot"=1,"AppleFWOHCI_CycleTimeManager"=1,"NVDA"=4,"CCDataPipe"=0,"AppleSMBusControllerICH"=1,"nvSurface"=10,"FakeSMCSensor"=0,"IOGUIDPartitionScheme"=2,"IOSerialStreamSync"=1,"AppleUSBEHCISplitPeriodicEndpoint"=0,"AppleIntelPchSeriesAHCI"=0,"AppleACPIEventPoller"=1,"IOFireWireControllerAux"=1,"AppleUSBHostIORequestPool"=17,"IOFireWireController"=1,"IORS232SerialStreamSync"=1,"AppleUSBUHCIqTDPool"=6,"IOSCSITargetDevice"=0,"IOHIDEventSystemUserClient"=0,"IOPlatformPluginFamilyPriv"=1,"IOSimpleReporter"=24,"IOPlatformCtrlLoop"=1,"DigitizerTransducer"=0,"IODeblocker"=0,"AppleDisplay"=2,"IOUSBControllerIsochEndpoint"=0,"NVDC"=1,"nvGLContext"=1,"AppleFWOHCI_DMAManager"=1,"IOUSBPipe"=1,"IOSurface"=145,"AppleFWOHCI_MultiIsochReceiver"=1,"IOAccelMemoryAllocator2"=0,"IOAccelDevice2"=1,"nvDisplayManager"=1,"AppleUSBEHCIqTDPool"=2,"IOGatedOutputQueue"=3,"IOSurfaceSendRight"=0,"AppleFWOHCI"=1,"AppleFWOHCI_IsocXmitHelperPort"=0,"IODisplayParameterHandler"=3,"AppleAHCIWatchdogTimer"=3,"_IOOpenServiceIterator"=0,"AppleAHCISerialATAPIWorkLoopLock"=1,"IONetworkStackUserClient"=1,"IOFWPseudoAddressSpace"=2,"IOCommand"=113,"AppleACPIPowerResource"=0,"IOReportUserClient"=1,"SMCWatchDogTimer"=1,"IOHIDResourceQueue"=0,"IOPMPowerSource"=0,"IOAHCISerialATAPI"=1,"AppleMCP79AHCI"=0,"IOBluetoothRFCOMMChannelUserClient"=0,"IOUSBMassStorageUFIDriver"=0,"AppleFWOHCI_AsyncReceive"=2,"IOFWAsyncStreamListener"=0,"IOAccelGLContext2"=1,"IOBacklightDisplay"=0,"SCSITaskUserClientIniter"=1,"IOUSBPipeV2"=1,"OSBoolean"=2,"IOUSBDevice"=1,"IOHIDParamUserClient"=1,"nvCLContext"=0,"IOHIDAsyncReportQueue"=0,"IOAudioEngineEntry"=0,"AppleSMCFamily"=1,"VoodooHDAEngine"=8,"AppleBacklightParameterHandler"=1,"IOBasicOutputQueue"=1,"ACPI_SMC_Idle_CtrlLoop"=0,"IOSCSIPrimaryCommandsDevice"=2,"AppleUSBEHCIQueueHeadPool"=2,"IOAHCIBlockStorageDriver"=1,"IOAccelDisplayPipe2"=4,"IOHDIXHDDriveNub"=0,"IOBluetoothInactivityTimerEventSource"=0,"IONDRVDevice"=4,"AppleUSBEHCIPCI"=2,"IOMbufLittleMemoryCursor"=0,"IOUserNotification"=2,"AppleAHCIDiskQueueManager"=3,"AppleUSBHostCompositeDevice"=1,"nvDisplayLayer"=2,"nvEventManager"=1,"nvPushBuffer"=1,"CCDataPipeUserClient"=0,"IOBlockStorageDriver"=8,"IOService"=134,"IOFWUserAsyncStreamListener"=0,"IOHIDEvent"=0,"IONetworkStack"=1,"IOBluetoothTimerEventSource"=0,"IOSerialDriverSync"=1,"IOUSBHostFamilyLog"=1,"IOAccelBufferMemoryDescriptorPool2"=0,"Dont_Steal_Mac_OS_X"=1,"IORegistryEntry"=19,"CCPipe"=0,"IOFWUserObjectExporter"=1,"AppleUSBHostBusCurrentAllocator"=30,"IODMAController"=0,"IOBootNDRV"=0,"IOFireWireLink"=1,"AppleUSBEHCIiTD"=0,"IOHIPointing"=2,"IOServiceUserNotification"=217,"IOStorage"=3,"IOModemSerialStreamSync"=0,"CCIOReporterDataStream"=0,"AppleUSBUHCIQueueHead"=1536,"IOBluetoothSCOMemoryDescriptorRetainer"=0,"IOPlatformPluginLegacy"=1,"IOAccelCLContext2"=0,"IOHDACodecDevice"=0,"CCLogPipeUserClient"=0,"AppleAPICInterruptController"=1,"IOSMBusRequest"=0,"AppleFWOHCI_PM"=1,"IOFireWireBus"=1,"IOUSBInterfaceUserClientV3"=0,"IOAccelDrawable2"=2,"IOBigMemoryCursor"=0,"nvEvoChannelInterface"=2,"nvGeneralDisplayLayer"=1,"IOHIDProviderPropertyMerger"=0,"IOUSBHIDDriver"=1,"OSCollection"=5,"CCDataStream"=0,"AppleUSBEHCIHubInfo"=1,"IOUSBHostDevice"=7,"AppleRTC"=1,"AppleAHCISerialATAPITimer"=1,"IOSCSIBlockCommandsDevice"=1,"AppleACPIPlatformExpert"=1,"IOPolledFilePollers"=0,"IOHDIXHDDrive"=0,"AppleAHCIWorkLoopLock"=3,"CCLogPipe"=0,"PMSettingHandle"=3,"IOConfigDirectory"=1,"IOFireWireUserClient"=0,"CCCapture"=0,"nvTimerAction"=6,"IOSyncer"=0,"IOAccelerator"=1,"nvRingBuffer"=11,"AppleUSBEHCISplitIsochronousRequest"=10,"IONaturalMemoryCursor"=1,"AppleFWOHCI_IRMSpace"=1,"IOSurfaceClient"=301,"hv_vmx_vm_t"=0,"nvTeslaSharedPixels"=1,"IOUSBHostIOSource"=1,"IOBluetoothHCIRequest"=0,"AHCISMARTUserClient"=0,"nvMemoryMap"=1879,"IONotifier"=3,"EventElementCollection"=0,"IOCatalogue"=1,"AppleUSBEHCI"=1,"AppleUSBHostController"=2,"nvChannelInterface"=2,"IOUSBMassStorageDriverUFIStorageServices"=0,"IOFWReadCommand"=0,"IOUserEthernetResource"=1,"IOBDMediaBSDClient"=0,"AppleFWOHCI_SendDCL"=0,"IOUSBWorkLoop"=4,"AppleUSBNetworkingCommandPool"=0,"IOPolledInterface"=5,"NVDAGK100HAL"=1,"IODVDBlockStorageDriver"=1,"IOSCSIProtocolInterface"=2,"IOFireWireIPDiagnostics"=1,"IOAccelNamespace"=20,"IOKernelDebugger"=0,"IOUSBIsocCommand"=0,"IOMedia"=8,"AppleACPIInterruptLink"=0,"AppleSMCControl"=4,"nvKeplerHAL"=1,"nvShared"=19,"AppleUSBEHCIsiTDPool"=2,"IOHIDInterface"=5,"IOAudioTimeIntervalFilterFIR"=0,"AppleMCCSIOController"=8,"IOAccelAllocationInfo"=0,"AppleUSBHostRequestCompleter"=9,"IOFWUserPHYCommand"=0,"AppleHDAController"=1,"IOFireWireLocalNodeAux"=1,"IOUserEthernetInterface"=0,"IONDRV"=0,"AppleFWOHCI_DescriptorPool"=1,"AppleUSBHostMergeProperties"=1,"AppleUSBIORequest"=85,"IOUSBMassStorageDriverUFIDevice"=0,"IOFWWriteQuadCommand"=0,"AppleHV"=1,"IOFWIsochPort"=0,"IOAccelDisplayPipeUserClient2"=0,"AppleUSBUHCIiTDPool"=6,"AppleAHCIDiskDriver"=3,"yukon2osx_userclient"=0,"IOUSBDeviceUserClientV2"=8,"IOHIDEventSystemQueue"=0,"AppleUSBHostLegacyClient"=7,"IOFWAsyncStreamCommand"=0,"IOAudioEngine"=1,"IOPMWorkQueue"=1,"IOFireWireDeviceAux"=0,"IOPCIDiagnosticsClient"=0,"IOCDPartitionScheme"=0,"AppleFWOHCI_AsyncTransmit"=2,"IOWorkLoop"=73,"IOFireWireMultiIsochReceiveListener"=0,"IOUSBMassStorageDriverNub"=1,"IOPMinformee"=142,"IOUSBNub"=2,"IOUserEthernetController"=0,"IOFWAsyncPHYCommand"=0,"IOPCIConfigurator"=1,"IOUSBUserClientLegacy"=1,"IOFramebufferSharedUserClient"=2,"IOFWReadQuadCommand"=0,"IOSurfaceDeviceCache"=131,"IOBluetoothWorkLoop"=0,"OSSet"=1224,"IOFWSkipCycleDCL"=0,"IOAccelTask"=1,"AppleUSBDiagnostics"=0,"IOBDBlockStorageDevice"=0,"AppleFWOHCI_KDP"=0,"NVDAUser"=0,"nvSysmemPushBuffer"=13,"IOBDMedia"=0,"AppleUSB20KeyboardHub"=0,"AppleFWOHCI_PM_PPC"=0,"IODisplay"=1,"FakeSMCKeyStore"=1,"com_apple_BootCache"=1,"KDIURL"=0,"IOAccelSegmentResourceList"=0,"IOFireWireNubAux"=1,"AppleUSBEHCIIsochronousEndpoint"=0,"IOUSBCommandPool"=0,"nvGpFifoBuffer"=11,"AppleAHCIEventSource"=6,"IOPCIEventSource"=0,"IOMbufBigMemoryCursor"=0,"AppleCSRBluetoothHostController"=0,"IOUSBHubPolicyMaker"=1,"IOUSBInterfaceUserClientV2"=0,"IOFramebufferI2CInterface"=4,"IOAccelVidMemory"=1,"AppleNVMeTranslationSMARTUserClient"=0,"IOPMCompletionQueue"=1,"IOFireWireMultiIsochReceivePacket"=0,"OverdriveUSB"=4,"IOFWUserPHYPacketListener"=0,"AppleUSBEHCIPort"=12,"AppleUSB20InternalHub"=0,"AppleUpstreamUserClient"=0,"AppleKeyStoreUserClient"=4,"AppleAHCIPort"=6,"CCDataSession"=0,"IOBluetoothSerialManager"=1,"IOSharedDataQueue"=0,"IOBlockStorageServices"=4,"IONetworkMedium"=27,"IOFWAddressSpaceAux"=2,"IOBluetoothL2CAPInformationFrameMemoryBlock"=0,"IOBluetoothSerialClientSerialStreamSync"=1,"nvStatistics"=1,"IOHDACodecDriver"=0,"hv_vm_t"=0,"AppleUSBEHCIiTDPool"=2,"AppleUSBDevice"=8,"AppleRTCUserClient"=0,"IOAccelDisplayPipeTransaction2"=0,"AppleUSB20InternalIntelHubPort"=0,"IOFWSendDCL"=0,"IOSCSIHierarchicalLogicalUnit"=0,"IOUSBMassStorageCBIDriverNub"=0,"IONetworkData"=9,"IOFWCompareAndSwapCommand"=1,"AppleUSBHostRequest"=5,"nvSharedUserClient"=19,"IOBluetoothRFCOMMMemoryBlock"=0,"nvCudaInterface"=0,"IOFWAddressSpace"=2,"com_apple_driver_pm_cpu_mbox"=0,"IOAccel2DContext2"=1,"nvPTEEntry"=148,"AppleBroadcomBluetoothHostController"=0,"IODVDServices"=1,"IOI2CInterfaceUserClient"=0,"IOCPUInterruptController"=1,"IOFWDelayCommand"=2,"ACPI_SMC_GPU_CtrlLoop"=0,"IOAccelSharedUserClient2"=1,"IOAccelSysMemory"=1,"IOReporter"=1,"IOAHCIDevice"=4,"IODataQueue"=0,"AppleFWOHCI_AsyncReceiveRequest"=1,"nvSegmentResourceList"=0,"IOUSBInterfaceUserClient"=0,"IOHIDUserDevice"=0,"IOFireWireNub"=1,"com_G13Joystick_Kext"=0,"IOAHCIPortMultiplier"=0,"IOAudioSelectorControl"=8,"IODisplayWrangler"=1,"IOPMPowerStateQueue"=1,"nvSharedPixels"=1,"AppleUSBHubPort"=1,"AppleHPET"=1,"AppleUSBHub"=1,"IOAudioTimerEvent"=1,"IOCDMedia"=0,"AppleFWOHCI_KPF"=0,"IOAccelFIFOChannel2"=0,"CoreCaptureUserClient"=0,"IOPlatformPluginThermalProfile"=0,"hv_vmx_vcpu_t"=0,"AppleSMBIOS"=1,"IOConfigEntry"=13,"CoreCaptureResponder"=1,"AppleVTD"=0,"IOFWIsochChannel"=0,"STUCWorkLoopLock"=0,"IONetworkInterface"=2,"IOPMrootDomain"=1,"AppleAHCI"=1,"IOFDiskPartitionScheme"=1,"IOEthernetController"=1,"ACPI_SMC_CtrlLoop"=2,"IOResources"=1,"IOAccelGPURestartReport2"=0,"IOFWDCL"=0,"AppleUSBEHCIIsochronousRequestPool"=3,"IOFireWireDuplicateGUIDList"=1,"com_apple_driver_pm_cpu_reporter"=1,"IODMAEventSource"=0,"IOUSBControllerIsochListElement"=0,"CCDataPipeBlob"=0,"IOCDBlockStorageDriver"=1,"OSOrderedSet"=202,"IOSharedInterruptController"=6,"_IOServiceJob"=0,"IOFWCommand"=2,"AppleIntelPchSeriesAHCIPort"=0,"IOHIDEventService"=1,"IOPlatformPluginDevice"=0,"AppleUSBNetworkingHostCommandPool"=0,"IOAccelBlockFence"=0,"IOAccelVideoContext2"=0,"IOBluetoothL2CAPMemoryBlock"=0,"IOAccelSubmitter2"=1,"AppleACPIPlatformUserClient"=0,"IOFWUserPhysicalAddressSpace"=0,"OverdriveHIDKeyboard"=4,"IOMachPort"=1476,"IODiskImageBlockStorageDeviceOutKernel"=0,"IOHDACodecDeviceUserClient"=0,"AppleACPIPCI"=1,"IOBluetoothMemoryBlock"=0,"IOFramebuffer"=1,"AppleUSBUHCIPort"=12,"IOUSBDeviceUserClient"=1,"IOAHCIPortInterface"=1,"__GLNVEvoOverlayPushBuf"=0,"IOKitDiagnostics"=1,"AppleUSBHostDeviceIdler"=7,"IOWorkQueue"=3,"IOACPIPlatformDevice"=75,"AppleFDEKeyStoreUserClient"=0,"AppleFWOHCI_AsyncTransmitRequest"=1,"AppleUSBEHCIExpressCardPort"=0,"IORangeAllocator"=2,"AppleFDEKeyStore"=1},"IOMalloc allocation"=60355001}
  | }
  | 
  +-o /  <class IOPlatformExpertDevice, id 0x100000112, registered, matched, active, busy 0 (7166 ms), retain 35>
    | {
    |   "IOInterruptSpecifiers" = (<0900000005000000>)
    |   "IOPolledInterface" = "SMCPolledInterface is not serializable"
    |   "system-type" = <01>
    |   "processor-memory-board-serial-number" = "C02140302D5DMT31M"
    |   "serial-number" = <354a34000000000000000000005738384137374141354a3400000000000000000000000000000000000000>
    |   "platform-feature" = <0000000000000000>
    |   "IOBusyInterest" = "IOCommand is not serializable"
    |   "IOInterruptControllers" = ("io-apic-0")
    |   "version" = <"1.3">
    |   "name" = <"/">
    |   "manufacturer" = <"Apple Inc.">
    |   "compatible" = <"MacPro3,1">
    |   "product-name" = <"MacPro3,1">
    |   "IOConsoleSecurityInterest" = "IOCommand is not serializable"
    |   "IOPlatformSerialNumber" = "W88A77AA5J4"
    |   "clock-frequency" = <004ddb45>
    |   "board-id" = <"Mac-F42C88C8">
    |   "model" = <"MacPro3,1">
    |   "IOGeneralInterest" = "IOCommand is not serializable"
    |   "IOPlatformUUID" = "283D6CE0-DCEB-59C8-AE11-86D6E3524376"
    | }
    | 
    +-o chosen  <class IOService, id 0x100000101, !registered, !matched, active, busy 0, retain 8>
    | | {
    | |   "boot-args" = <"kext-dev-mode=1 rootless=0 -alcdbg -liludbg ">
    | |   "boot-uuid" = <"5C8C0CEE-815F-3B06-95A8-A3F4AB8C53D6">
    | |   "IOScreenLockState" = <01000000>
    | |   "boot-file-path" = <040450005c00530079007300740065006d005c004c006900620072006100720079005c0043006f0072006500530065007200760069006300650073005c0062006f006f0074002e0065006600690000007fff0400>
    | |   "booter-name" = <"boot.efi">
    | |   "random-seed" = <00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000>
    | |   "boot-file" = <"System\Library\PrelinkedKernels\prelinkedkernel">
    | |   "booter-version" = <"version:307.40.6">
    | |   "booter-build-time" = <"Tue Feb  9 17:15:24 PST 2016">
    | |   "machine-signature" = <00000000>
    | |   "IOProgressColorTheme" = 1
    | |   "boot-kernelcache-adler32" = <370584b4>
    | |   "boot-device-path" = <02010c00d041080a0000000001010600021f03120a0000000000000004012a00010000000008000000000000880b5f34000000000c5e22252f7d734aba9ebc4fe5c066f902027fff0400>
    | |   "name" = <"chosen">
    | | }
    | | 
    | +-o memory-map  <class IOService, id 0x100000102, !registered, !matched, active, busy 0, retain 6>
    |     {
    |       "name" = <"memory-map">
    |       "FailedCLUT" = <00c0611700100000>
    |       "FailedImage" = <00d0611720190000>
    |     }
    |     
    +-o efi  <class IOService, id 0x100000103, !registered, !matched, active, busy 0, retain 8>
    | | {
    | |   "firmware-revision" = <72110100>
    | |   "device-properties" = < >
    | |   "firmware-abi" = <"EFI64">
    | |   "name" = <"efi">
    | |   "firmware-vendor" = <43004c004f005600450052000000>
    | | }
    | | 
    | +-o kernel-compatibility  <class IOService, id 0x100000104, !registered, !matched, active, busy 0, retain 4>
    | |   {
    | |     "name" = <"kernel-compatibility">
    | |     "x86_64" = <01000000>
    | |   }
    | |   
    | +-o runtime-services  <class IOService, id 0x100000105, !registered, !matched, active, busy 0, retain 4>
    | |   {
    | |     "name" = <"runtime-services">
    | |     "table" = <18ceaacf00000000>
    | |   }
    | |   
    | +-o configuration-table  <class IOService, id 0x100000106, !registered, !matched, active, busy 0, retain 14>
    | | | {
    | | |   "name" = <"configuration-table">
    | | | }
    | | | 
    | | +-o EB9D2D30-2D88-11D3-9A16-0090273FC14D  <class IOService, id 0x100000107, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "alias" = <"ACPI">
    | | |     "name" = <"EB9D2D30-2D88-11D3-9A16-0090273FC14D">
    | | |     "table" = <00f0c2cf00000000>
    | | |     "guid" = <302d9deb882dd3119a160090273fc14d>
    | | |   }
    | | |   
    | | +-o 587E72D7-CC50-4F79-8209-CA291FC1A10F  <class IOService, id 0x100000108, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"587E72D7-CC50-4F79-8209-CA291FC1A10F">
    | | |     "guid" = <d7727e5850cc794f8209ca291fc1a10f>
    | | |     "table" = <98a7aacf00000000>
    | | |   }
    | | |   
    | | +-o EF9FC172-A1B2-4693-B327-6D32FC416042  <class IOService, id 0x100000109, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"EF9FC172-A1B2-4693-B327-6D32FC416042">
    | | |     "guid" = <72c19fefb2a19346b3276d32fc416042>
    | | |     "table" = <1840a7cf00000000>
    | | |   }
    | | |   
    | | +-o 8868E871-E4F1-11D3-BC22-0080C73C8881  <class IOService, id 0x10000010a, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "alias" = <"ACPI_20">
    | | |     "name" = <"8868E871-E4F1-11D3-BC22-0080C73C8881">
    | | |     "table" = <00f0c2cf00000000>
    | | |     "guid" = <71e86888f1e4d311bc220080c73c8881>
    | | |   }
    | | |   
    | | +-o F2FD1544-9794-4A2C-992E-E5BBCF20E394  <class IOService, id 0x10000010b, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"F2FD1544-9794-4A2C-992E-E5BBCF20E394">
    | | |     "guid" = <4415fdf294972c4a992ee5bbcf20e394>
    | | |     "table" = <0050a8cf00000000>
    | | |   }
    | | |   
    | | +-o EB9D2D31-2D88-11D3-9A16-0090273FC14D  <class IOService, id 0x10000010c, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"EB9D2D31-2D88-11D3-9A16-0090273FC14D">
    | | |     "guid" = <312d9deb882dd3119a160090273fc14d>
    | | |     "table" = <00e0bacf00000000>
    | | |   }
    | | |   
    | | +-o 49152E77-1ADA-4764-B7A2-7AFEFED95E8B  <class IOService, id 0x10000010d, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"49152E77-1ADA-4764-B7A2-7AFEFED95E8B">
    | | |     "guid" = <772e1549da1a6447b7a27afefed95e8b>
    | | |     "table" = <3097cdcf00000000>
    | | |   }
    | | |   
    | | +-o 4C19049F-4137-4DD3-9C10-8B97A83FFDFA  <class IOService, id 0x10000010e, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"4C19049F-4137-4DD3-9C10-8B97A83FFDFA">
    | | |     "guid" = <9f04194c3741d34d9c108b97a83ffdfa>
    | | |     "table" = <808acdcf00000000>
    | | |   }
    | | |   
    | | +-o 7739F24C-93D7-11D4-9A3A-0090273FC14D  <class IOService, id 0x10000010f, !registered, !matched, active, busy 0, retain 4>
    | | |   {
    | | |     "name" = <"7739F24C-93D7-11D4-9A3A-0090273FC14D">
    | | |     "guid" = <4cf23977d793d4119a3a0090273fc14d>
    | | |     "table" = <18806acf00000000>
    | | |   }
    | | |   
    | | +-o 05AD34BA-6F02-4214-952E-4DA0398E2BB9  <class IOService, id 0x100000110, !registered, !matched, active, busy 0, retain 4>
    | |     {
    | |       "name" = <"05AD34BA-6F02-4214-952E-4DA0398E2BB9">
    | |       "guid" = <ba34ad05026f1442952e4da0398e2bb9>
    | |       "table" = <9091cdcf00000000>
    | |     }
    | |     
    | +-o platform  <class IOService, id 0x100000111, !registered, !matched, active, busy 0, retain 6>
    |     {
    |       "REV" = <01300f000003>
    |       "OEMBoard" = <"Maximus II Formula">
    |       "clovergui-revision" = <72110000>
    |       "OEMProduct" = <"Maximus II Formula">
    |       "FSBFrequency" = <8eff761100000000>
    |       "CPUFrequency" = <8040a4ae00000000>
    |       "board-rev" = <01>
    |       "OEMVendor" = <"ASUSTeK Computer INC.">
    |       "InitialTSC" = <0000000000000000>
    |       "EPCI" = <01900700>
    |       "DevicePathsSupported" = <01000000>
    |       "name" = <"platform">
    |       "SystemSerialNumber" = <5700380038004100370037004100410035004a0034000000>
    |       "BEMB" = <00>
    |       "RPlt" = <6d38360000000000>
    |       "Model" = <4d0061006300500072006f0033002c0031000000>
    |       "board-id" = <"Mac-F42C88C8">
    |       "system-id" = <e0fe001e8c00015c7ecd0022153fe0ee>
    |       "RBr" = <6d38360032330000>
    |       "boot-log" = < >
    |       "Settings" = < >
    |     }
    |     
    +-o cpus  <class IOPlatformDevice, id 0x100000119, registered, matched, active, busy 0 (1 ms), retain 10>
    | | {
    | |   "name" = <"cpus">
    | | }
    | | 
    | +-o P001@0  <class IOACPIPlatformDevice, id 0x10000011a, registered, matched, active, busy 0 (2108 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 0
    | |     "clock-frequency" = <8040a4ae>
    | |     "processor-number" = 0
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 1
    | |     "bus-frequency" = <004ddb45>
    | |     "cpu-type" = <0204>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 0
    | |     "name" = <"P001">
    | |   }
    | |   
    | +-o P002@1  <class IOACPIPlatformDevice, id 0x10000011b, registered, matched, active, busy 0 (16 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 1
    | |     "clock-frequency" = <8040a4ae>
    | |     "processor-number" = 1
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 2
    | |     "bus-frequency" = <004ddb45>
    | |     "cpu-type" = <0204>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 1
    | |     "name" = <"P002">
    | |   }
    | |   
    | +-o P003@2  <class IOACPIPlatformDevice, id 0x10000011c, registered, matched, active, busy 0 (17 ms), retain 8>
    | |   {
    | |     "processor-lapic" = 2
    | |     "clock-frequency" = <8040a4ae>
    | |     "processor-number" = 2
    | |     "timebase-frequency" = <00ca9a3b>
    | |     "processor-id" = 3
    | |     "bus-frequency" = <004ddb45>
    | |     "cpu-type" = <0204>
    | |     "device_type" = <"processor">
    | |     "processor-index" = 2
    | |     "name" = <"P003">
    | |   }
    | |   
    | +-o P004@3  <class IOACPIPlatformDevice, id 0x10000011d, registered, matched, active, busy 0 (49 ms), retain 8>
    |     {
    |       "processor-lapic" = 3
    |       "clock-frequency" = <8040a4ae>
    |       "processor-number" = 3
    |       "timebase-frequency" = <00ca9a3b>
    |       "processor-id" = 4
    |       "bus-frequency" = <004ddb45>
    |       "cpu-type" = <0204>
    |       "device_type" = <"processor">
    |       "processor-index" = 3
    |       "name" = <"P004">
    |     }
    |     
    +-o memory  <class IOService, id 0x100000132, !registered, !matched, active, busy 0, retain 4>
    |   {
    |     "dimm-part-number" = <"2G-UDIMM","2G-UDIMM","F2-9600CL5-2GBTD","F2-9600CL5-2GBTD">
    |     "dimm-types" = <"DDR2 SDRAM","DDR2 SDRAM","DDR2 SDRAM","DDR2 SDRAM">
    |     "slot-names" = <"   ","DIMM1","DIMM2","DIMM3","DIMM4">
    |     "dimm-speeds" = <"800 MHz","800 MHz","800 MHz","800 MHz">
    |     "dimm-manufacturer" = <"Kingston","Kingston","G Skill Intl","G Skill Intl">
    |     "ecc-enabled" = No
    |     "reg" = <0000000000000080000000000000008000000000000000800000000000000080>
    |     "dimm-info" = < >
    |     "dimm-serial-number" = <"090101090F010006","0901010902040103","0000000000000000","0000000000000000">
    |   }
    |   
    +-o rom@0  <class IOService, id 0x100000133, !registered, !matched, active, busy 0, retain 4>
    |   {
    |     "rom-size" = 2097152
    |     "vendor" = <"Apple Inc.">
    |     "fv-main-address" = 18446744073707454464
    |     "fv-main-size" = 1048576
    |     "release-date" = <"02/29/08">
    |     "version" = <"MP31.88Z.006C.B05.0802291410">
    |   }
    |   
    +-o PCI0@0  <class IOACPIPlatformDevice, id 0x100000135, registered, matched, active, busy 0 (7059 ms), retain 62>
    | | {
    | |   "compatible" = <"PNP0A03">
    | |   "IODTPersist" = 0
    | |   "_STA" = 18446744073709551615
    | |   "IOPCIConfigured" = Yes
    | |   "acpi-address-spaces" = < >
    | |   "IODeviceMemory" = (({"address"=3320,"length"=8}))
    | |   "#size-cells" = <02000000>
    | |   "_UID" = "0"
    | |   "acpi-pci-routing-table" = < >
    | |   "_ADR" = 0
    | |   "device-properties" = {"acpi-device"="IOACPIPlatformDevice is not serializable","acpi-path"="IOACPIPlane:/_SB/PCI0@0"}
    | |   "#address-cells" = <03000000>
    | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0"
    | |   "name" = <"PNP0A08">
    | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | }
    | | 
    | +-o MCH  <class IOACPIPlatformDevice, id 0x100000136, registered, matched, active, busy 0 (2 ms), retain 7>
    | |   {
    | |     "_STA" = 18446744073709551615
    | |     "_UID" = "10"
    | |     "IODeviceMemory" = (({"address"=4275126272,"length"=24576}))
    | |     "name" = <"PNP0C01">
    | |   }
    | |   
    | +-o P0P2@10000  <class IORegistryEntry, id 0x100000179, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/P0P2@10000"
    | |   }
    | |   
    | +-o PCIE  <class IOACPIPlatformDevice, id 0x10000014b, registered, matched, active, busy 0 (2 ms), retain 7>
    | |   {
    | |     "_STA" = 18446744073709551615
    | |     "_UID" = "17"
    | |     "IODeviceMemory" = (({"address"=3758096384,"length"=268435456}))
    | |     "name" = <"PNP0C02">
    | |   }
    | |   
    | +-o SAT1@1f0005  <class IORegistryEntry, id 0x100000187, retain 6>
    | | | {
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SAT1@1f0005"
    | | | }
    | | | 
    | | +-o CHN0@0  <class IORegistryEntry, id 0x100000188, retain 6>
    | | | | {
    | | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SAT1@1f0005/CHN0@0"
    | | | | }
    | | | | 
    | | | +-o DRV0@0  <class IORegistryEntry, id 0x100000189, retain 4>
    | | | |   {
    | | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SAT1@1f0005/CHN0@0/DRV0@0"
    | | | |   }
    | | | |   
    | | | +-o DRV1@1  <class IORegistryEntry, id 0x10000018a, retain 4>
    | | |     {
    | | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SAT1@1f0005/CHN0@0/DRV1@1"
    | | |     }
    | | |     
    | | +-o CHN1@1  <class IORegistryEntry, id 0x10000018b, retain 6>
    | |   | {
    | |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SAT1@1f0005/CHN1@1"
    | |   | }
    | |   | 
    | |   +-o DRV0@0  <class IORegistryEntry, id 0x10000018c, retain 4>
    | |   |   {
    | |   |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |   |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SAT1@1f0005/CHN1@1/DRV0@0"
    | |   |   }
    | |   |   
    | |   +-o DRV1@1  <class IORegistryEntry, id 0x10000018d, retain 4>
    | |       {
    | |         "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |         "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SAT1@1f0005/CHN1@1/DRV1@1"
    | |       }
    | |       
    | +-o P0P9@1c0005  <class IORegistryEntry, id 0x100000195, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/P0P9@1c0005"
    | |   }
    | |   
    | +-o GBEC@190000  <class IORegistryEntry, id 0x100000196, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/GBEC@190000"
    | |   }
    | |   
    | +-o USB3@1d0003  <class IORegistryEntry, id 0x10000019a, retain 4>
    | |   {
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/USB3@1d0003"
    | |   }
    | |   
    | +-o pci8086,2e20@0  <class IOPCIDevice, id 0x1000001ab, registered, matched, active, busy 0 (16 ms), retain 9>
    | |   {
    | |     "compatible" = <"pci1043,82d3","pci8086,2e20","pciclass,060000">
    | |     "subsystem-vendor-id" = <43100000>
    | |     "IOName" = "pci8086,2e20"
    | |     "reg" = <0000000000000000000000000000000000000000>
    | |     "device-id" = <202e0000>
    | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "IOPCIResourced" = Yes
    | |     "revision-id" = <02000000>
    | |     "vendor-id" = <86800000>
    | |     "pcidebug" = "0:0:0"
    | |     "class-code" = <00000600>
    | |     "name" = <"pci8086,2e20">
    | |     "subsystem-id" = <d3820000>
    | |   }
    | |   
    | +-o P0P3@6  <class IOPCIDevice, id 0x10000017a, registered, matched, active, busy 0 (201 ms), retain 13>
    | | | {
    | | |   "IOPCIPMCSState" = 0
    | | |   "IOInterruptSpecifiers" = (<1000000007000000>)
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOPCIExpressSlotStatus" = 72
    | | |   "subsystem-vendor-id" = <0f000000>
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "pci-aspm-default" = 0
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "built-in" = <00>
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "name" = <"pci-bridge">
    | | |   "vendor-id" = <86800000>
    | | |   "device-id" = <292e0000>
    | | |   "acpi-pmcap-offset" = 128
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = 0
    | | |   "compatible" = <"pcif,0","pci8086,2e29","pciclass,060400","P0P3">
    | | |   "ranges" = <0000008200000000000000f80000008200000000000000f80000000000001001000000c20f00000000000080000000c20f00000000000080000000000000000a000000810000000000a00000000000810000000000a000000000000000100000>
    | | |   "IOPCIExpressLinkCapabilities" = 52513922
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/P0P3@60000"
    | | |   "subsystem-id" = <00000000>
    | | |   "revision-id" = <02000000>
    | | |   "IOPCIExpressLinkStatus" = 20609
    | | |   "IOPCIExpressCapabilities" = 322
    | | |   "pcidebug" = "0:6:0(1:1)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <0030000000000000000000000000000000000000>
    | | |   "IOPCIExpressSlotCapabilities" = 1313920
    | | | }
    | | | 
    | | +-o GFX0@0  <class IOPCIDevice, id 0x10000017b, registered, matched, active, busy 0 (129 ms), retain 27>
    | | | | {
    | | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | | |   "NVDA,noEFI" = <"true">
    | | | |   "assigned-addresses" = <1000018200000000000000f80000000000000001140001c20f0000000000008000000000000000081c0001c20f000000000000880000000000000002240001810000000000ac000000000000800000003000018200000000000000f90000000000000800>
    | | | |   "class-code" = <00000300>
    | | | |   "subsystem-vendor-id" = <62140000>
    | | | |   "NVArch" = "GK100"
    | | | |   "hda-gfx" = <"onboard-1">
    | | | |   "vendor-id" = <de100000>
    | | | |   "IOPCIExpressLinkCapabilities" = 21314819
    | | | |   "IOName" = "display"
    | | | |   "rom-revision" = <"preset 1.0.0">
    | | | |   "IOPCIPMCSState" = 0
    | | | |   "IOPCIMSIMode" = Yes
    | | | |   "VRAM,totalsize" = <00000080>
    | | | |   "IOChildIndex" = 1
    | | | |   "pcidebug" = "1:0:0"
    | | | |   "IOPCIExpressLinkStatus" = 4225
    | | | |   "pci-aspm-default" = 0
    | | | |   "NVCLASS" = "NVDA"
    | | | |   "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | | | |   "IOPCIExpressCapabilities" = 2
    | | | |   "NVCAP" = <050000000000ffffffff00000000000e00000000>
    | | | |   "nvAcceleratorLoaded" = <01000000>
    | | | |   "IOPCIResourced" = Yes
    | | | |   "IOPMIsPowerManaged" = Yes
    | | | |   "IODeviceMemory" = (({"address"=4160749568,"length"=16777216}),({"address"=66571993088,"length"=134217728}),({"address"=66706210816,"length"=33554432}),"IOSubMemoryDescriptor is not serializable",({"address"=4177526784,"length"=524288}))
    | | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | | |   "AAPL,slot-name" = <"PCI Slot 0">
    | | | |   "saved-config" = < >
    | | | |   "name" = <"display">
    | | | |   "subsystem-id" = <10000000>
    | | | |   "AAPL,ndrv-dev" = Yes
    | | | |   "rm_board_number" = <00000000>
    | | | |   "model" = <"NVIDIA GeForce GTX 670">
    | | | |   "VRAM,totalMB" = <00080000>
    | | | |   "device_type" = <"NVDA,Parent">
    | | | |   "compatible" = <"pci1462,2842","pci10de,1189","pciclass,030000","GFX0">
    | | | |   "vbios-revision" = <29005c0480>
    | | | |   "IOHibernateState" = <00000000>
    | | | |   "NVDA,Features" = <00080000>
    | | | |   "NVDAType" = "Official"
    | | | |   "IOReportLegendPublic" = Yes
    | | | |   "IONVRAMProperty" = Yes
    | | | |   "reg" = <0000010000000000000000000000000000000000100001020000000000000000000000000000000114000142000000000000000000000000000000081c0001420000000000000000000000000000000224000101000000000000000000000000800000003000010200000000000000000000000000000800>
    | | | |   "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="GFX0 1"})
    | | | |   "device-id" = <89110000>
    | | | |   "revision-id" = <a2000000>
    | | | |   "IOInterruptSpecifiers" = (<1000000007000000>,<0100000000000100>)
    | | | |   "NVDAinitgl_created" = "yes"
    | | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/P0P3@60000/GFX0@0"
    | | | | }
    | | | | 
    | | | +-o NVDA,Display-A@0  <class IONDRVDevice, id 0x100000385, registered, matched, active, busy 0 (9 ms), retain 8>
    | | | |   {
    | | | |     "display-connect-flags" = <00000000>
    | | | |     "compatible" = <"NVDA,NVMac">
    | | | |     "IOFBDependentIndex" = 0
    | | | |     "nativeNDRV" = <"advn">
    | | | |     "AAPL,RegEntryID" = <f092ecffffffffff0f6d130000000000656d6953000000007a6c755200000000>
    | | | |     "AAPL,ndrv-dev" = Yes
    | | | |     "IODeviceMemory" = (({"address"=4160749568,"length"=16777216}),({"address"=66571993088,"length"=134217728}),({"address"=66706210816,"length"=33554432}),"IOSubMemoryDescriptor is not serializable",({"address"=4177526784,"length"=524288}))
    | | | |     "IOFBDependentID" = 4294967675
    | | | |     "AAPL,gray-page" = <01000000>
    | | | |     "device_type" = <"display">
    | | | |     "NVDA,DeviceClass" = <80000000>
    | | | |     "NVDA,SubDeviceClass" = <80200000>
    | | | |     "av-signal-type" = <02000000>
    | | | |     "display-cfg" = <ffffffff>
    | | | |     "AAPL,gray-value" = <00000000>
    | | | |     "noNVRAM" = <01000000>
    | | | |     "name" = <"NVDA,Display-A">
    | | | |     "port-number" = <00000000>
    | | | |   }
    | | | |   
    | | | +-o NVDA,Display-B@1  <class IONDRVDevice, id 0x100000386, registered, matched, active, busy 0 (5 ms), retain 8>
    | | | |   {
    | | | |     "display-connect-flags" = <00000000>
    | | | |     "compatible" = <"NVDA,NVMac">
    | | | |     "IOFBDependentIndex" = 1
    | | | |     "nativeNDRV" = <"advn">
    | | | |     "AAPL,RegEntryID" = <703b0000000000008fc4ffffffffffff656d6953000000007a6c755200000000>
    | | | |     "AAPL,ndrv-dev" = Yes
    | | | |     "IODeviceMemory" = (({"address"=4160749568,"length"=16777216}),({"address"=66571993088,"length"=134217728}),({"address"=66706210816,"length"=33554432}),"IOSubMemoryDescriptor is not serializable",({"address"=4177526784,"length"=524288}))
    | | | |     "IOFBDependentID" = 4294967675
    | | | |     "AAPL,gray-page" = <01000000>
    | | | |     "device_type" = <"display">
    | | | |     "NVDA,DeviceClass" = <80000000>
    | | | |     "NVDA,SubDeviceClass" = <80200000>
    | | | |     "av-signal-type" = <02000000>
    | | | |     "display-cfg" = <ffffffff>
    | | | |     "AAPL,gray-value" = <00000000>
    | | | |     "noNVRAM" = <01000000>
    | | | |     "name" = <"NVDA,Display-B">
    | | | |     "port-number" = <01000000>
    | | | |   }
    | | | |   
    | | | +-o NVDA,Display-C@2  <class IONDRVDevice, id 0x100000387, registered, matched, active, busy 0 (2 ms), retain 8>
    | | | |   {
    | | | |     "display-connect-flags" = <00000000>
    | | | |     "compatible" = <"NVDA,NVMac">
    | | | |     "IOFBDependentIndex" = 2
    | | | |     "nativeNDRV" = <"advn">
    | | | |     "AAPL,RegEntryID" = <10b2e2ffffffffffef4d1d0000000000656d6953000000007a6c755200000000>
    | | | |     "AAPL,ndrv-dev" = Yes
    | | | |     "IODeviceMemory" = (({"address"=4160749568,"length"=16777216}),({"address"=66571993088,"length"=134217728}),({"address"=66706210816,"length"=33554432}),"IOSubMemoryDescriptor is not serializable",({"address"=4177526784,"length"=524288}))
    | | | |     "IOFBDependentID" = 4294967675
    | | | |     "AAPL,gray-page" = <01000000>
    | | | |     "device_type" = <"display">
    | | | |     "NVDA,DeviceClass" = <80000000>
    | | | |     "NVDA,SubDeviceClass" = <80200000>
    | | | |     "av-signal-type" = <00000000>
    | | | |     "display-cfg" = <ffffffff>
    | | | |     "AAPL,gray-value" = <00000000>
    | | | |     "noNVRAM" = <01000000>
    | | | |     "name" = <"NVDA,Display-C">
    | | | |     "port-number" = <02000000>
    | | | |   }
    | | | |   
    | | | +-o NVDA,Display-D@3  <class IONDRVDevice, id 0x100000388, registered, matched, active, busy 0 (1 ms), retain 8>
    | | |     {
    | | |       "display-connect-flags" = <00000000>
    | | |       "compatible" = <"NVDA,NVMac">
    | | |       "IOFBDependentIndex" = 3
    | | |       "nativeNDRV" = <"advn">
    | | |       "AAPL,RegEntryID" = <f0c7e2ffffffffff0f381d0000000000656d6953000000007a6c755200000000>
    | | |       "AAPL,ndrv-dev" = Yes
    | | |       "IODeviceMemory" = (({"address"=4160749568,"length"=16777216}),({"address"=66571993088,"length"=134217728}),({"address"=66706210816,"length"=33554432}),"IOSubMemoryDescriptor is not serializable",({"address"=4177526784,"length"=524288}))
    | | |       "IOFBDependentID" = 4294967675
    | | |       "AAPL,gray-page" = <01000000>
    | | |       "device_type" = <"display">
    | | |       "NVDA,DeviceClass" = <80000000>
    | | |       "NVDA,SubDeviceClass" = <80200000>
    | | |       "av-signal-type" = <00000000>
    | | |       "display-cfg" = <ffffffff>
    | | |       "AAPL,gray-value" = <00000000>
    | | |       "noNVRAM" = <01000000>
    | | |       "name" = <"NVDA,Display-D">
    | | |       "port-number" = <03000000>
    | | |     }
    | | |     
    | | +-o HDAU@0,1  <class IOPCIDevice, id 0x10000017c, registered, matched, active, busy 0 (103 ms), retain 12>
    | |     {
    | |       "assigned-addresses" = <1001018200000000000008f90000000000400000>
    | |       "IOInterruptSpecifiers" = (<1100000007000000>,<0200000000000100>)
    | |       "class-code" = <00030400>
    | |       "IODeviceMemory" = (({"address"=4178051072,"length"=16384}))
    | |       "IOReportLegendPublic" = Yes
    | |       "PinConfigurations" = <e0005628>
    | |       "subsystem-vendor-id" = <62140000>
    | |       "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |       "pci-aspm-default" = 3
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "built-in" = <00>
    | |       "hda-gfx" = <"onboard-1">
    | |       "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |       "IOPCIMSIMode" = Yes
    | |       "name" = <"pci10de,e0a">
    | |       "IOChildIndex" = 2
    | |       "device-id" = <0a0e0000>
    | |       "vendor-id" = <de100000>
    | |       "layout-id" = <01000000>
    | |       "IOPCIResourced" = Yes
    | |       "compatible" = <"pci1462,2842","pci10de,e0a","pciclass,040300","HDAU">
    | |       "IOPCIExpressLinkCapabilities" = 21314819
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/P0P3@60000/HDAU@1"
    | |       "subsystem-id" = <42280000>
    | |       "revision-id" = <a1000000>
    | |       "IOPCIExpressLinkStatus" = 4225
    | |       "IOPCIExpressCapabilities" = 2
    | |       "pcidebug" = "1:0:1"
    | |       "IOName" = "pci10de,e0a"
    | |       "IOPCIPMCSState" = 0
    | |       "reg" = <00010100000000000000000000000000000000001001010200000000000000000000000000400000>
    | |       "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="HDAU 1"})
    | |     }
    | |     
    | +-o USB4@1A  <class IOPCIDevice, id 0x10000019b, registered, matched, active, busy 0 (44 ms), retain 12>
    | |   {
    | |     "assigned-addresses" = <20d0008100000000009800000000000020000000>
    | |     "IOInterruptSpecifiers" = (<1000000007000000>)
    | |     "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="USB4 0"})
    | |     "class-code" = <00030c00>
    | |     "IODeviceMemory" = ("IOSubMemoryDescriptor is not serializable")
    | |     "IOReportLegendPublic" = Yes
    | |     "built-in" = <00>
    | |     "subsystem-vendor-id" = <43100000>
    | |     "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "IOInterruptControllers" = ("io-apic-0")
    | |     "name" = <"pci8086,3a37">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <373a0000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci1043,82d4","pci8086,3a37","pciclass,0c0300","USB4">
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/USB4@1a0000"
    | |     "subsystem-id" = <d4820000>
    | |     "revision-id" = <00000000>
    | |     "pcidebug" = "0:26:0"
    | |     "IOName" = "pci8086,3a37"
    | |     "device_type" = <"UHCI">
    | |     "reg" = <00d000000000000000000000000000000000000020d0000100000000000000000000000020000000>
    | |     "AAPL,clock-id" = <00>
    | |   }
    | |   
    | +-o USB5@1A,1  <class IOPCIDevice, id 0x10000019c, registered, matched, active, busy 0 (54 ms), retain 12>
    | |   {
    | |     "assigned-addresses" = <20d1008100000000809800000000000020000000>
    | |     "IOInterruptSpecifiers" = (<1500000007000000>)
    | |     "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="USB5 0"})
    | |     "class-code" = <00030c00>
    | |     "IODeviceMemory" = ("IOSubMemoryDescriptor is not serializable")
    | |     "IOReportLegendPublic" = Yes
    | |     "built-in" = <00>
    | |     "subsystem-vendor-id" = <43100000>
    | |     "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "IOInterruptControllers" = ("io-apic-0")
    | |     "name" = <"pci8086,3a38">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <383a0000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci1043,82d4","pci8086,3a38","pciclass,0c0300","USB5">
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/USB5@1a0001"
    | |     "subsystem-id" = <d4820000>
    | |     "revision-id" = <00000000>
    | |     "pcidebug" = "0:26:1"
    | |     "IOName" = "pci8086,3a38"
    | |     "device_type" = <"UHCI">
    | |     "reg" = <00d100000000000000000000000000000000000020d1000100000000000000000000000020000000>
    | |     "AAPL,clock-id" = <00>
    | |   }
    | |   
    | +-o USB6@1A,2  <class IOPCIDevice, id 0x10000019d, registered, matched, active, busy 0 (42 ms), retain 12>
    | |   {
    | |     "assigned-addresses" = <20d2008100000000009c00000000000020000000>
    | |     "IOInterruptSpecifiers" = (<1200000007000000>)
    | |     "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="USB6 0"})
    | |     "class-code" = <00030c00>
    | |     "IODeviceMemory" = ("IOSubMemoryDescriptor is not serializable")
    | |     "IOReportLegendPublic" = Yes
    | |     "built-in" = <00>
    | |     "subsystem-vendor-id" = <43100000>
    | |     "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "IOInterruptControllers" = ("io-apic-0")
    | |     "name" = <"pci8086,3a39">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <393a0000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci1043,82d4","pci8086,3a39","pciclass,0c0300","USB6">
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/USB6@1a0002"
    | |     "subsystem-id" = <d4820000>
    | |     "revision-id" = <00000000>
    | |     "pcidebug" = "0:26:2"
    | |     "IOName" = "pci8086,3a39"
    | |     "device_type" = <"UHCI">
    | |     "reg" = <00d200000000000000000000000000000000000020d2000100000000000000000000000020000000>
    | |     "AAPL,clock-id" = <00>
    | |   }
    | |   
    | +-o USBE@1A,7  <class IOPCIDevice, id 0x10000018f, registered, matched, active, busy 0 (466 ms), retain 12>
    | |   {
    | |     "assigned-addresses" = <10d700820000000000fcfff70000000000040000>
    | |     "IOInterruptSpecifiers" = (<1200000007000000>)
    | |     "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="USBE 0"})
    | |     "class-code" = <20030c00>
    | |     "IODeviceMemory" = (({"address"=4160748544,"length"=1024}))
    | |     "IOReportLegendPublic" = Yes
    | |     "built-in" = <00>
    | |     "subsystem-vendor-id" = <43100000>
    | |     "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "AAPL,current-extra" = 1000
    | |     "IOInterruptControllers" = ("io-apic-0")
    | |     "vendor-id" = <86800000>
    | |     "name" = <"pci8086,3a3c">
    | |     "device-id" = <3c3a0000>
    | |     "acpi-pmcap-offset" = 80
    | |     "IOPCIResourced" = Yes
    | |     "AAPL,current-available" = 1500
    | |     "compatible" = <"pci1043,82d4","pci8086,3a3c","pciclass,0c0320","USBE">
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/USBE@1a0007"
    | |     "AAPL,current-in-sleep" = 3000
    | |     "subsystem-id" = <d4820000>
    | |     "revision-id" = <00000000>
    | |     "IOPCIPMCSState" = 0
    | |     "pcidebug" = "0:26:7"
    | |     "device_type" = <"EHCI">
    | |     "IOName" = "pci8086,3a3c"
    | |     "reg" = <00d700000000000000000000000000000000000010d7000200000000000000000000000000040000>
    | |     "AAPL,clock-id" = <00>
    | |   }
    | |   
    | +-o P0P4@1C  <class IOPCIDevice, id 0x10000019e, registered, matched, active, busy 0 (37 ms), retain 11>
    | |   {
    | |     "IOPCIPMCSState" = 0
    | |     "IOInterruptSpecifiers" = (<1100000007000000>)
    | |     "#address-cells" = <03000000>
    | |     "class-code" = <00040600>
    | |     "IOPCIExpressSlotStatus" = 0
    | |     "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "built-in" = <00>
    | |     "pci-aspm-default" = 0
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "IOInterruptControllers" = ("io-apic-0")
    | |     "vendor-id" = <86800000>
    | |     "name" = <"pci-bridge">
    | |     "device-id" = <403a0000>
    | |     "acpi-pmcap-offset" = 160
    | |     "IOPCIResourced" = Yes
    | |     "IODTPersist" = 0
    | |     "compatible" = <"pci8086,3a40","pciclass,060400","P0P4">
    | |     "ranges" = <0000008200000000000000000000008200000000000000000000000000000000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | |     "IOPCIExpressLinkCapabilities" = 17902609
    | |     "IOPCIConfigured" = Yes
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/P0P4@1c0000"
    | |     "revision-id" = <00000000>
    | |     "IOPCIExpressLinkStatus" = 4097
    | |     "IOPCIExpressCapabilities" = 321
    | |     "pcidebug" = "0:28:0(6:6)"
    | |     "IOName" = "pci-bridge"
    | |     "#size-cells" = <02000000>
    | |     "reg" = <00e0000000000000000000000000000000000000>
    | |     "IOPCIExpressSlotCapabilities" = 1376
    | |   }
    | |   
    | +-o P0P5@1C,1  <class IOPCIDevice, id 0x100000190, registered, matched, active, busy 0 (140 ms), retain 12>
    | | | {
    | | |   "IOPCIPMCSState" = 0
    | | |   "IOInterruptSpecifiers" = (<1000000007000000>)
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOPCIExpressSlotStatus" = 328
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "built-in" = <00>
    | | |   "pci-aspm-default" = 0
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "vendor-id" = <86800000>
    | | |   "name" = <"pci-bridge">
    | | |   "device-id" = <423a0000>
    | | |   "acpi-pmcap-offset" = 160
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = 0
    | | |   "compatible" = <"pci8086,3a42","pciclass,060400","P0P5">
    | | |   "ranges" = <00000082000000000000f0f900000082000000000000f0f90000000000001000000000c20000000000000000000000c2000000000000000000000000000000000000008100000000000000000000008100000000000000000000000000000000>
    | | |   "IOPCIExpressLinkCapabilities" = 34679825
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/P0P5@1c0001"
    | | |   "revision-id" = <00000000>
    | | |   "IOPCIExpressLinkStatus" = 12305
    | | |   "IOPCIExpressCapabilities" = 321
    | | |   "pcidebug" = "0:28:1(5:5)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <00e1000000000000000000000000000000000000>
    | | |   "IOPCIExpressSlotCapabilities" = 1376
    | | | }
    | | | 
    | | +-o pci1102,12@0  <class IOPCIDevice, id 0x1000001af, registered, matched, active, busy 0 (104 ms), retain 11>
    | |     {
    | |       "assigned-addresses" = <100005820000000000c0fff9000000000040000018000582000000000080fff90000000000400000>
    | |       "IOInterruptSpecifiers" = (<1100000007000000>,<0500000000000100>)
    | |       "class-code" = <00030400>
    | |       "IODeviceMemory" = (({"address"=4194287616,"length"=16384}),({"address"=4194271232,"length"=16384}))
    | |       "IOReportLegendPublic" = Yes
    | |       "MaximumBootBeepVolume" = <00>
    | |       "subsystem-vendor-id" = <02110000>
    | |       "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |       "pci-aspm-default" = 0
    | |       "PinConfigurations" = <00>
    | |       "IOPCIMSIMode" = Yes
    | |       "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |       "vendor-id" = <02110000>
    | |       "IOChildIndex" = 1
    | |       "device-id" = <12000000>
    | |       "name" = <"pci1102,12">
    | |       "IOPCIResourced" = Yes
    | |       "layout-id" = <01000000>
    | |       "compatible" = <"pci1102,10","pci1102,12","pciclass,040300">
    | |       "IOPCIExpressLinkCapabilities" = 146449
    | |       "subsystem-id" = <10000000>
    | |       "revision-id" = <01000000>
    | |       "IOPCIExpressLinkStatus" = 4113
    | |       "IOPCIExpressCapabilities" = 2
    | |       "pcidebug" = "5:0:0"
    | |       "IOName" = "pci1102,12"
    | |       "IOPCIPMCSState" = 0
    | |       "reg" = <000005000000000000000000000000000000000010000502000000000000000000000000004000001800050200000000000000000000000000400000>
    | |       "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="pci1102,12 1"})
    | |     }
    | |     
    | +-o P0P6@1C,2  <class IOPCIDevice, id 0x100000191, registered, matched, active, busy 0 (6990 ms), retain 12>
    | | | {
    | | |   "IOPCIPMCSState" = 0
    | | |   "IOInterruptSpecifiers" = (<1200000007000000>)
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOPCIExpressSlotStatus" = 328
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "built-in" = <00>
    | | |   "pci-aspm-default" = 0
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "vendor-id" = <86800000>
    | | |   "name" = <"pci-bridge">
    | | |   "device-id" = <443a0000>
    | | |   "acpi-pmcap-offset" = 160
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = 0
    | | |   "compatible" = <"pci8086,3a44","pciclass,060400","P0P6">
    | | |   "ranges" = <00000082000000000000e0f900000082000000000000e0f90000000000001000000000c20000000000000000000000c200000000000000000000000000000000000000810000000000d00000000000810000000000d000000000000000100000>
    | | |   "IOPCIExpressLinkCapabilities" = 51457041
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/P0P6@1c0002"
    | | |   "revision-id" = <00000000>
    | | |   "IOPCIExpressLinkStatus" = 12305
    | | |   "IOPCIExpressCapabilities" = 321
    | | |   "pcidebug" = "0:28:2(4:4)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <00e2000000000000000000000000000000000000>
    | | |   "IOPCIExpressSlotCapabilities" = 1376
    | | | }
    | | | 
    | | +-o ethernet@0  <class IOPCIDevice, id 0x1000001b0, registered, matched, active, busy 0 (6952 ms), retain 11>
    | |     {
    | |       "assigned-addresses" = <100004820000000000c0eff90000000000400000180004810000000000d800000000000000010000>
    | |       "IOInterruptSpecifiers" = (<1200000007000000>,<0600000000000100>)
    | |       "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="ethernet 1"})
    | |       "class-code" = <00000200>
    | |       "IODeviceMemory" = (({"address"=4193239040,"length"=16384}),"IOSubMemoryDescriptor is not serializable")
    | |       "IOReportLegendPublic" = Yes
    | |       "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |       "subsystem-vendor-id" = <43100000>
    | |       "pci-aspm-default" = 0
    | |       "IOPCIMSIMode" = Yes
    | |       "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |       "vendor-id" = <ab110000>
    | |       "IOChildIndex" = 1
    | |       "device-id" = <64430000>
    | |       "name" = <"ethernet">
    | |       "acpi-pmcap-offset" = 72
    | |       "IOPCIResourced" = Yes
    | |       "compatible" = <"pci1043,81f8","pci11ab,4364","pciclass,020000">
    | |       "IOPCIExpressLinkCapabilities" = 502801
    | |       "model" = "Marvell Yukon Gigabit Adapter 88E8056 Singleport Copper SA"
    | |       "subsystem-id" = <f8810000>
    | |       "IOPCIPMCSState" = 8451
    | |       "revision-id" = <12000000>
    | |       "IOPCIExpressCapabilities" = 17
    | |       "pcidebug" = "4:0:0"
    | |       "IOName" = "ethernet"
    | |       "IOPCIExpressLinkStatus" = 4113
    | |       "reg" = <000004000000000000000000000000000000000010000402000000000000000000000000004000001800040100000000000000000000000000010000>
    | |       "acpi-wake-type" = 2
    | |     }
    | |     
    | +-o P0P7@1C,3  <class IOPCIDevice, id 0x100000192, registered, matched, active, busy 0 (6970 ms), retain 12>
    | | | {
    | | |   "IOPCIPMCSState" = 0
    | | |   "IOInterruptSpecifiers" = (<1300000007000000>)
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOPCIExpressSlotStatus" = 328
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "built-in" = <00>
    | | |   "pci-aspm-default" = 0
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "vendor-id" = <86800000>
    | | |   "name" = <"pci-bridge">
    | | |   "device-id" = <463a0000>
    | | |   "acpi-pmcap-offset" = 160
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = 0
    | | |   "compatible" = <"pci8086,3a46","pciclass,060400","P0P7">
    | | |   "ranges" = <00000082000000000000d0f900000082000000000000d0f90000000000001000000000c20000000000000000000000c200000000000000000000000000000000000000810000000000c00000000000810000000000c000000000000000100000>
    | | |   "IOPCIExpressLinkCapabilities" = 68234257
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/P0P7@1c0003"
    | | |   "revision-id" = <00000000>
    | | |   "IOPCIExpressLinkStatus" = 12305
    | | |   "IOPCIExpressCapabilities" = 321
    | | |   "pcidebug" = "0:28:3(3:3)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <00e3000000000000000000000000000000000000>
    | | |   "IOPCIExpressSlotCapabilities" = 1376
    | | | }
    | | | 
    | | +-o GIGE@0  <class IOPCIDevice, id 0x100000193, registered, matched, active, busy 0 (6944 ms), retain 12>
    | |     {
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/P0P7@1c0003/GIGE@0"
    | |       "assigned-addresses" = <100003820000000000c0dff90000000000400000180003810000000000c800000000000000010000>
    | |       "class-code" = <00000200>
    | |       "subsystem-vendor-id" = <43100000>
    | |       "vendor-id" = <ab110000>
    | |       "IOPCIExpressLinkCapabilities" = 502801
    | |       "IOName" = "ethernet"
    | |       "IOPCIPMCSState" = 8451
    | |       "IOChildIndex" = 1
    | |       "pcidebug" = "3:0:0"
    | |       "IOPCIExpressLinkStatus" = 4113
    | |       "pci-aspm-default" = 0
    | |       "IOPCIExpressCapabilities" = 17
    | |       "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |       "built-in" = <00>
    | |       "IOPCIResourced" = Yes
    | |       "IODeviceMemory" = (({"address"=4192190464,"length"=16384}),"IOSubMemoryDescriptor is not serializable")
    | |       "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |       "AAPL,slot-name" = <"Ethernet">
    | |       "acpi-pmcap-offset" = 72
    | |       "name" = <"ethernet">
    | |       "subsystem-id" = <f8810000>
    | |       "model" = "Marvell Yukon Gigabit Adapter 88E8056 Singleport Copper SA"
    | |       "acpi-wake-type" = 2
    | |       "compatible" = <"pci1043,81f8","pci11ab,4364","pciclass,020000","GIGE">
    | |       "IOReportLegendPublic" = Yes
    | |       "reg" = <000003000000000000000000000000000000000010000302000000000000000000000000004000001800030100000000000000000000000000010000>
    | |       "empty" = 0
    | |       "device-id" = <64430000>
    | |       "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="GIGE 1"})
    | |       "revision-id" = <12000000>
    | |       "IOInterruptSpecifiers" = (<1300000007000000>,<0400000000000100>)
    | |       "IOPCIMSIMode" = Yes
    | |     }
    | |     
    | +-o P0P8@1C,4  <class IOPCIDevice, id 0x100000194, registered, matched, active, busy 0 (37 ms), retain 12>
    | | | {
    | | |   "IOPCIPMCSState" = 0
    | | |   "IOInterruptSpecifiers" = (<1100000007000000>)
    | | |   "#address-cells" = <03000000>
    | | |   "class-code" = <00040600>
    | | |   "IOPCIExpressSlotStatus" = 328
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "built-in" = <00>
    | | |   "pci-aspm-default" = 0
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOInterruptControllers" = ("io-apic-0")
    | | |   "vendor-id" = <86800000>
    | | |   "name" = <"pci-bridge">
    | | |   "device-id" = <483a0000>
    | | |   "acpi-pmcap-offset" = 160
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = 0
    | | |   "compatible" = <"pci8086,3a48","pciclass,060400","P0P8">
    | | |   "ranges" = <00000082000000000000c0f900000082000000000000c0f90000000000001000000000c20000000000000000000000c200000000000000000000000000000000000000810000000000b00000000000810000000000b000000000000000100000>
    | | |   "IOPCIExpressLinkCapabilities" = 85011473
    | | |   "IOPCIConfigured" = Yes
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/P0P8@1c0004"
    | | |   "revision-id" = <00000000>
    | | |   "IOPCIExpressLinkStatus" = 12305
    | | |   "IOPCIExpressCapabilities" = 321
    | | |   "pcidebug" = "0:28:4(2:2)"
    | | |   "IOName" = "pci-bridge"
    | | |   "#size-cells" = <02000000>
    | | |   "reg" = <00e4000000000000000000000000000000000000>
    | | |   "IOPCIExpressSlotCapabilities" = 1376
    | | | }
    | | | 
    | | +-o pci11ab,6121@0  <class IOPCIDevice, id 0x1000001b1, registered, matched, active, busy 0 (16 ms), retain 9>
    | |     {
    | |       "assigned-addresses" = <100002810000000000bc00000000000008000000140002810000000080b800000000000004000000180002810000000000b8000000000000080000001c0002810000000080b400000000000004000000200002810000000000b400000000000010000000240002820000000000fccff90000000000040000>
    | |       "IOInterruptSpecifiers" = (<1000000007000000>,<0300000000000100>)
    | |       "class-code" = <8f010100>
    | |       "IODeviceMemory" = ("IOSubMemoryDescriptor is not serializable","IOSubMemoryDescriptor is not serializable","IOSubMemoryDescriptor is not serializable","IOSubMemoryDescriptor is not serializable","IOSubMemoryDescriptor is not serializable",({"address"=4191157248,"length"=1024}))
    | |       "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |       "subsystem-vendor-id" = <ab110000>
    | |       "pci-aspm-default" = 0
    | |       "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | |       "vendor-id" = <ab110000>
    | |       "IOChildIndex" = 1
    | |       "device-id" = <21610000>
    | |       "name" = <"pci11ab,6121">
    | |       "acpi-pmcap-offset" = 72
    | |       "IOPCIResourced" = Yes
    | |       "compatible" = <"pci11ab,6121","pciclass,01018f">
    | |       "IOPCIExpressLinkCapabilities" = 238609
    | |       "subsystem-id" = <21610000>
    | |       "IOPCIPMCSState" = 0
    | |       "revision-id" = <b1000000>
    | |       "IOPCIExpressCapabilities" = 17
    | |       "pcidebug" = "2:0:0"
    | |       "IOName" = "pci11ab,6121"
    | |       "IOPCIExpressLinkStatus" = 4113
    | |       "reg" = <00000200000000000000000000000000000000001000020100000000000000000000000008000000140002010000000000000000000000000400000018000201000000000000000000000000080000001c0002010000000000000000000000000400000020000201000000000000000000000000100000002400020200000000000000000000000000040000>
    | |     }
    | |     
    | +-o USB0@1D  <class IOPCIDevice, id 0x100000197, registered, matched, active, busy 0 (43 ms), retain 12>
    | |   {
    | |     "assigned-addresses" = <20e8008100000000809000000000000020000000>
    | |     "IOInterruptSpecifiers" = (<1700000007000000>)
    | |     "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="USB0 0"})
    | |     "class-code" = <00030c00>
    | |     "IODeviceMemory" = ("IOSubMemoryDescriptor is not serializable")
    | |     "IOReportLegendPublic" = Yes
    | |     "built-in" = <00>
    | |     "subsystem-vendor-id" = <43100000>
    | |     "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "IOInterruptControllers" = ("io-apic-0")
    | |     "name" = <"pci8086,3a34">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <343a0000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci1043,82d4","pci8086,3a34","pciclass,0c0300","USB0">
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/USB0@1d0000"
    | |     "subsystem-id" = <d4820000>
    | |     "revision-id" = <00000000>
    | |     "pcidebug" = "0:29:0"
    | |     "IOName" = "pci8086,3a34"
    | |     "device_type" = <"UHCI">
    | |     "reg" = <00e800000000000000000000000000000000000020e8000100000000000000000000000020000000>
    | |     "AAPL,clock-id" = <00>
    | |   }
    | |   
    | +-o USB1@1D,1  <class IOPCIDevice, id 0x100000198, registered, matched, active, busy 0 (37 ms), retain 12>
    | |   {
    | |     "assigned-addresses" = <20e9008100000000009400000000000020000000>
    | |     "IOInterruptSpecifiers" = (<1300000007000000>)
    | |     "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="USB1 0"})
    | |     "class-code" = <00030c00>
    | |     "IODeviceMemory" = ("IOSubMemoryDescriptor is not serializable")
    | |     "IOReportLegendPublic" = Yes
    | |     "built-in" = <00>
    | |     "subsystem-vendor-id" = <43100000>
    | |     "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "IOInterruptControllers" = ("io-apic-0")
    | |     "name" = <"pci8086,3a35">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <353a0000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci1043,82d4","pci8086,3a35","pciclass,0c0300","USB1">
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/USB1@1d0001"
    | |     "subsystem-id" = <d4820000>
    | |     "revision-id" = <00000000>
    | |     "pcidebug" = "0:29:1"
    | |     "IOName" = "pci8086,3a35"
    | |     "device_type" = <"UHCI">
    | |     "reg" = <00e900000000000000000000000000000000000020e9000100000000000000000000000020000000>
    | |     "AAPL,clock-id" = <00>
    | |   }
    | |   
    | +-o USB2@1D,2  <class IOPCIDevice, id 0x100000199, registered, matched, active, busy 0 (152 ms), retain 12>
    | |   {
    | |     "assigned-addresses" = <20ea008100000000809400000000000020000000>
    | |     "IOInterruptSpecifiers" = (<1200000007000000>)
    | |     "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="USB2 0"})
    | |     "class-code" = <00030c00>
    | |     "IODeviceMemory" = ("IOSubMemoryDescriptor is not serializable")
    | |     "IOReportLegendPublic" = Yes
    | |     "built-in" = <00>
    | |     "subsystem-vendor-id" = <43100000>
    | |     "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "IOInterruptControllers" = ("io-apic-0")
    | |     "name" = <"pci8086,3a36">
    | |     "vendor-id" = <86800000>
    | |     "device-id" = <363a0000>
    | |     "IOPCIResourced" = Yes
    | |     "compatible" = <"pci1043,82d4","pci8086,3a36","pciclass,0c0300","USB2">
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/USB2@1d0002"
    | |     "subsystem-id" = <d4820000>
    | |     "revision-id" = <00000000>
    | |     "pcidebug" = "0:29:2"
    | |     "IOName" = "pci8086,3a36"
    | |     "device_type" = <"UHCI">
    | |     "reg" = <00ea00000000000000000000000000000000000020ea000100000000000000000000000020000000>
    | |     "AAPL,clock-id" = <00>
    | |   }
    | |   
    | +-o EUSB@1D,7  <class IOPCIDevice, id 0x10000018e, registered, matched, active, busy 0 (45 ms), retain 12>
    | |   {
    | |     "assigned-addresses" = <10ef00820000000000f8fff70000000000040000>
    | |     "IOInterruptSpecifiers" = (<1700000007000000>)
    | |     "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="EUSB 0"})
    | |     "class-code" = <20030c00>
    | |     "IODeviceMemory" = (({"address"=4160747520,"length"=1024}))
    | |     "IOReportLegendPublic" = Yes
    | |     "built-in" = <00>
    | |     "subsystem-vendor-id" = <43100000>
    | |     "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |     "AAPL,current-extra" = 1000
    | |     "IOInterruptControllers" = ("io-apic-0")
    | |     "vendor-id" = <86800000>
    | |     "name" = <"pci8086,3a3a">
    | |     "device-id" = <3a3a0000>
    | |     "acpi-pmcap-offset" = 80
    | |     "IOPCIResourced" = Yes
    | |     "AAPL,current-available" = 1500
    | |     "compatible" = <"pci1043,82d4","pci8086,3a3a","pciclass,0c0320","EUSB">
    | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/EUSB@1d0007"
    | |     "AAPL,current-in-sleep" = 3000
    | |     "subsystem-id" = <d4820000>
    | |     "revision-id" = <00000000>
    | |     "IOPCIPMCSState" = 0
    | |     "pcidebug" = "0:29:7"
    | |     "device_type" = <"EHCI">
    | |     "IOName" = "pci8086,3a3a"
    | |     "reg" = <00ef00000000000000000000000000000000000010ef000200000000000000000000000000040000>
    | |     "AAPL,clock-id" = <00>
    | |   }
    | |   
    | +-o P0P1@1E  <class IOPCIDevice, id 0x10000017d, registered, matched, active, busy 0 (86 ms), retain 16>
    | | | {
    | | |   "compatible" = <"pci8086,244e","pciclass,060401","P0P1">
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "IOName" = "pci-bridge"
    | | |   "reg" = <00f0000000000000000000000000000000000000>
    | | |   "device-id" = <4e240000>
    | | |   "IOPCIConfigured" = Yes
    | | |   "built-in" = <00>
    | | |   "IOPCIResourced" = Yes
    | | |   "IODTPersist" = 0
    | | |   "ranges" = <0000008200000000000000fa0000008200000000000000fa0000000000001004000000c20000000000000000000000c200000000000000000000000000000000000000810000000000e00000000000810000000000e000000000000000100000>
    | | |   "revision-id" = <90000000>
    | | |   "vendor-id" = <86800000>
    | | |   "pcidebug" = "0:30:0(7:7)"
    | | |   "class-code" = <01040600>
    | | |   "#address-cells" = <03000000>
    | | |   "#size-cells" = <02000000>
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/P0P1@1e0000"
    | | |   "name" = <"pci-bridge">
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | | }
    | | | 
    | | +-o pci14f1,8800@0  <class IOPCIDevice, id 0x1000001b2, registered, matched, active, busy 0 (11 ms), retain 9>
    | | |   {
    | | |     "IOChildIndex" = 1
    | | |     "compatible" = <"pci70,9202","pci14f1,8800","pciclass,040000">
    | | |     "subsystem-vendor-id" = <70000000>
    | | |     "IOName" = "pci14f1,8800"
    | | |     "reg" = <00000700000000000000000000000000000000001000070200000000000000000000000000000001>
    | | |     "device-id" = <00880000>
    | | |     "assigned-addresses" = <1000078200000000000000fa0000000000000001>
    | | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |     "IOPCIResourced" = Yes
    | | |     "IODeviceMemory" = (({"address"=4194304000,"length"=16777216}))
    | | |     "revision-id" = <05000000>
    | | |     "IOInterruptControllers" = ("io-apic-0")
    | | |     "vendor-id" = <f1140000>
    | | |     "pcidebug" = "7:0:0"
    | | |     "class-code" = <00000400>
    | | |     "IOInterruptSpecifiers" = (<1000000007000000>)
    | | |     "IOPCIPMCSState" = 0
    | | |     "subsystem-id" = <02920000>
    | | |     "name" = <"pci14f1,8800">
    | | |   }
    | | |   
    | | +-o pci14f1,8801@0,1  <class IOPCIDevice, id 0x1000001b3, registered, matched, active, busy 0 (12 ms), retain 9>
    | | |   {
    | | |     "IOChildIndex" = 2
    | | |     "compatible" = <"pci70,9202","pci14f1,8801","pciclass,048000">
    | | |     "subsystem-vendor-id" = <70000000>
    | | |     "IOName" = "pci14f1,8801"
    | | |     "reg" = <00010700000000000000000000000000000000001001070200000000000000000000000000000001>
    | | |     "device-id" = <01880000>
    | | |     "assigned-addresses" = <1001078200000000000000fb0000000000000001>
    | | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |     "IOPCIResourced" = Yes
    | | |     "IODeviceMemory" = (({"address"=4211081216,"length"=16777216}))
    | | |     "revision-id" = <05000000>
    | | |     "IOInterruptControllers" = ("io-apic-0")
    | | |     "vendor-id" = <f1140000>
    | | |     "pcidebug" = "7:0:1"
    | | |     "class-code" = <00800400>
    | | |     "IOInterruptSpecifiers" = (<1000000007000000>)
    | | |     "IOPCIPMCSState" = 0
    | | |     "subsystem-id" = <02920000>
    | | |     "name" = <"pci14f1,8801">
    | | |   }
    | | |   
    | | +-o pci14f1,8802@0,2  <class IOPCIDevice, id 0x1000001b4, registered, matched, active, busy 0 (11 ms), retain 9>
    | | |   {
    | | |     "IOChildIndex" = 3
    | | |     "compatible" = <"pci70,9202","pci14f1,8802","pciclass,048000">
    | | |     "subsystem-vendor-id" = <70000000>
    | | |     "IOName" = "pci14f1,8802"
    | | |     "reg" = <00020700000000000000000000000000000000001002070200000000000000000000000000000001>
    | | |     "device-id" = <02880000>
    | | |     "assigned-addresses" = <1002078200000000000000fc0000000000000001>
    | | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |     "IOPCIResourced" = Yes
    | | |     "IODeviceMemory" = (({"address"=4227858432,"length"=16777216}))
    | | |     "revision-id" = <05000000>
    | | |     "IOInterruptControllers" = ("io-apic-0")
    | | |     "vendor-id" = <f1140000>
    | | |     "pcidebug" = "7:0:2"
    | | |     "class-code" = <00800400>
    | | |     "IOInterruptSpecifiers" = (<1000000007000000>)
    | | |     "IOPCIPMCSState" = 0
    | | |     "subsystem-id" = <02920000>
    | | |     "name" = <"pci14f1,8802">
    | | |   }
    | | |   
    | | +-o pci14f1,8804@0,4  <class IOPCIDevice, id 0x1000001b5, registered, matched, active, busy 0 (12 ms), retain 9>
    | | |   {
    | | |     "IOChildIndex" = 4
    | | |     "compatible" = <"pci70,9202","pci14f1,8804","pciclass,048000">
    | | |     "subsystem-vendor-id" = <70000000>
    | | |     "IOName" = "pci14f1,8804"
    | | |     "reg" = <00040700000000000000000000000000000000001004070200000000000000000000000000000001>
    | | |     "device-id" = <04880000>
    | | |     "assigned-addresses" = <1004078200000000000000fd0000000000000001>
    | | |     "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |     "IOPCIResourced" = Yes
    | | |     "IODeviceMemory" = (({"address"=4244635648,"length"=16777216}))
    | | |     "revision-id" = <05000000>
    | | |     "IOInterruptControllers" = ("io-apic-0")
    | | |     "vendor-id" = <f1140000>
    | | |     "pcidebug" = "7:0:4"
    | | |     "class-code" = <00800400>
    | | |     "IOInterruptSpecifiers" = (<1000000007000000>)
    | | |     "IOPCIPMCSState" = 0
    | | |     "subsystem-id" = <02920000>
    | | |     "name" = <"pci14f1,8804">
    | | |   }
    | | |   
    | | +-o FRWR@3  <class IOPCIDevice, id 0x10000017e, registered, matched, active, busy 0 (42 ms), retain 12>
    | |     {
    | |       "assigned-addresses" = <1018078200000000000000fe0000000000080000141807810000000000ec00000000000080000000>
    | |       "IOInterruptSpecifiers" = (<1300000007000000>)
    | |       "class-code" = <10000c00>
    | |       "IODeviceMemory" = (({"address"=4261412864,"length"=2048}),"IOSubMemoryDescriptor is not serializable")
    | |       "IOReportLegendPublic" = Yes
    | |       "IOPowerManagement" = {"ChildrenPowerState"=1,"CurrentPowerState"=1,"CapabilityFlags"=0,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | |       "subsystem-vendor-id" = <43100000>
    | |       "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | |       "IOInterruptControllers" = ("io-apic-0")
    | |       "name" = <"pci1106,3044">
    | |       "IOChildIndex" = 5
    | |       "acpi-pmcap-offset" = 80
    | |       "device-id" = <44300000>
    | |       "vendor-id" = <06110000>
    | |       "IOPCIResourced" = Yes
    | |       "compatible" = <"pci1043,81fe","pci1106,3044","pciclass,0c0010","FRWR">
    | |       "fwhub" = <00000000>
    | |       "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/P0P1@1e0000/FRWR@30000"
    | |       "IOPMIsPowerManaged" = Yes
    | |       "subsystem-id" = <fe810000>
    | |       "revision-id" = <c0000000>
    | |       "IOPCIPMCSState" = 0
    | |       "pcidebug" = "7:3:0"
    | |       "IOName" = "pci1106,3044"
    | |       "AAPL,slot-name" = <"FireWire">
    | |       "reg" = <001807000000000000000000000000000000000010180702000000000000000000000000000800001418070100000000000000000000000080000000>
    | |       "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="FRWR 0"})
    | |     }
    | |     
    | +-o SBRG@1F  <class IOPCIDevice, id 0x10000017f, registered, matched, active, busy 0 (14 ms), retain 22>
    | | | {
    | | |   "name" = <"pci8086,3a16">
    | | |   "compatible" = <"pci1043,82d4","pci8086,3a16","pciclass,060100","SBRG">
    | | |   "subsystem-vendor-id" = <43100000>
    | | |   "IOName" = "pci8086,3a16"
    | | |   "reg" = <00f8000000000000000000000000000000000000>
    | | |   "device-id" = <163a0000>
    | | |   "IOPowerManagement" = {"CapabilityFlags"=258,"CurrentPowerState"=2,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "built-in" = <00>
    | | |   "IOPCIResourced" = Yes
    | | |   "revision-id" = <00000000>
    | | |   "vendor-id" = <86800000>
    | | |   "pcidebug" = "0:31:0"
    | | |   "class-code" = <00010600>
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SBRG@1f0000"
    | | |   "subsystem-id" = <d4820000>
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | | }
    | | | 
    | | +-o PIC  <class IOACPIPlatformDevice, id 0x10000013e, registered, matched, active, busy 0 (0 ms), retain 7>
    | | |   {
    | | |     "name" = <"PNP0000">
    | | |     "_STA" = 18446744073709551615
    | | |     "IODeviceMemory" = (({"address"=32,"length"=2}),({"address"=160,"length"=2}))
    | | |   }
    | | |   
    | | +-o DMAD  <class IOACPIPlatformDevice, id 0x10000013f, registered, matched, active, busy 0 (2 ms), retain 7>
    | | |   {
    | | |     "name" = <"PNP0200">
    | | |     "_STA" = 18446744073709551615
    | | |     "IODeviceMemory" = (({"address"=0,"length"=16}),({"address"=129,"length"=3}),({"address"=135,"length"=1}),({"address"=137,"length"=3}),({"address"=143,"length"=1}),({"address"=192,"length"=32}))
    | | |   }
    | | |   
    | | +-o TMR  <class IOACPIPlatformDevice, id 0x100000140, registered, matched, active, busy 0 (2 ms), retain 7>
    | | |   {
    | | |     "name" = <"PNP0100">
    | | |     "_STA" = 18446744073709551615
    | | |     "IODeviceMemory" = (({"address"=64,"length"=4}))
    | | |   }
    | | |   
    | | +-o RTC0  <class IOACPIPlatformDevice, id 0x100000141, registered, matched, active, busy 0 (4 ms), retain 9>
    | | |   {
    | | |     "IODeviceMemory" = (({"address"=112,"length"=2}))
    | | |     "_STA" = 18446744073709551615
    | | |     "IOInterruptSpecifiers" = (<0400000000000000>)
    | | |     "acpi-wake-type" = 4
    | | |     "name" = <"PNP0B00">
    | | |     "IOInterruptControllers" = ("ACPIEventController")
    | | |   }
    | | |   
    | | +-o COPR  <class IOACPIPlatformDevice, id 0x100000142, registered, matched, active, busy 0 (2 ms), retain 7>
    | | |   {
    | | |     "_STA" = 18446744073709551615
    | | |     "IODeviceMemory" = (({"address"=240,"length"=16}))
    | | |     "IOInterruptControllers" = ("io-apic-0")
    | | |     "IOInterruptSpecifiers" = (<0d00000000000000>)
    | | |     "name" = <"PNP0C04">
    | | |   }
    | | |   
    | | +-o FDC  <class IOACPIPlatformDevice, id 0x100000143, registered, matched, active, busy 0 (0 ms), retain 7>
    | | |   {
    | | |     "_STA" = 15
    | | |     "IODeviceMemory" = (({"address"=1008,"length"=6}),({"address"=1015,"length"=1}))
    | | |     "IOInterruptControllers" = ("io-apic-0")
    | | |     "IOInterruptSpecifiers" = (<0600000000000000>)
    | | |     "name" = <"PNP0700">
    | | |   }
    | | |   
    | | +-o SIOR  <class IOACPIPlatformDevice, id 0x100000144, registered, matched, active, busy 0 (0 ms), retain 7>
    | | |   {
    | | |     "_STA" = 18446744073709551615
    | | |     "_UID" = "46"
    | | |     "IODeviceMemory" = (({"address"=656,"length"=16}))
    | | |     "name" = <"PNP0C02">
    | | |   }
    | | |   
    | | +-o RMSC  <class IOACPIPlatformDevice, id 0x100000145, registered, matched, active, busy 0 (1 ms), retain 7>
    | | |   {
    | | |     "_STA" = 18446744073709551615
    | | |     "_UID" = "16"
    | | |     "IODeviceMemory" = (({"address"=16,"length"=16}),({"address"=34,"length"=30}),({"address"=68,"length"=10}),({"address"=80,"length"=16}),({"address"=98,"length"=2}),({"address"=101,"length"=11}),({"address"=114,"length"=14}),({"address"=128,"length"=1}),({"address"=132,"length"=3}),({"address"=136,"length"=1}),({"address"=140,"length"=3}),({"address"=144,"length"=16}),({"address"=162,"length"=30}),({"address"=224,"length"=16}),({"address"=1232,"length"=2}),({"address"=2048,"length"=128}),({"address"=1280,"length"=128}),({"address"=4275077120,"length"=4096}),({"address"=4275159040,"length"=16384}),({"address"=4275175424,"length"=131072}),({"address"=4275372032,"length"=262144}))
    | | |     "name" = <"PNP0C02">
    | | |   }
    | | |   
    | | +-o ASOC  <class IOACPIPlatformDevice, id 0x100000146, registered, matched, active, busy 0 (2 ms), retain 7>
    | | |   {
    | | |     "_UID" = "16843024"
    | | |     "_STA" = 15
    | | |     "name" = <"ATK0110">
    | | |   }
    | | |   
    | | +-o HPET  <class IOACPIPlatformDevice, id 0x100000147, registered, matched, active, busy 0 (3 ms), retain 8>
    | | |   {
    | | |     "_STA" = 15
    | | |     "IODeviceMemory" = (({"address"=4275044352,"length"=1024}))
    | | |     "name" = <"PNP0103">
    | | |     "IOInterruptControllers" = ("io-apic-0","io-apic-0","io-apic-0","io-apic-0")
    | | |     "IOInterruptSpecifiers" = (<0200000000000000>,<0800000000000000>,<0b00000000000000>,<0c00000000000000>)
    | | |     "compatible" = <"PNP0C01">
    | | |   }
    | | |   
    | | +-o FWH  <class IOACPIPlatformDevice, id 0x100000148, registered, matched, active, busy 0 (2 ms), retain 7>
    | | |   {
    | | |     "name" = <"INT0800">
    | | |     "_STA" = 18446744073709551615
    | | |     "IODeviceMemory" = (({"address"=4288675840,"length"=2097152}),({"address"=4292870144,"length"=2097152}))
    | | |   }
    | | |   
    | | +-o FWHE  <class IOACPIPlatformDevice, id 0x100000149, registered, matched, active, busy 0 (2 ms), retain 7>
    | | |   {
    | | |     "_STA" = 18446744073709551615
    | | |     "_UID" = "3"
    | | |     "IODeviceMemory" = (({"address"=4290772992,"length"=2097152}))
    | | |     "name" = <"PNP0C02">
    | | |   }
    | | |   
    | | +-o OMSC  <class IOACPIPlatformDevice, id 0x10000014a, registered, matched, active, busy 0 (2 ms), retain 7>
    | |     {
    | |       "_STA" = 18446744073709551615
    | |       "_UID" = "0"
    | |       "IODeviceMemory" = (({"address"=96,"length"=1}),({"address"=100,"length"=1}),({"address"=4273995776,"length"=4096}),({"address"=4276092928,"length"=4096}))
    | |       "name" = <"PNP0C02">
    | |     }
    | |     
    | +-o SATA@1F,2  <class IOPCIDevice, id 0x100000180, registered, matched, active, busy 0 (6309 ms), retain 18>
    | | | {
    | | |   "assigned-addresses" = <10fa008100000000008c0000000000000800000014fa00810000000080880000000000000400000018fa0081000000000088000000000000080000001cfa00810000000080840000000000000400000020fa00810000000000840000000000002000000024fa00820000000000e8fff70000000000080000>
    | | |   "IOInterruptSpecifiers" = (<1300000007000000>,<0000000000000100>)
    | | |   "class-code" = <01060100>
    | | |   "IODeviceMemory" = ("IOSubMemoryDescriptor is not serializable","IOSubMemoryDescriptor is not serializable","IOSubMemoryDescriptor is not serializable","IOSubMemoryDescriptor is not serializable","IOSubMemoryDescriptor is not serializable",({"address"=4160743424,"length"=2048}))
    | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    | | |   "subsystem-vendor-id" = <43100000>
    | | |   "built-in" = <00>
    | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | |   "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
    | | |   "name" = <"pci8086,3a22">
    | | |   "vendor-id" = <86800000>
    | | |   "acpi-pmcap-offset" = 112
    | | |   "device-id" = <223a0000>
    | | |   "IOPCIResourced" = Yes
    | | |   "compatible" = <"pci1043,82d4","pci8086,3a22","pciclass,010601","SATA">
    | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SATA@1f0002"
    | | |   "subsystem-id" = <d4820000>
    | | |   "IOPCIPMCSState" = 0
    | | |   "revision-id" = <00000000>
    | | |   "pcidebug" = "0:31:2"
    | | |   "IOName" = "pci8086,3a22"
    | | |   "reg" = <00fa00000000000000000000000000000000000010fa00010000000000000000000000000800000014fa00010000000000000000000000000400000018fa0001000000000000000000000000080000001cfa00010000000000000000000000000400000020fa00010000000000000000000000002000000024fa000200000000000000000000000000080000>
    | | | }
    | | | 
    | | +-o CHN0@0  <class AppleAHCIPort, id 0x100000181, registered, matched, active, busy 0 (7 ms), retain 15>
    | | | | {
    | | | |   "AHCI Port ALPM" = No
    | | | |   "IOPolledInterface" = "AppleAHCIPortPolledAdapter is not serializable"
    | | | |   "AHCI Port Hot Plug" = Yes
    | | | |   "IOMaximumSegmentByteCountRead" = 4194304
    | | | |   "64-bit" = Yes
    | | | |   "Trace ID" = 2032128
    | | | |   "IOMaximumSegmentByteCountWrite" = 4194304
    | | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"MaxPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=32768,"ChildProxyPowerState"=2,"DriverPowerState"=2}
    | | | |   "AHCI-Built-In" = Yes
    | | | |   "AHCI Port Command Based" = Yes
    | | | |   "AHCI Port Optimized Device Number" = 0
    | | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | | |   "IOMaximumSegmentCountRead" = 256
    | | | |   "Physical Interconnect Location" = "External"
    | | | |   "AHCI Port SNotification" = Yes
    | | | |   "IOMaximumSegmentCountWrite" = 256
    | | | |   "AHCI Port ESATA" = Yes
    | | | |   "Controller Characteristics" = {"Port Description"="AHCI Version 1.20 Supported","Product Name"="ICH10 AHCI","Vendor Name"="Intel","Port Speed"="3 Gigabit"}
    | | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SATA@1f0002/CHN0@0"
    | | | |   "AHCI Port FIS Based" = No
    | | | |   "Protocol Characteristics" = {"Physical Interconnect"="SATA","Physical Interconnect Location"="External"}
    | | | |   "AHCI-Ejectable" = No
    | | | | }
    | | | | 
    | | | +-o DRV0@0  <class IORegistryEntry, id 0x100000182, retain 4>
    | | | |   {
    | | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SATA@1f0002/CHN0@0/DRV0@0"
    | | | |   }
    | | | |   
    | | | +-o DRV1@1  <class IORegistryEntry, id 0x100000183, retain 4>
    | | | |   {
    | | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SATA@1f0002/CHN0@0/DRV1@1"
    | | | |   }
    | | | |   
    | | | +-o PMP@0  <class IOAHCIDevice, id 0x1000002d7, registered, matched, active, busy 0 (7 ms), retain 12>
    | | |   | {
    | | |   |   "IOUnit" = 0
    | | |   |   "Trace ID" = 2032128
    | | |   |   "Protocol Characteristics" = {"Physical Interconnect"="SATA","AHCI Port Number"=0,"Port Speed"="3 Gigabit","Physical Interconnect Location"="External"}
    | | |   | }
    | | |   | 
    | | |   +-o @0:0  <class IOMedia, id 0x1000002de, registered, matched, active, busy 0 (3 ms), retain 11>
    | | |   |   {
    | | |   |     "Removable" = No
    | | |   |     "Content" = "GUID_partition_scheme"
    | | |   |     "Whole" = Yes
    | | |   |     "Leaf" = No
    | | |   |     "BSD Name" = "disk0"
    | | |   |     "Ejectable" = No
    | | |   |     "Preferred Block Size" = 512
    | | |   |     "IOMediaIcon" = {"IOBundleResourceFile"="External.icns","CFBundleIdentifier"="com.apple.iokit.IOStorageFamily"}
    | | |   |     "BSD Minor" = 0
    | | |   |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |   |     "Writable" = Yes
    | | |   |     "BSD Major" = 1
    | | |   |     "Size" = 500107862016
    | | |   |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |   |     "Open" = Yes
    | | |   |     "Content Hint" = ""
    | | |   |     "BSD Unit" = 0
    | | |   |   }
    | | |   |   
    | | |   +-o @0:1  <class IOMedia, id 0x1000002e5, registered, matched, active, busy 0 (0 ms), retain 11>
    | | |   |   {
    | | |   |     "Removable" = No
    | | |   |     "Content" = "48465300-0000-11AA-AA11-00306543ECAC"
    | | |   |     "Whole" = No
    | | |   |     "Leaf" = Yes
    | | |   |     "BSD Name" = "disk0s1"
    | | |   |     "Ejectable" = No
    | | |   |     "Preferred Block Size" = 512
    | | |   |     "Base" = 1048576
    | | |   |     "BSD Minor" = 1
    | | |   |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |   |     "Writable" = Yes
    | | |   |     "UUID" = "25225E0C-7D2F-4A73-BA9E-BC4FE5C066F9"
    | | |   |     "Partition ID" = 1
    | | |   |     "BSD Major" = 1
    | | |   |     "Size" = 449865781248
    | | |   |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |   |     "Open" = Yes
    | | |   |     "Content Hint" = "48465300-0000-11AA-AA11-00306543ECAC"
    | | |   |     "BSD Unit" = 0
    | | |   |   }
    | | |   |   
    | | |   +-o @0:2  <class IOMedia, id 0x1000002e6, registered, matched, active, busy 0 (0 ms), retain 9>
    | | |       {
    | | |         "Removable" = No
    | | |         "Content" = "C12A7328-F81F-11D2-BA4B-00A0C93EC93B"
    | | |         "Whole" = No
    | | |         "Leaf" = Yes
    | | |         "BSD Name" = "disk0s2"
    | | |         "Ejectable" = No
    | | |         "Preferred Block Size" = 512
    | | |         "Base" = 450001047552
    | | |         "BSD Minor" = 2
    | | |         "IOGeneralInterest" = "IOCommand is not serializable"
    | | |         "Writable" = Yes
    | | |         "UUID" = "679B8C49-7CFB-4191-BE30-FCC7A437F982"
    | | |         "Partition ID" = 2
    | | |         "BSD Major" = 1
    | | |         "Size" = 209715200
    | | |         "IOBusyInterest" = "IOCommand is not serializable"
    | | |         "Open" = No
    | | |         "Content Hint" = "C12A7328-F81F-11D2-BA4B-00A0C93EC93B"
    | | |         "BSD Unit" = 0
    | | |       }
    | | |       
    | | +-o CHN1@1  <class AppleAHCIPort, id 0x100000184, registered, matched, active, busy 0 (4 ms), retain 15>
    | | | | {
    | | | |   "AHCI Port ALPM" = No
    | | | |   "IOPolledInterface" = "AppleAHCIPortPolledAdapter is not serializable"
    | | | |   "AHCI Port Hot Plug" = Yes
    | | | |   "IOMaximumSegmentByteCountRead" = 4194304
    | | | |   "64-bit" = Yes
    | | | |   "Trace ID" = 2032144
    | | | |   "IOMaximumSegmentByteCountWrite" = 4194304
    | | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"MaxPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=32768,"ChildProxyPowerState"=2,"DriverPowerState"=2}
    | | | |   "AHCI-Built-In" = Yes
    | | | |   "AHCI Port Command Based" = Yes
    | | | |   "AHCI Port Optimized Device Number" = 0
    | | | |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | | |   "IOMaximumSegmentCountRead" = 256
    | | | |   "Physical Interconnect Location" = "External"
    | | | |   "AHCI Port SNotification" = Yes
    | | | |   "IOMaximumSegmentCountWrite" = 256
    | | | |   "AHCI Port ESATA" = Yes
    | | | |   "Controller Characteristics" = {"Port Description"="AHCI Version 1.20 Supported","Product Name"="ICH10 AHCI","Vendor Name"="Intel","Port Speed"="3 Gigabit"}
    | | | |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SATA@1f0002/CHN1@1"
    | | | |   "AHCI Port FIS Based" = No
    | | | |   "Protocol Characteristics" = {"Physical Interconnect"="SATA","Physical Interconnect Location"="External"}
    | | | |   "AHCI-Ejectable" = No
    | | | | }
    | | | | 
    | | | +-o DRV0@0  <class IORegistryEntry, id 0x100000185, retain 4>
    | | | |   {
    | | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SATA@1f0002/CHN1@1/DRV0@0"
    | | | |   }
    | | | |   
    | | | +-o DRV1@1  <class IORegistryEntry, id 0x100000186, retain 4>
    | | | |   {
    | | | |     "acpi-device" = "IOACPIPlatformDevice is not serializable"
    | | | |     "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SATA@1f0002/CHN1@1/DRV1@1"
    | | | |   }
    | | | |   
    | | | +-o PMP@0  <class IOAHCIDevice, id 0x100000319, registered, matched, active, busy 0 (4 ms), retain 11>
    | | |   | {
    | | |   |   "IOUnit" = 0
    | | |   |   "Trace ID" = 2032144
    | | |   |   "Protocol Characteristics" = {"Physical Interconnect"="SATA","AHCI Port Number"=0,"Port Speed"="3 Gigabit","Physical Interconnect Location"="External"}
    | | |   | }
    | | |   | 
    | | |   +-o @0:0  <class IOMedia, id 0x100000321, registered, matched, active, busy 0 (1 ms), retain 11>
    | | |   |   {
    | | |   |     "Removable" = No
    | | |   |     "Content" = "FDisk_partition_scheme"
    | | |   |     "Whole" = Yes
    | | |   |     "Leaf" = No
    | | |   |     "BSD Name" = "disk1"
    | | |   |     "Ejectable" = No
    | | |   |     "Preferred Block Size" = 512
    | | |   |     "IOMediaIcon" = {"IOBundleResourceFile"="External.icns","CFBundleIdentifier"="com.apple.iokit.IOStorageFamily"}
    | | |   |     "BSD Minor" = 3
    | | |   |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |   |     "Writable" = Yes
    | | |   |     "BSD Major" = 1
    | | |   |     "Size" = 500107862016
    | | |   |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |   |     "Open" = Yes
    | | |   |     "Content Hint" = ""
    | | |   |     "BSD Unit" = 1
    | | |   |   }
    | | |   |   
    | | |   +-o @0:1  <class IOMedia, id 0x100000327, registered, matched, active, busy 0 (0 ms), retain 10>
    | | |       {
    | | |         "Removable" = No
    | | |         "Content" = "Windows_NTFS"
    | | |         "Whole" = No
    | | |         "Leaf" = Yes
    | | |         "BSD Name" = "disk1s1"
    | | |         "Ejectable" = No
    | | |         "Preferred Block Size" = 512
    | | |         "Base" = 1048576
    | | |         "BSD Minor" = 4
    | | |         "IOGeneralInterest" = "IOCommand is not serializable"
    | | |         "Writable" = Yes
    | | |         "Partition ID" = 1
    | | |         "BSD Major" = 1
    | | |         "Size" = 449126583296
    | | |         "IOBusyInterest" = "IOCommand is not serializable"
    | | |         "Open" = Yes
    | | |         "Content Hint" = "Windows_NTFS"
    | | |         "BSD Unit" = 1
    | | |       }
    | | |       
    | | +-o PRT2@2  <class AppleAHCIPort, id 0x10000031b, registered, matched, active, busy 0 (21 ms), retain 13>
    | | | | {
    | | | |   "AHCI Port ALPM" = No
    | | | |   "IOPolledInterface" = "AppleAHCIPortPolledAdapter is not serializable"
    | | | |   "AHCI Port Hot Plug" = Yes
    | | | |   "IOMaximumSegmentByteCountRead" = 4194304
    | | | |   "64-bit" = Yes
    | | | |   "Trace ID" = 2032160
    | | | |   "IOMaximumSegmentByteCountWrite" = 4194304
    | | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"MaxPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=32768,"ChildProxyPowerState"=2,"DriverPowerState"=2}
    | | | |   "AHCI-Built-In" = Yes
    | | | |   "AHCI Port Command Based" = Yes
    | | | |   "AHCI Port Optimized Device Number" = 0
    | | | |   "IOMaximumSegmentCountRead" = 256
    | | | |   "Physical Interconnect Location" = "External"
    | | | |   "AHCI Port ESATA" = Yes
    | | | |   "AHCI Port SNotification" = Yes
    | | | |   "IOMaximumSegmentCountWrite" = 256
    | | | |   "Controller Characteristics" = {"Port Description"="AHCI Version 1.20 Supported","Product Name"="ICH10 AHCI","Vendor Name"="Intel","Port Speed"="3 Gigabit"}
    | | | |   "AHCI Port FIS Based" = No
    | | | |   "Protocol Characteristics" = {"Physical Interconnect"="SATA","Physical Interconnect Location"="External"}
    | | | |   "AHCI-Ejectable" = No
    | | | | }
    | | | | 
    | | | +-o PMP@0  <class IOAHCIDevice, id 0x100000331, registered, matched, active, busy 0 (21 ms), retain 12>
    | | |   | {
    | | |   |   "IOUnit" = 0
    | | |   |   "Trace ID" = 2032160
    | | |   |   "Protocol Characteristics" = {"Physical Interconnect"="SATA","AHCI Port Number"=0,"Port Speed"="1.5 Gigabit","Physical Interconnect Location"="External"}
    | | |   | }
    | | |   | 
    | | |   +-o @0:0  <class IOMedia, id 0x10000033a, registered, matched, active, busy 0 (17 ms), retain 11>
    | | |   |   {
    | | |   |     "Removable" = No
    | | |   |     "Content" = "GUID_partition_scheme"
    | | |   |     "Whole" = Yes
    | | |   |     "Leaf" = No
    | | |   |     "BSD Name" = "disk2"
    | | |   |     "Ejectable" = No
    | | |   |     "Preferred Block Size" = 512
    | | |   |     "IOMediaIcon" = {"IOBundleResourceFile"="External.icns","CFBundleIdentifier"="com.apple.iokit.IOStorageFamily"}
    | | |   |     "BSD Minor" = 5
    | | |   |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |   |     "Writable" = Yes
    | | |   |     "BSD Major" = 1
    | | |   |     "Size" = 500107862016
    | | |   |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |   |     "Open" = Yes
    | | |   |     "Content Hint" = ""
    | | |   |     "BSD Unit" = 2
    | | |   |   }
    | | |   |   
    | | |   +-o @0:1  <class IOMedia, id 0x100000340, registered, matched, active, busy 0 (0 ms), retain 9>
    | | |   |   {
    | | |   |     "Removable" = No
    | | |   |     "Content" = "C12A7328-F81F-11D2-BA4B-00A0C93EC93B"
    | | |   |     "Whole" = No
    | | |   |     "Leaf" = Yes
    | | |   |     "BSD Name" = "disk2s1"
    | | |   |     "Ejectable" = No
    | | |   |     "Preferred Block Size" = 512
    | | |   |     "Base" = 20480
    | | |   |     "BSD Minor" = 6
    | | |   |     "IOGeneralInterest" = "IOCommand is not serializable"
    | | |   |     "Writable" = Yes
    | | |   |     "UUID" = "9F2DF056-59BB-4697-905A-B8885AE162C4"
    | | |   |     "Partition ID" = 1
    | | |   |     "BSD Major" = 1
    | | |   |     "Size" = 209715200
    | | |   |     "IOBusyInterest" = "IOCommand is not serializable"
    | | |   |     "Open" = No
    | | |   |     "Content Hint" = "C12A7328-F81F-11D2-BA4B-00A0C93EC93B"
    | | |   |     "BSD Unit" = 2
    | | |   |   }
    | | |   |   
    | | |   +-o @0:2  <class IOMedia, id 0x100000341, registered, matched, active, busy 0 (0 ms), retain 10>
    | | |       {
    | | |         "Removable" = No
    | | |         "Content" = "48465300-0000-11AA-AA11-00306543ECAC"
    | | |         "Whole" = No
    | | |         "Leaf" = Yes
    | | |         "BSD Name" = "disk2s2"
    | | |         "Ejectable" = No
    | | |         "Preferred Block Size" = 512
    | | |         "Base" = 209735680
    | | |         "BSD Minor" = 7
    | | |         "IOGeneralInterest" = "IOCommand is not serializable"
    | | |         "Writable" = Yes
    | | |         "UUID" = "68830374-F9F0-44F7-9EC0-3BE9463DCD86"
    | | |         "Partition ID" = 2
    | | |         "BSD Major" = 1
    | | |         "Size" = 499763888128
    | | |         "IOBusyInterest" = "IOCommand is not serializable"
    | | |         "Open" = Yes
    | | |         "Content Hint" = "48465300-0000-11AA-AA11-00306543ECAC"
    | | |         "BSD Unit" = 2
    | | |       }
    | | |       
    | | +-o PRT3@3  <class AppleAHCIPort, id 0x100000332, registered, matched, active, busy 0 (139 ms), retain 13>
    | | | | {
    | | | |   "AHCI Port Optimized Device Number" = 0
    | | | |   "AHCI Port Hot Plug" = Yes
    | | | |   "AHCI Port Command Based" = Yes
    | | | |   "Controller Characteristics" = {"Port Description"="AHCI Version 1.20 Supported","Product Name"="ICH10 AHCI","Vendor Name"="Intel","Port Speed"="3 Gigabit"}
    | | | |   "IOMaximumSegmentCountWrite" = 256
    | | | |   "IOPowerManagement" = {"ChildrenPowerState"=2,"MaxPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=32768,"ChildProxyPowerState"=2,"DriverPowerState"=2}
    | | | |   "IOMaximumSegmentByteCountWrite" = 4194304
    | | | |   "IOMaximumSegmentByteCountRead" = 4194304
    | | | |   "Trace ID" = 2032176
    | | | |   "AHCI Port FIS Based" = No
    | | | |   "AHCI-Ejectable" = No
    | | | |   "Protocol Characteristics" = {"Physical Interconnect"="SATA","Physical Interconnect Location"="External"}
    | | | |   "64-bit" = Yes
    | | | |   "AHCI-Built-In" = Yes
    | | | |   "IOMaximumSegmentCountRead" = 256
    | | | |   "Physical Interconnect Location" = "External"
    | | | |   "AHCI Port ESATA" = Yes
    | | | |   "AHCI Port ALPM" = No
    | | | |   "AHCI Port SNotification" = Yes
    | | | | }
    | | | | 
    | | | +-o PMP@0  <class IOAHCIDevice, id 0x1000003b0, registered, matched, active, busy 0 (139 ms), retain 9>
    | | |     {
    | | |       "IOUnit" = 0
    | | |       "Trace ID" = 2032176
    | | |       "Protocol Characteristics" = {"Physical Interconnect"="SATA","AHCI Port Number"=0,"Port Speed"="1.5 Gigabit","Physical Interconnect Location"="External","ATAPI"=Yes}
    | | |     }
    | | |     
    | | +-o PRT4@4  <class AppleAHCIPort, id 0x1000003b1, registered, matched, active, busy 0 (0 ms), retain 10>
    | | |   {
    | | |     "AHCI Port Optimized Device Number" = 0
    | | |     "AHCI Port Hot Plug" = Yes
    | | |     "AHCI Port Command Based" = Yes
    | | |     "Controller Characteristics" = {"Port Description"="AHCI Version 1.20 Supported","Product Name"="ICH10 AHCI","Vendor Name"="Intel","Port Speed"="3 Gigabit"}
    | | |     "IOMaximumSegmentCountWrite" = 256
    | | |     "IOPowerManagement" = {"MaxPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=32768,"ChildProxyPowerState"=2,"DriverPowerState"=2}
    | | |     "IOMaximumSegmentByteCountWrite" = 4194304
    | | |     "IOMaximumSegmentByteCountRead" = 4194304
    | | |     "Trace ID" = 2032192
    | | |     "AHCI Port FIS Based" = No
    | | |     "AHCI-Ejectable" = No
    | | |     "Protocol Characteristics" = {"Physical Interconnect"="SATA","Physical Interconnect Location"="External"}
    | | |     "64-bit" = Yes
    | | |     "AHCI-Built-In" = Yes
    | | |     "IOMaximumSegmentCountRead" = 256
    | | |     "Physical Interconnect Location" = "External"
    | | |     "AHCI Port ESATA" = Yes
    | | |     "AHCI Port ALPM" = No
    | | |     "AHCI Port SNotification" = Yes
    | | |   }
    | | |   
    | | +-o PRT5@5  <class AppleAHCIPort, id 0x1000003ff, registered, matched, active, busy 0 (0 ms), retain 10>
    | |     {
    | |       "AHCI Port Optimized Device Number" = 0
    | |       "AHCI Port Hot Plug" = Yes
    | |       "AHCI Port Command Based" = Yes
    | |       "Controller Characteristics" = {"Port Description"="AHCI Version 1.20 Supported","Product Name"="ICH10 AHCI","Vendor Name"="Intel","Port Speed"="3 Gigabit"}
    | |       "IOMaximumSegmentCountWrite" = 256
    | |       "IOPowerManagement" = {"MaxPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=32768,"ChildProxyPowerState"=2,"DriverPowerState"=2}
    | |       "IOMaximumSegmentByteCountWrite" = 4194304
    | |       "IOMaximumSegmentByteCountRead" = 4194304
    | |       "Trace ID" = 2032208
    | |       "AHCI Port FIS Based" = No
    | |       "AHCI-Ejectable" = No
    | |       "Protocol Characteristics" = {"Physical Interconnect"="SATA","Physical Interconnect Location"="External"}
    | |       "64-bit" = Yes
    | |       "AHCI-Built-In" = Yes
    | |       "IOMaximumSegmentCountRead" = 256
    | |       "Physical Interconnect Location" = "External"
    | |       "AHCI Port ESATA" = Yes
    | |       "AHCI Port ALPM" = No
    | |       "AHCI Port SNotification" = Yes
    | |     }
    | |     
    | +-o SBUS@1F,3  <class IOPCIDevice, id 0x10000019f, registered, matched, active, busy 0 (53 ms), retain 12>
    |   | {
    |   |   "assigned-addresses" = <10fb00820f0000000000008a000000000001000020fb008100000000000400000000000020000000>
    |   |   "IOInterruptSpecifiers" = (<1200000007000000>)
    |   |   "IODeviceMemory" = (({"address"=66739765248,"length"=256}),"IOSubMemoryDescriptor is not serializable")
    |   |   "class-code" = <00050c00>
    |   |   "built-in" = <00>
    |   |   "subsystem-vendor-id" = <43100000>
    |   |   "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
    |   |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    |   |   "IOInterruptControllers" = ("io-apic-0")
    |   |   "vendor-id" = <86800000>
    |   |   "name" = <"SMBus controller">
    |   |   "device-id" = <303a0000>
    |   |   "IOPCIResourced" = Yes
    |   |   "compatible" = <"pci1043,82d4","pci8086,3a30","pciclass,0c0500","SBUS">
    |   |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SBUS@1f0003"
    |   |   "model" = <"Intel 82801JI ICH10 Family">
    |   |   "subsystem-id" = <d4820000>
    |   |   "revision-id" = <00000000>
    |   |   "pcidebug" = "0:31:3"
    |   |   "IOName" = "pci8086,3a30"
    |   |   "reg" = <00fb00000000000000000000000000000000000010fb00020000000000000000000000000001000020fb000100000000000000000000000020000000>
    |   | }
    |   | 
    |   +-o BUS0@0  <class IORegistryEntry, id 0x1000001a0, retain 5>
    |     | {
    |     |   "acpi-device" = "IOACPIPlatformDevice is not serializable"
    |     |   "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SBUS@1f0003/BUS0@0"
    |     | }
    |     | 
    |     +-o DVL0@57  <class IORegistryEntry, id 0x1000001a1, retain 4>
    |         {
    |           "address" = 87
    |           "acpi-device" = "IOACPIPlatformDevice is not serializable"
    |           "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/SBUS@1f0003/BUS0@0/DVL0@57"
    |         }
    |         
    +-o RMEM  <class IOACPIPlatformDevice, id 0x10000016e, registered, matched, active, busy 0 (1 ms), retain 7>
    |   {
    |     "_STA" = 18446744073709551615
    |     "_UID" = "1"
    |     "IODeviceMemory" = (({"address"=0,"length"=655360}),({"address"=786432,"length"=65536}),({"address"=917504,"length"=131072}),({"address"=1048576,"length"=3488612352}))
    |     "name" = <"PNP0C01">
    |   }
    |   
    +-o PNLF  <class IOACPIPlatformDevice, id 0x10000016f, registered, matched, active, busy 0 (2501 ms), retain 8>
    |   {
    |     "_STA" = 11
    |     "_UID" = "10"
    |     "name" = <"APP0002">
    |     "compatible" = <"backlight">
    |   }
    |   
    +-o PWRB  <class IOACPIPlatformDevice, id 0x100000170, registered, matched, active, busy 0 (4 ms), retain 9>
    |   {
    |     "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182005248,4295098369,"               First Level Interrupt Handler Count"),(5291294645182005249,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182005250,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182005251,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182005252,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="PWRB 0"})
    |     "_UID" = "170"
    |     "IOReportLegendPublic" = Yes
    |     "IOInterruptControllers" = ("ACPIEventController")
    |     "_STA" = 11
    |     "IOInterruptSpecifiers" = (<0200000000000000>)
    |     "name" = <"PNP0C0C">
    |     "acpi-wake-type" = 1
    |   }
    |   
    +-o LNKA  <class IOACPIPlatformDevice, id 0x100000171, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "1"
    |     "_STA" = 11
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKB  <class IOACPIPlatformDevice, id 0x100000172, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "2"
    |     "_STA" = 11
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKC  <class IOACPIPlatformDevice, id 0x100000173, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "3"
    |     "_STA" = 11
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKD  <class IOACPIPlatformDevice, id 0x100000174, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "4"
    |     "_STA" = 11
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKE  <class IOACPIPlatformDevice, id 0x100000175, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "5"
    |     "_STA" = 9
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKF  <class IOACPIPlatformDevice, id 0x100000176, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "6"
    |     "_STA" = 11
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKG  <class IOACPIPlatformDevice, id 0x100000177, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "7"
    |     "_STA" = 9
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o LNKH  <class IOACPIPlatformDevice, id 0x100000178, !registered, !matched, active, busy 0, retain 5>
    |   {
    |     "_UID" = "8"
    |     "_STA" = 11
    |     "name" = <"PNP0C0F">
    |   }
    |   
    +-o options  <class AppleEFINVRAM, id 0x1000001ae, registered, matched, active, busy 0 (0 ms), retain 546>
        {
          "fakesmc-key-MSWr-ui8" = <00>
          "flagstate" = <0000000000000000000000000000000000000000000000000000000000000000>
          "fakesmc-key-RBr -ch8*" = <6d38360032330000>
          "fakesmc-key-EPCI-ui32" = <01900700>
          "fakesmc-key-MSAc-ui16" = <0000>
          "efi-boot-device" = <"<array><dict><key>IOMatch</key><dict><key>IOProviderClass</key><string>IOMedia</string><key>IOPropertyMatch</key><dict><key>UUID</key><string>25225E0C-7D2F-4A73-BA9E-BC4FE5C066F9</string></dict></dict></dict></array>">
          "fakesmc-key-CLKH-{clh" = <0000708000011940>
          "bootercfg" = <"(">
          "fakesmc-key-NATi-ui16" = <0000>
          "fakesmc-key-NTOK-ui8" = <01>
          "fakesmc-key-BATP-flag" = <00>
          "fakesmc-key-$Num-ui8" = <01>
          "fakesmc-key-REV -ch8*" = <01300f000003>
          "fmm-computer-name" = <"Manuel-PC">
          "fakesmc-key-MSLD-ui8" = <00>
          "fakesmc-key-MSTc-ui8" = <00>
          "Clover.KeepBackupLimit" = <30>
          "fakesmc-key-MSPS-ui16" = <0003>
          "fakesmc-key-RMde-char" = <41>
          "Clover.Theme" = <"LightUp">
          "csr-active-config" = <67000000>
          "fakesmc-key-RPlt-ch8*" = <6d38360000000000>
          "fakesmc-key-BEMB-flag" = <00>
          "fakesmc-key-#KEY-ui32" = <00000017>
          "boot-args" = "kext-dev-mode=1 rootless=0"
          "fakesmc-key-MSFW-ui8" = <0100>
          "SystemAudioVolume" = <01>
          "security-mode" = "none"
          "install-product-url" = <"x-osproduct://55B4090A-C041-3176-AFF3-294AEBACC868/OS%20X%20Install%20Data">
          "fakesmc-key-$Adr-ui32" = <00000300>
          "EFILoginHiDPI" = <00000000>
          "fakesmc-key-CLKT-ui32" = <0001403b>
          "fakesmc-key-MSDW-ui8" = <01>
          "fakesmc-key-BNum-ui8" = <00>
          "SystemAudioVolumeDB" = <ee>
          "fakesmc-key-NATJ-ui8" = <00>
          "efi-boot-device-data" = <02010c00d041080a0000000001010600021f03120a0000000000000004012a00010000000008000000000000880b5f34000000000c5e22252f7d734aba9ebc4fe5c066f902027fff0400>
          "prev-lang:kbd" = <"de:4711">
          "rc_imgsrc_info" = <62706c6973743030a101d102035f102435354234303930412d433034312d333137362d414646332d323934414542414343383638594d6176657269636b73080a0d34000000000000010100000000000000040000000000000000000000000000003e>
        }
        
