Found a device of class VoodooHDADevice: IOService:/AppleACPIPlatformExpert/PCI0@0/AppleACPIPCI/P0P3@6/IOPP/HDAU@0,1/VoodooHDADevice


Probing codec #0...
 HDA Codec #0: NVidia (Unknown)
 HDA Codec ID: 0x10de0040
       Vendor: 0x10de
       Device: 0x0040
     Revision: 0x01
     Stepping: 0x00
PCI Subvendor: 0x28421462
	startNode=1 endNode=2
	Found audio FG nid=1 startNode=4 endNode=12 total=8

Processing audio FG cad=0 nid=1...
Powering up...
Parsing audio FG...
GPIO: 0x00000000 NumGPIO=0 NumGPO=0 NumGPI=0 GPIWake=0 GPIUnsol=0
 nid  4 0x185600f0 as 15 seq  0 Digital-out   Jack  Digital Special Internal Unknown misc 0
 nid  5 0x185600f0 as 15 seq  0 Digital-out   Jack  Digital Special Internal Unknown misc 0
 nid  6 0x185600f0 as 15 seq  0 Digital-out   Jack  Digital Special Internal Unknown misc 0
 nid  7 0x185600f0 as 15 seq  0 Digital-out   Jack  Digital Special Internal Unknown misc 0
Parsing vendor patch...
Nodes patching. Codec = 0 
NumNodes = 2
VHDevice NID= 4 Config=185600f0 (pin: Digital-o) Cap=09000094 Ctrl=00000000 -- Conns: 0=8 1=9 2=10 3=11
VHDevice NID= 5 Config=185600f0 (pin: Digital-o) Cap=09000094 Ctrl=00000000 -- Conns: 0=8 1=9 2=10 3=11
VHDevice NID= 6 Config=185600f0 (pin: Digital-o) Cap=09000094 Ctrl=00000000 -- Conns: 0=8 1=9 2=10 3=11
VHDevice NID= 7 Config=185600f0 (pin: Digital-o) Cap=09000094 Ctrl=00000000 -- Conns: 0=8 1=9 2=10 3=11
VHDevice NID= 8 Config=00000000 (audio output  ) Cap=00000000 Ctrl=00000000 -- Conns:
VHDevice NID= 9 Config=00000000 (audio output  ) Cap=00000000 Ctrl=00000000 -- Conns:
VHDevice NID=10 Config=00000000 (audio output  ) Cap=00000000 Ctrl=00000000 -- Conns:
VHDevice NID=11 Config=00000000 (audio output  ) Cap=00000000 Ctrl=00000000 -- Conns:
Parsing Ctls...
Disabling nonaudio...
Disabling useless...
Patched pins configuration:
 nid  4 0x185600f0 as 15 seq  0 Digital-out   Jack  Digital Special Internal Unknown misc 0
 nid  5 0x185600f0 as 15 seq  0 Digital-out   Jack  Digital Special Internal Unknown misc 0
 nid  6 0x185600f0 as 15 seq  0 Digital-out   Jack  Digital Special Internal Unknown misc 0
 nid  7 0x185600f0 as 15 seq  0 Digital-out   Jack  Digital Special Internal Unknown misc 0
Parsing pin associations...
4 associations found:
Association 0 (15) out:
 Pin nid=4 seq=0
   Redir type=-1 jack=0 def=-1
Association 1 (15) out:
 Pin nid=5 seq=0
   Redir type=-1 jack=0 def=-1
Association 2 (15) out:
 Pin nid=6 seq=0
   Redir type=-1 jack=0 def=-1
Association 3 (15) out:
 Pin nid=7 seq=0
   Redir type=-1 jack=0 def=-1
Building AFG tree...
Tracing association 0 (15)
 Tracing pin 4 with min nid 0
   nid 8 returned 8
   nid 9 returned 9
   nid 10 returned 10
   nid 11 returned 11
  nid 4 returned 8
 Pin 4 traced to DAC 8
Association 0 (15) trace succeeded
Tracing association 1 (15)
 Tracing pin 5 with min nid 0
   nid 8 busy by association 0
   nid 9 returned 9
   nid 10 returned 10
   nid 11 returned 11
  nid 5 returned 9
 Pin 5 traced to DAC 9
Association 1 (15) trace succeeded
Tracing association 2 (15)
 Tracing pin 6 with min nid 0
   nid 8 busy by association 0
   nid 9 busy by association 1
   nid 10 returned 10
   nid 11 returned 11
  nid 6 returned 10
 Pin 6 traced to DAC 10
Association 2 (15) trace succeeded
Tracing association 3 (15)
 Tracing pin 7 with min nid 0
   nid 8 busy by association 0
   nid 9 busy by association 1
   nid 10 busy by association 2
   nid 11 returned 11
  nid 7 returned 11
 Pin 7 traced to DAC 11
Association 3 (15) trace succeeded
Tracing input monitor
Tracing other input monitors
Tracing beeper
Disabling unassociated widgets...
Disabling nonselected inputs...
Disabling useless...
Disabling crossassociated connections...
Disabling useless...
Binding associations to channels...
Assigning names to signal sources...
Assigning mixers to the tree...
Preparing pin controls...
AFG commit...
Creating PCM devices...
pcmAttach: HDA NVidia (Unknown) PCM #0 DisplayPort at cad 0 nid 1
+--------------------------------------+
| DUMPING PCM Playback/Record Channels |
+--------------------------------------+

Playback:

     Stream cap: 0x00000005
                 AC3 PCM
        PCM cap: 0x000e07f0
                 16 20 24 bits, 32 44 48 88 96 176 192 KHz
            DAC: 8

+-------------------------------+
| DUMPING Playback/Record Paths |
+-------------------------------+

Playback:

    nid=4 [pin: Digital-out (HDMI)]
      |
      + <- nid=8 [audio output] [src: pcm] bindSeq=00000001


+-------------------------+
| DUMPING Volume Controls |
+-------------------------+

OSS mixer initialization...
Registering PCM channels...
pcmAttach: HDA NVidia (Unknown) PCM #1 DisplayPort at cad 0 nid 1
+--------------------------------------+
| DUMPING PCM Playback/Record Channels |
+--------------------------------------+

Playback:

     Stream cap: 0x00000005
                 AC3 PCM
        PCM cap: 0x000e07f0
                 16 20 24 bits, 32 44 48 88 96 176 192 KHz
            DAC: 9

+-------------------------------+
| DUMPING Playback/Record Paths |
+-------------------------------+

Playback:

    nid=5 [pin: Digital-out (HDMI)]
      |
      + <- nid=9 [audio output] [src: pcm] bindSeq=00000001


+-------------------------+
| DUMPING Volume Controls |
+-------------------------+

OSS mixer initialization...
Registering PCM channels...
pcmAttach: HDA NVidia (Unknown) PCM #2 DisplayPort at cad 0 nid 1
+--------------------------------------+
| DUMPING PCM Playback/Record Channels |
+--------------------------------------+

Playback:

     Stream cap: 0x00000005
                 AC3 PCM
        PCM cap: 0x000e07f0
                 16 20 24 bits, 32 44 48 88 96 176 192 KHz
            DAC: 10

+-------------------------------+
| DUMPING Playback/Record Paths |
+-------------------------------+

Playback:

    nid=6 [pin: Digital-out (HDMI)]
      |
      + <- nid=10 [audio output] [src: pcm] bindSeq=00000001


+-------------------------+
| DUMPING Volume Controls |
+-------------------------+

OSS mixer initialization...
Registering PCM channels...
pcmAttach: HDA NVidia (Unknown) PCM #3 DisplayPort at cad 0 nid 1
+--------------------------------------+
| DUMPING PCM Playback/Record Channels |
+--------------------------------------+

Playback:

     Stream cap: 0x00000005
                 AC3 PCM
        PCM cap: 0x000e07f0
                 16 20 24 bits, 32 44 48 88 96 176 192 KHz
            DAC: 11

+-------------------------------+
| DUMPING Playback/Record Paths |
+-------------------------------+

Playback:

    nid=7 [pin: Digital-out (HDMI)]
      |
      + <- nid=11 [audio output] [src: pcm] bindSeq=00000001


+-------------------------+
| DUMPING Volume Controls |
+-------------------------+

OSS mixer initialization...
Registering PCM channels...
FG config/quirks: forcestereo ivref50 ivref80 ivref100 ivref
HP switch init...

+-------------------+
| DUMPING HDA NODES |
+-------------------+

Default Parameter
-----------------
         IN amp: 0x00000000
        OUT amp: 0x00000000

            nid: 4
           Name: pin: Digital-out (HDMI)
     Widget cap: 0x00407381
                 CP DIGITAL UNSOL 8CH
    Association: 0 (0x00000001)
        Pin cap: 0x09000094
                 PDC OUT HDMI DP HBR
     Pin config: 0x185600f0
    Pin control: 0x00000040 OUT
    connections: 4 enabled 1
          |
          + <- nid=8 [audio output] (selected)
          + [DISABLED] <- nid=9 [audio output]
          + [DISABLED] <- nid=10 [audio output]
          + [DISABLED] <- nid=11 [audio output]

            nid: 5
           Name: pin: Digital-out (HDMI)
     Widget cap: 0x00407381
                 CP DIGITAL UNSOL 8CH
    Association: 1 (0x00000001)
        Pin cap: 0x09000094
                 PDC OUT HDMI DP HBR
     Pin config: 0x185600f0
    Pin control: 0x00000040 OUT
    connections: 4 enabled 1
          |
          + [DISABLED] <- nid=8 [audio output]
          + <- nid=9 [audio output] (selected)
          + [DISABLED] <- nid=10 [audio output]
          + [DISABLED] <- nid=11 [audio output]

            nid: 6
           Name: pin: Digital-out (HDMI)
     Widget cap: 0x00407381
                 CP DIGITAL UNSOL 8CH
    Association: 2 (0x00000001)
        Pin cap: 0x09000094
                 PDC OUT HDMI DP HBR
     Pin config: 0x185600f0
    Pin control: 0x00000040 OUT
    connections: 4 enabled 1
          |
          + [DISABLED] <- nid=8 [audio output]
          + [DISABLED] <- nid=9 [audio output]
          + <- nid=10 [audio output] (selected)
          + [DISABLED] <- nid=11 [audio output]

            nid: 7
           Name: pin: Digital-out (HDMI)
     Widget cap: 0x00407381
                 CP DIGITAL UNSOL 8CH
    Association: 3 (0x00000001)
        Pin cap: 0x09000094
                 PDC OUT HDMI DP HBR
     Pin config: 0x185600f0
    Pin control: 0x00000040 OUT
    connections: 4 enabled 1
          |
          + [DISABLED] <- nid=8 [audio output]
          + [DISABLED] <- nid=9 [audio output]
          + [DISABLED] <- nid=10 [audio output]
          + <- nid=11 [audio output] (selected)

            nid: 8
           Name: audio output
     Widget cap: 0x000062b1
                 DIGITAL UNSOL STRIPE(x4) FORMAT_OVR 8CH
    Association: 0 (0x00000001)
            OSS: pcm (pcm)
     Stream cap: 0x00000005
                 AC3 PCM
        PCM cap: 0x000e07f0
                 16 20 24 bits, 32 44 48 88 96 176 192 KHz

            nid: 9
           Name: audio output
     Widget cap: 0x000062b1
                 DIGITAL UNSOL STRIPE(x4) FORMAT_OVR 8CH
    Association: 1 (0x00000001)
            OSS: pcm (pcm)
     Stream cap: 0x00000005
                 AC3 PCM
        PCM cap: 0x000e07f0
                 16 20 24 bits, 32 44 48 88 96 176 192 KHz

            nid: 10
           Name: audio output
     Widget cap: 0x000062b1
                 DIGITAL UNSOL STRIPE(x4) FORMAT_OVR 8CH
    Association: 2 (0x00000001)
            OSS: pcm (pcm)
     Stream cap: 0x00000005
                 AC3 PCM
        PCM cap: 0x000e07f0
                 16 20 24 bits, 32 44 48 88 96 176 192 KHz

            nid: 11
           Name: audio output
     Widget cap: 0x000062b1
                 DIGITAL UNSOL STRIPE(x4) FORMAT_OVR 8CH
    Association: 3 (0x00000001)
            OSS: pcm (pcm)
     Stream cap: 0x00000005
                 AC3 PCM
        PCM cap: 0x000e07f0
                 16 20 24 bits, 32 44 48 88 96 176 192 KHz


Found a device of class VoodooHDADevice: IOService:/AppleACPIPlatformExpert/PCI0@0/AppleACPIPCI/P0P5@1C,1/IOPP/pci1102,12@0/VoodooHDADevice


Probing codec #1...
 HDA Codec #1: Realtek ALC899
 HDA Codec ID: 0x10ec0899
       Vendor: 0x10ec
       Device: 0x0899
     Revision: 0x00
     Stepping: 0x03
PCI Subvendor: 0x00101102
	startNode=1 endNode=2
	Found audio FG nid=1 startNode=2 endNode=39 total=37

Processing audio FG cad=1 nid=1...
Powering up...
Parsing audio FG...
GPIO: 0x40000002 NumGPIO=2 NumGPO=0 NumGPI=0 GPIWake=0 GPIUnsol=1
 nid 17 0x40130000 as  0 seq  0 Speaker       None  ATAPI   N/A     External Unknown misc 0
 nid 18 0x411111f0 as 15 seq  0 Speaker       None  1/8     Rear    External Black   misc 0 NoPresenceDetect
 nid 20 0x01014010 as  1 seq  0 Line-out      Jack  1/8     Rear    External Green   misc 0
 nid 21 0x01011012 as  1 seq  2 Line-out      Jack  1/8     Rear    External Black   misc 0
 nid 22 0x01016011 as  1 seq  1 Line-out      Jack  1/8     Rear    External Orange  misc 0
 nid 23 0x41012014 as  1 seq  4 Line-out      None  1/8     Rear    External Grey    misc 0
 nid 24 0x01a19040 as  4 seq  0 Microphone    Jack  1/8     Rear    External Pink    misc 0
 nid 25 0x02a19050 as  5 seq  0 Microphone    Jack  1/8     Front   External Pink    misc 0
 nid 26 0x01813060 as  6 seq  0 Line-in       Jack  1/8     Rear    External Blue    misc 0
 nid 27 0x0221401f as  1 seq 15 Headphones    Jack  1/8     Front   External Green   misc 0
 nid 28 0x411111f0 as 15 seq  0 Speaker       None  1/8     Rear    External Black   misc 0 NoPresenceDetect
Patching widget caps nid=29 0x00400400 -> 0x00700400
 nid 30 0x41441130 as  3 seq  0 SPDIF-out     None  RCA     Rear    External Black   misc 0 NoPresenceDetect
 nid 31 0x41c46170 as  7 seq  0 SPDIF-in      None  RCA     Rear    External Orange  misc 0 NoPresenceDetect
Parsing vendor patch...
Nodes patching. Codec = 1 
NumNodes = 2
VHDevice NID= 2 Config=00000000 (audio output  ) Cap=00000000 Ctrl=00000000 -- Conns:
VHDevice NID= 3 Config=00000000 (audio output  ) Cap=00000000 Ctrl=00000000 -- Conns:
VHDevice NID= 4 Config=00000000 (audio output  ) Cap=00000000 Ctrl=00000000 -- Conns:
VHDevice NID= 5 Config=00000000 (audio output  ) Cap=00000000 Ctrl=00000000 -- Conns:
VHDevice NID= 6 Config=00000000 (audio output  ) Cap=00000000 Ctrl=00000000 -- Conns:
VHDevice NID= 7 Config=00000000 (audio input   ) Cap=00000000 Ctrl=00000000 -- Conns: 0=36
VHDevice NID= 8 Config=00000000 (audio input   ) Cap=00000000 Ctrl=00000000 -- Conns: 0=35
VHDevice NID= 9 Config=00000000 (audio input   ) Cap=00000000 Ctrl=00000000 -- Conns: 0=34
VHDevice NID=10 Config=00000000 (audio input   ) Cap=00000000 Ctrl=00000000 -- Conns: 0=31
VHDevice NID=11 disabled for Realtek by user info.list
VHDevice NID=12 Config=00000000 (audio mixer   ) Cap=00000000 Ctrl=00000000 -- Conns: 0=2 1=11
VHDevice NID=13 Config=00000000 (audio mixer   ) Cap=00000000 Ctrl=00000000 -- Conns: 0=3 1=11
VHDevice NID=14 Config=00000000 (audio mixer   ) Cap=00000000 Ctrl=00000000 -- Conns: 0=4 1=11
VHDevice NID=15 Config=00000000 (audio mixer   ) Cap=00000000 Ctrl=00000000 -- Conns: 0=5 1=11
VHDevice NID=16 Config=00000000 (audio output  ) Cap=00000000 Ctrl=00000000 -- Conns:
VHDevice NID=17 Config=40130000 (pin: Speaker () Cap=00000010 Ctrl=00000040 -- Conns: 0=16
VHDevice NID=18 Config=411111f0 (pin: Speaker () Cap=00000020 Ctrl=00000000 -- Conns:
VHDevice NID=19 Config=00000000 (vendor widget ) Cap=00000000 Ctrl=00000000 -- Conns:
VHDevice NID=20 Config=01014010 (pin: Line-out ) Cap=0001003c Ctrl=00000020 -- Conns: 0=12 1=13 2=14 3=15 4=38
VHDevice NID=21 Config=01011012 (pin: Line-out ) Cap=0000003c Ctrl=00000020 -- Conns: 0=12 1=13 2=14 3=15 4=38
VHDevice NID=22 Config=01016011 (pin: Line-out ) Cap=0000003c Ctrl=00000020 -- Conns: 0=12 1=13 2=14 3=15 4=38
VHDevice NID=23 Config=41012014 (pin: Line-out ) Cap=0000003c Ctrl=00000020 -- Conns: 0=12 1=13 2=14 3=15 4=38
VHDevice NID=24 Config=01a19040 (pin: Microphon) Cap=0000373c Ctrl=00000021 -- Conns: 0=12 1=13 2=14 3=15 4=38
VHDevice NID=25 Config=02a19050 (pin: Microphon) Cap=0000373c Ctrl=00000020 -- Conns: 0=12 1=13 2=14 3=15 4=38
VHDevice NID=26 Config=01813060 (pin: Line-in () Cap=0000373c Ctrl=00000020 -- Conns: 0=12 1=13 2=14 3=15 4=38
VHDevice NID=27 Config=0221401f (pin: Headphone) Cap=0001373c Ctrl=00000020 -- Conns: 0=12 1=13 2=14 3=15 4=38
VHDevice NID=28 Config=411111f0 (pin: Speaker () Cap=00000024 Ctrl=00000020 -- Conns:
VHDevice NID=29 Config=00000000 (beep widget   ) Cap=00000000 Ctrl=00000000 -- Conns:
VHDevice NID=30 Config=41441130 (pin: SPDIF-out) Cap=00000010 Ctrl=00000040 -- Conns: 0=6
VHDevice NID=31 Config=41c46170 (pin: SPDIF-in ) Cap=00000020 Ctrl=00000020 -- Conns:
VHDevice NID=32 Config=00000000 (vendor widget ) Cap=00000000 Ctrl=00000000 -- Conns:
VHDevice NID=33 Config=00000000 (vendor widget ) Cap=00000000 Ctrl=00000000 -- Conns:
VHDevice NID=34 Config=00000000 (audio mixer   ) Cap=00000000 Ctrl=00000000 -- Conns: 0=24 1=25 2=26 3=27 4=28 5=29 6=20 7=21 8=22 9=23 10=11
VHDevice NID=35 Config=00000000 (audio mixer   ) Cap=00000000 Ctrl=00000000 -- Conns: 0=24 1=25 2=26 3=27 4=28 5=29 6=20 7=21 8=22 9=23 10=11
VHDevice NID=36 Config=00000000 (audio selector) Cap=00000000 Ctrl=00000000 -- Conns: 0=24 1=25 2=26 3=27 4=28 5=29 6=20 7=21 8=22 9=23 10=11 11=18
VHDevice NID=37 Config=00000000 (audio output  ) Cap=00000000 Ctrl=00000000 -- Conns:
VHDevice NID=38 Config=00000000 (audio mixer   ) Cap=00000000 Ctrl=00000000 -- Conns: 0=37 1=11
Parsing Ctls...
Disabling nonaudio...
Disabling useless...
 Disabling control 15 nid 23 cnid -1 due to disabled widget.
 Disabling control 28 nid 34 cnid 28 due to disabled widget.
 Disabling control 33 nid 34 cnid 23 due to disabled widget.
 Disabling control 38 nid 35 cnid 28 due to disabled widget.
 Disabling control 43 nid 35 cnid 23 due to disabled widget.
 Disabling nid 10 connection 0 due to disabled child widget.
 Disabling nid 12 connection 1 due to disabled child widget.
 Disabling nid 13 connection 1 due to disabled child widget.
 Disabling nid 14 connection 1 due to disabled child widget.
 Disabling nid 15 connection 1 due to disabled child widget.
 Disabling nid 34 connection 10 due to disabled child widget.
 Disabling nid 35 connection 10 due to disabled child widget.
 Disabling nid 36 connection 4 due to disabled child widget.
 Disabling nid 36 connection 9 due to disabled child widget.
 Disabling nid 36 connection 10 due to disabled child widget.
 Disabling nid 36 connection 11 due to disabled child widget.
 Disabling nid 38 connection 1 due to disabled child widget.
Patched pins configuration:
 nid 17 0x40130000 as  0 seq  0 Speaker       None  ATAPI   N/A     External Unknown misc 0 [DISABLED]
 nid 18 0x411111f0 as 15 seq  0 Speaker       None  1/8     Rear    External Black   misc 0 NoPresenceDetect [DISABLED]
 nid 20 0x01014010 as  1 seq  0 Line-out      Jack  1/8     Rear    External Green   misc 0
 nid 21 0x01011012 as  1 seq  2 Line-out      Jack  1/8     Rear    External Black   misc 0
 nid 22 0x01016011 as  1 seq  1 Line-out      Jack  1/8     Rear    External Orange  misc 0
 nid 23 0x41012014 as  1 seq  4 Line-out      None  1/8     Rear    External Grey    misc 0 [DISABLED]
 nid 24 0x01a19040 as  4 seq  0 Microphone    Jack  1/8     Rear    External Pink    misc 0
 nid 25 0x02a19050 as  5 seq  0 Microphone    Jack  1/8     Front   External Pink    misc 0
 nid 26 0x01813060 as  6 seq  0 Line-in       Jack  1/8     Rear    External Blue    misc 0
 nid 27 0x0221401f as  1 seq 15 Headphones    Jack  1/8     Front   External Green   misc 0
 nid 28 0x411111f0 as 15 seq  0 Speaker       None  1/8     Rear    External Black   misc 0 NoPresenceDetect [DISABLED]
 nid 30 0x41441130 as  3 seq  0 SPDIF-out     None  RCA     Rear    External Black   misc 0 NoPresenceDetect [DISABLED]
 nid 31 0x41c46170 as  7 seq  0 SPDIF-in      None  RCA     Rear    External Orange  misc 0 NoPresenceDetect [DISABLED]
Parsing pin associations...
4 associations found:
Association 0 (1) out:
 Pin nid=20 seq=0
 Pin nid=22 seq=1
 Pin nid=21 seq=2
 Pin nid=27 seq=15
   Redir type=0 jack=15 def=0
Association 1 (4) in:
 Pin nid=24 seq=0
   Redir type=-1 jack=0 def=0
Association 2 (5) in:
 Pin nid=25 seq=0
   Redir type=-1 jack=0 def=0
Association 3 (6) in:
 Pin nid=26 seq=0
   Redir type=-1 jack=0 def=0
Building AFG tree...
Tracing association 0 (1)
 Tracing pin 20 with min nid 0
    nid 2 returned 2
   nid 12 returned 2
    nid 3 returned 3
   nid 13 returned 3
    nid 4 returned 4
   nid 14 returned 4
    nid 5 returned 5
   nid 15 returned 5
    nid 37 returned 37
   nid 38 returned 37
  nid 20 returned 2
 Pin 20 traced to DAC 2
 Tracing pin 22 with min nid 0
   nid 12 busy by seqmask 1
    nid 3 returned 3
   nid 13 returned 3
    nid 4 returned 4
   nid 14 returned 4
    nid 5 returned 5
   nid 15 returned 5
    nid 37 returned 37
   nid 38 returned 37
  nid 22 returned 3
 Pin 22 traced to DAC 3
 Tracing pin 21 with min nid 0
   nid 12 busy by seqmask 1
   nid 13 busy by seqmask 2
    nid 4 returned 4
   nid 14 returned 4
    nid 5 returned 5
   nid 15 returned 5
    nid 37 returned 37
   nid 38 returned 37
  nid 21 returned 4
 Pin 21 traced to DAC 4
 Tracing pin 27 with min nid 0 and hpredir 0
    nid 2 returned 2
   nid 12 returned 2
  nid 27 returned 2
 Pin 27 traced to DAC 2 and hpredir 0
Association 0 (1) trace succeeded
Tracing association 1 (4)
 Tracing pin 24 to ADC 7
  tracing via nid 24
   tracing via nid 34
    tracing via nid 9
    nid 9 returned 0
   nid 34 returned 0
   tracing via nid 35
    tracing via nid 8
    nid 8 returned 0
   nid 35 returned 0
   tracing via nid 36
    tracing via nid 7
    nid 7 returned 1
   nid 36 returned 1
  nid 24 returned 1
 Pin 24 traced to ADC 7
Association 1 (4) trace succeeded
Tracing association 2 (5)
 Tracing pin 25 to ADC 8
  tracing via nid 25
   tracing via nid 34
    tracing via nid 9
    nid 9 returned 0
   nid 34 returned 0
   tracing via nid 35
    tracing via nid 8
    nid 8 returned 1
   nid 35 returned 1
   tracing via nid 36
   nid 36 busy by association 1
  nid 25 returned 1
 Pin 25 traced to ADC 8
Association 2 (5) trace succeeded
Tracing association 3 (6)
 Tracing pin 26 to ADC 9
  tracing via nid 26
   tracing via nid 34
    tracing via nid 9
    nid 9 returned 1
   nid 34 returned 1
   tracing via nid 35
   nid 35 busy by association 2
   tracing via nid 36
   nid 36 busy by association 1
  nid 26 returned 1
 Pin 26 traced to ADC 9
Association 3 (6) trace succeeded
Tracing input monitor
 Tracing nid mix 34 to out
  tracing via nid 34
   tracing via nid 9
   nid 9 busy by input association 3
  nid 34 returned 0
 Tracing nid mix 35 to out
  tracing via nid 35
   tracing via nid 8
   nid 8 busy by input association 2
  nid 35 returned 0
Tracing other input monitors
 Tracing nid complex 24 to out
  tracing via nid 24
   tracing via nid 34
   nid 34 busy by input association 3
   tracing via nid 35
   nid 35 busy by input association 2
   tracing via nid 36
   nid 36 busy by input association 1
  nid 24 returned 0
 Tracing nid complex 25 to out
  tracing via nid 25
   tracing via nid 34
   nid 34 busy by input association 3
   tracing via nid 35
   nid 35 busy by input association 2
   tracing via nid 36
   nid 36 busy by input association 1
  nid 25 returned 0
 Tracing nid complex 26 to out
  tracing via nid 26
   tracing via nid 34
   nid 34 busy by input association 3
   tracing via nid 35
   nid 35 busy by input association 2
   tracing via nid 36
   nid 36 busy by input association 1
  nid 26 returned 0
Tracing beeper
 Tracing nid 29 to out
  tracing via nid 29
   tracing via nid 34
   nid 34 busy by input association 3
   tracing via nid 35
   nid 35 busy by input association 2
   tracing via nid 36
   nid 36 busy by input association 1
  nid 29 returned 0
Disabling unassociated widgets...
Disabling nonselected inputs...
Disabling useless...
 Disabling control 10 nid 15 cnid -1 due to disabled widget.
 Disabling control 11 nid 15 cnid 5 due to disabled widget.
 Disabling control 44 nid 38 cnid -1 due to disabled widget.
 Disabling control 45 nid 38 cnid 37 due to disabled widget.
Disabling crossassociated connections...
Disabling useless...
Binding associations to channels...
Assigning names to signal sources...
Assigning mixers to the tree...
Preparing pin controls...
AFG commit...
Creating PCM devices...
pcmAttach: HDA Realtek ALC899 PCM #0 Analog at cad 1 nid 1
+--------------------------------------+
| DUMPING PCM Playback/Record Channels |
+--------------------------------------+

Playback:

     Stream cap: 0x00000001
                 PCM
        PCM cap: 0x000e05e0
                 16 20 24 bits, 44 48 88 96 192 KHz
            DAC: 2 3 4

Record:

     Stream cap: 0x00000001
                 PCM
        PCM cap: 0x000e05e0
                 16 20 24 bits, 44 48 88 96 192 KHz
            ADC: 7

+-------------------------------+
| DUMPING Playback/Record Paths |
+-------------------------------+

Playback:

    nid=20 [pin: Line-out (Green Rear)]
      |
      + <- nid=12 [audio mixer] [src: mix] bindSeq=00008001

             |
             + <- nid=2 [audio output] [src: pcm] bindSeq=00008001


    nid=22 [pin: Line-out (Orange Rear)]
      |
      + <- nid=13 [audio mixer] [src: mix] bindSeq=00000002

             |
             + <- nid=3 [audio output] [src: pcm] bindSeq=00000002


    nid=21 [pin: Line-out (Black Rear)]
      |
      + <- nid=14 [audio mixer] [src: mix] bindSeq=00000004

             |
             + <- nid=4 [audio output] [src: pcm] bindSeq=00000004


    nid=27 [pin: Headphones (Green Front)]
      |
      + <- nid=12 [audio mixer] [src: mix] bindSeq=00008001

             |
             + <- nid=2 [audio output] [src: pcm] bindSeq=00008001


Record:

    nid=7 [audio input]
      |
      + <- nid=36 [audio selector] [src: speaker, mic] bindSeq=00000001

             |
             + <- nid=24 [pin: Microphone (Pink Rear)] [src: mic] bindSeq=00000001

             + <- nid=29 [beep widget]

Input Mix:

    nid=12 [audio mixer]
      |
      + <- nid=2 [audio output] [src: pcm] bindSeq=00008001


    nid=13 [audio mixer]
      |
      + <- nid=3 [audio output] [src: pcm] bindSeq=00000002


    nid=14 [audio mixer]
      |
      + <- nid=4 [audio output] [src: pcm] bindSeq=00000004


    nid=34 [audio mixer]
      |
      + <- nid=26 [pin: Line-in (Blue Rear)] [src: line] bindSeq=00000001

      + <- nid=29 [beep widget]

    nid=35 [audio mixer]
      |
      + <- nid=25 [pin: Microphone (Pink Front)] [src: monitor] bindSeq=00000001

      + <- nid=29 [beep widget]

+-------------------------+
| DUMPING Volume Controls |
+-------------------------+

Master Volume (OSS: vol)
   |
   +- control  4 (nid  12 out):    dir - out oss: vol, mix -65/+0dB (88 steps)
   +- control  5 (nid  12 in   0): dir - out oss: vol, pcm mute
   +- control  6 (nid  13 out):    dir - out oss: vol, mix -65/+0dB (88 steps)
   +- control  7 (nid  13 in   0): dir - out oss: vol, pcm mute
   +- control  8 (nid  14 out):    dir - out oss: vol, mix -65/+0dB (88 steps)
   +- control  9 (nid  14 in   0): dir - out oss: vol, pcm mute
   +- control 12 (nid  20 out):    dir - out oss: vol, mix mute
   +- control 13 (nid  21 out):    dir - out oss: vol, mix mute
   +- control 14 (nid  22 out):    dir - out oss: vol, mix mute
   +- control 22 (nid  27 out):    dir - out oss: vol, mix mute

PCM Volume (OSS: pcm)
   |
   +- control  5 (nid  12 in   0): dir - out oss: vol, pcm mute
   +- control  7 (nid  13 in   0): dir - out oss: vol, pcm mute
   +- control  9 (nid  14 in   0): dir - out oss: vol, pcm mute

Microphone Volume (OSS: mic)
   |
   +- control 17 (nid  24 in   0): dir - in oss: mic +0/+30dB (4 steps)

Recording Level (OSS: rec)
   |
   +- control  1 (nid   7 in   0): dir - in oss: rec -17/+30dB (64 steps) + mute

Input Mix Level (OSS: mix)
   |
   +- control  4 (nid  12 out):    dir - out oss: vol, mix -65/+0dB (88 steps)
   +- control  6 (nid  13 out):    dir - out oss: vol, mix -65/+0dB (88 steps)
   +- control  8 (nid  14 out):    dir - out oss: vol, mix -65/+0dB (88 steps)
   +- control 12 (nid  20 out):    dir - out oss: vol, mix mute
   +- control 13 (nid  21 out):    dir - out oss: vol, mix mute
   +- control 14 (nid  22 out):    dir - out oss: vol, mix mute
   +- control 22 (nid  27 out):    dir - out oss: vol, mix mute

OSS mixer initialization...
Recsel (line, mic, cd, monitor): nid 36 source 0 select
Registering PCM channels...
pcmAttach: HDA Realtek ALC899 PCM #1 Analog at cad 1 nid 1
+--------------------------------------+
| DUMPING PCM Playback/Record Channels |
+--------------------------------------+

Record:

     Stream cap: 0x00000001
                 PCM
        PCM cap: 0x000e05e0
                 16 20 24 bits, 44 48 88 96 192 KHz
            ADC: 8

+-------------------------------+
| DUMPING Playback/Record Paths |
+-------------------------------+

Record:

    nid=8 [audio input]
      |
      + <- nid=35 [audio mixer] [src: mix] bindSeq=00000001

             |
             + <- nid=25 [pin: Microphone (Pink Front)] [src: monitor] bindSeq=00000001

             + <- nid=29 [beep widget]

+-------------------------+
| DUMPING Volume Controls |
+-------------------------+

Microphone2 Volume (OSS: monitor)
   |
   +- control 19 (nid  25 in   0): dir - in oss: monitor +0/+30dB (4 steps)
   +- control 35 (nid  35 in   1): dir - in oss: rec, monitor mute

Speaker/Beep Volume (OSS: speaker)
   |
   +- control 39 (nid  35 in   5): dir - in oss: speaker, rec mute

Recording Level (OSS: rec)
   |
   +- control  2 (nid   8 in   0): dir - in oss: mix, rec -17/+30dB (64 steps) + mute
   +- control 35 (nid  35 in   1): dir - in oss: rec, monitor mute
   +- control 39 (nid  35 in   5): dir - in oss: speaker, rec mute

Input Mix Level (OSS: mix)
   |
   +- control  2 (nid   8 in   0): dir - in oss: mix, rec -17/+30dB (64 steps) + mute

OSS mixer initialization...
Registering PCM channels...
pcmAttach: HDA Realtek ALC899 PCM #2 Analog at cad 1 nid 1
+--------------------------------------+
| DUMPING PCM Playback/Record Channels |
+--------------------------------------+

Record:

     Stream cap: 0x00000001
                 PCM
        PCM cap: 0x000e05e0
                 16 20 24 bits, 44 48 88 96 192 KHz
            ADC: 9

+-------------------------------+
| DUMPING Playback/Record Paths |
+-------------------------------+

Record:

    nid=9 [audio input]
      |
      + <- nid=34 [audio mixer] [src: mix] bindSeq=00000001

             |
             + <- nid=26 [pin: Line-in (Blue Rear)] [src: line] bindSeq=00000001

             + <- nid=29 [beep widget]

+-------------------------+
| DUMPING Volume Controls |
+-------------------------+

Line-in Volume (OSS: line)
   |
   +- control 21 (nid  26 in   0): dir - in oss: line +0/+30dB (4 steps)
   +- control 26 (nid  34 in   2): dir - in oss: line, rec mute

Speaker/Beep Volume (OSS: speaker)
   |
   +- control 29 (nid  34 in   5): dir - in oss: speaker, rec mute

Recording Level (OSS: rec)
   |
   +- control  3 (nid   9 in   0): dir - in oss: mix, rec -17/+30dB (64 steps) + mute
   +- control 26 (nid  34 in   2): dir - in oss: line, rec mute
   +- control 29 (nid  34 in   5): dir - in oss: speaker, rec mute

Input Mix Level (OSS: mix)
   |
   +- control  3 (nid   9 in   0): dir - in oss: mix, rec -17/+30dB (64 steps) + mute

OSS mixer initialization...
Registering PCM channels...
FG config/quirks: forcestereo ivref50 ivref80 ivref100 ivref
HP switch init...

+-------------------+
| DUMPING HDA NODES |
+-------------------+

Default Parameter
-----------------
     Stream cap: 0x00000001
                 PCM
        PCM cap: 0x000e05f0
                 16 20 24 bits, 32 44 48 88 96 192 KHz
         IN amp: 0x00000000
        OUT amp: 0x00000000

            nid: 2
           Name: audio output
     Widget cap: 0x00000411
                 PWR FORMAT_OVR STEREO
    Association: 0 (0x00008001)
            OSS: pcm (pcm)
     Stream cap: 0x00000001
                 PCM
        PCM cap: 0x000e05e0
                 16 20 24 bits, 44 48 88 96 192 KHz

            nid: 3
           Name: audio output
     Widget cap: 0x00000411
                 PWR FORMAT_OVR STEREO
    Association: 0 (0x00000002)
            OSS: pcm (pcm)
     Stream cap: 0x00000001
                 PCM
        PCM cap: 0x000e05e0
                 16 20 24 bits, 44 48 88 96 192 KHz

            nid: 4
           Name: audio output
     Widget cap: 0x00000411
                 PWR FORMAT_OVR STEREO
    Association: 0 (0x00000004)
            OSS: pcm (pcm)
     Stream cap: 0x00000001
                 PCM
        PCM cap: 0x000e05e0
                 16 20 24 bits, 44 48 88 96 192 KHz

            nid: 5 [DISABLED]
           Name: audio output
     Widget cap: 0x00000411
                 PWR FORMAT_OVR STEREO
     Stream cap: 0x00000001
                 PCM
        PCM cap: 0x000e05e0
                 16 20 24 bits, 44 48 88 96 192 KHz

            nid: 6 [DISABLED]
           Name: audio output
     Widget cap: 0x00000611
                 PWR DIGITAL FORMAT_OVR STEREO
     Stream cap: 0x00000001
                 PCM
        PCM cap: 0x000e05f0
                 16 20 24 bits, 32 44 48 88 96 192 KHz

            nid: 7
           Name: audio input
     Widget cap: 0x0010051b
                 PWR FORMAT_OVR AMP_OVR IN_AMP STEREO
    Association: 1 (0x00000001)
     Stream cap: 0x00000001
                 PCM
        PCM cap: 0x000e05e0
                 16 20 24 bits, 44 48 88 96 192 KHz
      Input amp: 0x80023f17
                 mute=1 step=63 size=2 offset=23
      Input val: [0x39 0x39] 
    connections: 1 enabled 1
          |
          + <- nid=36 [audio selector]

            nid: 8
           Name: audio input
     Widget cap: 0x0010051b
                 PWR FORMAT_OVR AMP_OVR IN_AMP STEREO
    Association: 2 (0x00000001)
     Stream cap: 0x00000001
                 PCM
        PCM cap: 0x000e05e0
                 16 20 24 bits, 44 48 88 96 192 KHz
      Input amp: 0x80023f17
                 mute=1 step=63 size=2 offset=23
      Input val: [0x33 0x33] 
    connections: 1 enabled 1
          |
          + <- nid=35 [audio mixer]

            nid: 9
           Name: audio input
     Widget cap: 0x0010051b
                 PWR FORMAT_OVR AMP_OVR IN_AMP STEREO
    Association: 3 (0x00000001)
     Stream cap: 0x00000001
                 PCM
        PCM cap: 0x000e05e0
                 16 20 24 bits, 44 48 88 96 192 KHz
      Input amp: 0x80023f17
                 mute=1 step=63 size=2 offset=23
      Input val: [0x33 0x33] 
    connections: 1 enabled 1
          |
          + <- nid=34 [audio mixer]

            nid: 10 [DISABLED]
           Name: audio input
     Widget cap: 0x00100791
                 PWR DIGITAL UNSOL FORMAT_OVR STEREO
     Stream cap: 0x00000001
                 PCM
        PCM cap: 0x000e0570
                 16 20 24 bits, 32 44 48 96 192 KHz
    connections: 1 enabled 0
          |
          + [DISABLED] <- nid=31 [pin: SPDIF-in (None)] [DISABLED]

            nid: 11 [DISABLED]
           Name: audio mixer
     Widget cap: 0x0020010b
                 AMP_OVR IN_AMP STEREO
      Input amp: 0x80051f17
                 mute=1 step=31 size=5 offset=23
      Input val: [0x97 0x97] [0x97 0x97] [0x97 0x97] [0x97 0x97] [0x97 0x97] [0x97 0x97] [0x97 0x97] [0x97 0x97] [0x97 0x97] [0x97 0x97] 
    connections: 10 enabled 10
          |
          + <- nid=24 [pin: Microphone (Pink Rear)]
          + <- nid=25 [pin: Microphone (Pink Front)]
          + <- nid=26 [pin: Line-in (Blue Rear)]
          + <- nid=27 [pin: Headphones (Green Front)]
          + <- nid=28 [pin: Speaker (None)] [DISABLED]
          + <- nid=29 [beep widget]
          + <- nid=20 [pin: Line-out (Green Rear)]
          + <- nid=21 [pin: Line-out (Black Rear)]
          + <- nid=22 [pin: Line-out (Orange Rear)]
          + <- nid=23 [pin: Line-out (None)] [DISABLED]

            nid: 12
           Name: audio mixer
     Widget cap: 0x0020010f
                 AMP_OVR OUT_AMP IN_AMP STEREO
    Association: 0 (0x00008001)
            OSS: mix (mix)
     Output amp: 0x00025757
                 mute=0 step=87 size=2 offset=87
     Output val: [0x3F 0x3F]
      Input amp: 0x80000000
                 mute=1 step=0 size=0 offset=0
      Input val: [0x00 0x00] [0x80 0x80] 
    connections: 2 enabled 1
          |
          + <- nid=2 [audio output]
          + [DISABLED] <- nid=11 [audio mixer] [DISABLED]

            nid: 13
           Name: audio mixer
     Widget cap: 0x0020010f
                 AMP_OVR OUT_AMP IN_AMP STEREO
    Association: 0 (0x00000002)
            OSS: mix (mix)
     Output amp: 0x00025757
                 mute=0 step=87 size=2 offset=87
     Output val: [0x3F 0x3F]
      Input amp: 0x80000000
                 mute=1 step=0 size=0 offset=0
      Input val: [0x00 0x00] [0x80 0x80] 
    connections: 2 enabled 1
          |
          + <- nid=3 [audio output]
          + [DISABLED] <- nid=11 [audio mixer] [DISABLED]

            nid: 14
           Name: audio mixer
     Widget cap: 0x0020010f
                 AMP_OVR OUT_AMP IN_AMP STEREO
    Association: 0 (0x00000004)
            OSS: mix (mix)
     Output amp: 0x00025757
                 mute=0 step=87 size=2 offset=87
     Output val: [0x3F 0x3F]
      Input amp: 0x80000000
                 mute=1 step=0 size=0 offset=0
      Input val: [0x00 0x00] [0x80 0x80] 
    connections: 2 enabled 1
          |
          + <- nid=4 [audio output]
          + [DISABLED] <- nid=11 [audio mixer] [DISABLED]

            nid: 15 [DISABLED]
           Name: audio mixer
     Widget cap: 0x0020010f
                 AMP_OVR OUT_AMP IN_AMP STEREO
     Output amp: 0x00025757
                 mute=0 step=87 size=2 offset=87
     Output val: [0x00 0x00]
      Input amp: 0x80000000
                 mute=1 step=0 size=0 offset=0
      Input val: [0x80 0x80] [0x80 0x80] 
    connections: 2 enabled 1
          |
          + <- nid=5 [audio output] [DISABLED]
          + [DISABLED] <- nid=11 [audio mixer] [DISABLED]

            nid: 16 [DISABLED]
           Name: audio output
     Widget cap: 0x00000611
                 PWR DIGITAL FORMAT_OVR STEREO
     Stream cap: 0x00000001
                 PCM
        PCM cap: 0x000e05f0
                 16 20 24 bits, 32 44 48 88 96 192 KHz

            nid: 17 [DISABLED]
           Name: pin: Speaker (None)
     Widget cap: 0x00400701
                 PWR DIGITAL STEREO
        Pin cap: 0x00000010
                 OUT
     Pin config: 0x40130000
    Pin control: 0x00000000
    connections: 1 enabled 1
          |
          + <- nid=16 [audio output] [DISABLED]

            nid: 18 [DISABLED]
           Name: pin: Speaker (None)
     Widget cap: 0x00400401
                 PWR STEREO
        Pin cap: 0x00000020
                 IN
     Pin config: 0x411111f0
    Pin control: 0x00000000

            nid: 19 [DISABLED]
           Name: vendor widget
     Widget cap: 0x00f00000

            nid: 20
           Name: pin: Line-out (Green Rear)
     Widget cap: 0x0040058d
                 PWR UNSOL AMP_OVR OUT_AMP STEREO
    Association: 0 (0x00000001)
        Pin cap: 0x0001003c
                 PDC HP OUT IN EAPD
     Pin config: 0x01014010
    Pin control: 0x00000040 OUT
           EAPD: 0x00000002
     Output amp: 0x80000000
                 mute=1 step=0 size=0 offset=0
     Output val: [0x00 0x00]
    connections: 5 enabled 1
          |
          + <- nid=12 [audio mixer] (selected)
          + [DISABLED] <- nid=13 [audio mixer]
          + [DISABLED] <- nid=14 [audio mixer]
          + [DISABLED] <- nid=15 [audio mixer] [DISABLED]
          + [DISABLED] <- nid=38 [audio mixer] [DISABLED]

            nid: 21
           Name: pin: Line-out (Black Rear)
     Widget cap: 0x0040058d
                 PWR UNSOL AMP_OVR OUT_AMP STEREO
    Association: 0 (0x00000004)
        Pin cap: 0x0000003c
                 PDC HP OUT IN
     Pin config: 0x01011012
    Pin control: 0x00000040 OUT
     Output amp: 0x80000000
                 mute=1 step=0 size=0 offset=0
     Output val: [0x00 0x00]
    connections: 5 enabled 1
          |
          + [DISABLED] <- nid=12 [audio mixer]
          + [DISABLED] <- nid=13 [audio mixer]
          + <- nid=14 [audio mixer] (selected)
          + [DISABLED] <- nid=15 [audio mixer] [DISABLED]
          + [DISABLED] <- nid=38 [audio mixer] [DISABLED]

            nid: 22
           Name: pin: Line-out (Orange Rear)
     Widget cap: 0x0040058d
                 PWR UNSOL AMP_OVR OUT_AMP STEREO
    Association: 0 (0x00000002)
        Pin cap: 0x0000003c
                 PDC HP OUT IN
     Pin config: 0x01016011
    Pin control: 0x00000040 OUT
     Output amp: 0x80000000
                 mute=1 step=0 size=0 offset=0
     Output val: [0x00 0x00]
    connections: 5 enabled 1
          |
          + [DISABLED] <- nid=12 [audio mixer]
          + <- nid=13 [audio mixer] (selected)
          + [DISABLED] <- nid=14 [audio mixer]
          + [DISABLED] <- nid=15 [audio mixer] [DISABLED]
          + [DISABLED] <- nid=38 [audio mixer] [DISABLED]

            nid: 23 [DISABLED]
           Name: pin: Line-out (None)
     Widget cap: 0x0040058d
                 PWR UNSOL AMP_OVR OUT_AMP STEREO
        Pin cap: 0x0000003c
                 PDC HP OUT IN
     Pin config: 0x41012014
    Pin control: 0x00000000
     Output amp: 0x80000000
                 mute=1 step=0 size=0 offset=0
     Output val: [0x80 0x80]
    connections: 5 enabled 5
          |
          + <- nid=12 [audio mixer] (selected)
          + <- nid=13 [audio mixer]
          + <- nid=14 [audio mixer]
          + <- nid=15 [audio mixer] [DISABLED]
          + <- nid=38 [audio mixer] [DISABLED]

            nid: 24
           Name: pin: Microphone (Pink Rear)
     Widget cap: 0x0040058f
                 PWR UNSOL AMP_OVR OUT_AMP IN_AMP STEREO
    Association: 1 (0x00000001)
            OSS: mic (mic)
        Pin cap: 0x0000373c
                 PDC HP OUT IN VREF[ 50 80 100 GROUND HIZ ]
     Pin config: 0x01a19040
    Pin control: 0x00000025 IN VREFs
     Output amp: 0x80000000
                 mute=1 step=0 size=0 offset=0
     Output val: [0x80 0x80]
      Input amp: 0x00270300
                 mute=0 step=3 size=39 offset=0
      Input val: [0x02 0x02] 
    connections: 5 enabled 0
          |
          + [DISABLED] <- nid=12 [audio mixer] (selected)
          + [DISABLED] <- nid=13 [audio mixer]
          + [DISABLED] <- nid=14 [audio mixer]
          + [DISABLED] <- nid=15 [audio mixer] [DISABLED]
          + [DISABLED] <- nid=38 [audio mixer] [DISABLED]

            nid: 25
           Name: pin: Microphone (Pink Front)
     Widget cap: 0x0040058f
                 PWR UNSOL AMP_OVR OUT_AMP IN_AMP STEREO
    Association: 2 (0x00000001)
            OSS: monitor (monitor)
        Pin cap: 0x0000373c
                 PDC HP OUT IN VREF[ 50 80 100 GROUND HIZ ]
     Pin config: 0x02a19050
    Pin control: 0x00000025 IN VREFs
     Output amp: 0x80000000
                 mute=1 step=0 size=0 offset=0
     Output val: [0x80 0x80]
      Input amp: 0x00270300
                 mute=0 step=3 size=39 offset=0
      Input val: [0x02 0x02] 
    connections: 5 enabled 0
          |
          + [DISABLED] <- nid=12 [audio mixer] (selected)
          + [DISABLED] <- nid=13 [audio mixer]
          + [DISABLED] <- nid=14 [audio mixer]
          + [DISABLED] <- nid=15 [audio mixer] [DISABLED]
          + [DISABLED] <- nid=38 [audio mixer] [DISABLED]

            nid: 26
           Name: pin: Line-in (Blue Rear)
     Widget cap: 0x0040058f
                 PWR UNSOL AMP_OVR OUT_AMP IN_AMP STEREO
    Association: 3 (0x00000001)
            OSS: line (line)
        Pin cap: 0x0000373c
                 PDC HP OUT IN VREF[ 50 80 100 GROUND HIZ ]
     Pin config: 0x01813060
    Pin control: 0x00000025 IN VREFs
     Output amp: 0x80000000
                 mute=1 step=0 size=0 offset=0
     Output val: [0x80 0x80]
      Input amp: 0x00270300
                 mute=0 step=3 size=39 offset=0
      Input val: [0x02 0x02] 
    connections: 5 enabled 0
          |
          + [DISABLED] <- nid=12 [audio mixer] (selected)
          + [DISABLED] <- nid=13 [audio mixer]
          + [DISABLED] <- nid=14 [audio mixer]
          + [DISABLED] <- nid=15 [audio mixer] [DISABLED]
          + [DISABLED] <- nid=38 [audio mixer] [DISABLED]

            nid: 27
           Name: pin: Headphones (Green Front)
     Widget cap: 0x0040058f
                 PWR UNSOL AMP_OVR OUT_AMP IN_AMP STEREO
    Association: 0 (0x00008000)
        Pin cap: 0x0001373c
                 PDC HP OUT IN VREF[ 50 80 100 GROUND HIZ ] EAPD
     Pin config: 0x0221401f
    Pin control: 0x000000c0 HP OUT
           EAPD: 0x00000002
     Output amp: 0x80000000
                 mute=1 step=0 size=0 offset=0
     Output val: [0x00 0x00]
      Input amp: 0x00270300
                 mute=0 step=3 size=39 offset=0
      Input val: [0x00 0x00] 
    connections: 5 enabled 1
          |
          + <- nid=12 [audio mixer] (selected)
          + [DISABLED] <- nid=13 [audio mixer]
          + [DISABLED] <- nid=14 [audio mixer]
          + [DISABLED] <- nid=15 [audio mixer] [DISABLED]
          + [DISABLED] <- nid=38 [audio mixer] [DISABLED]

            nid: 28 [DISABLED]
           Name: pin: Speaker (None)
     Widget cap: 0x00400481
                 PWR UNSOL STEREO
        Pin cap: 0x00000024
                 PDC IN
     Pin config: 0x411111f0
    Pin control: 0x00000000

            nid: 29
           Name: beep widget
     Widget cap: 0x00700400
                 PWR
    Association: -2 (0x00000000)
            OSS: speaker (speaker)

            nid: 30 [DISABLED]
           Name: pin: SPDIF-out (None)
     Widget cap: 0x00400701
                 PWR DIGITAL STEREO
        Pin cap: 0x00000010
                 OUT
     Pin config: 0x41441130
    Pin control: 0x00000000
    connections: 1 enabled 1
          |
          + <- nid=6 [audio output] [DISABLED]

            nid: 31 [DISABLED]
           Name: pin: SPDIF-in (None)
     Widget cap: 0x00400681
                 PWR DIGITAL UNSOL STEREO
        Pin cap: 0x00000020
                 IN
     Pin config: 0x41c46170
    Pin control: 0x00000000

            nid: 32 [DISABLED]
           Name: vendor widget
     Widget cap: 0x00f00040
                 PROC

            nid: 33 [DISABLED]
           Name: vendor widget
     Widget cap: 0x00f00000

            nid: 34
           Name: audio mixer
     Widget cap: 0x0020010b
                 AMP_OVR IN_AMP STEREO
    Association: 3 (0x00000001)
            OSS: mix (mix)
      Input amp: 0x80000000
                 mute=1 step=0 size=0 offset=0
      Input val: [0x80 0x80] [0x80 0x80] [0x00 0x00] [0x80 0x80] [0x80 0x80] [0x00 0x00] [0x80 0x80] [0x80 0x80] [0x80 0x80] [0x80 0x80] [0x80 0x80] 
    connections: 11 enabled 2
          |
          + [DISABLED] <- nid=24 [pin: Microphone (Pink Rear)]
          + [DISABLED] <- nid=25 [pin: Microphone (Pink Front)]
          + <- nid=26 [pin: Line-in (Blue Rear)]
          + [DISABLED] <- nid=27 [pin: Headphones (Green Front)]
          + [DISABLED] <- nid=28 [pin: Speaker (None)] [DISABLED]
          + <- nid=29 [beep widget]
          + [DISABLED] <- nid=20 [pin: Line-out (Green Rear)]
          + [DISABLED] <- nid=21 [pin: Line-out (Black Rear)]
          + [DISABLED] <- nid=22 [pin: Line-out (Orange Rear)]
          + [DISABLED] <- nid=23 [pin: Line-out (None)] [DISABLED]
          + [DISABLED] <- nid=11 [audio mixer] [DISABLED]

            nid: 35
           Name: audio mixer
     Widget cap: 0x0020010b
                 AMP_OVR IN_AMP STEREO
    Association: 2 (0x00000001)
            OSS: mix (mix)
      Input amp: 0x80000000
                 mute=1 step=0 size=0 offset=0
      Input val: [0x80 0x80] [0x00 0x00] [0x80 0x80] [0x80 0x80] [0x80 0x80] [0x00 0x00] [0x80 0x80] [0x80 0x80] [0x80 0x80] [0x80 0x80] [0x80 0x80] 
    connections: 11 enabled 2
          |
          + [DISABLED] <- nid=24 [pin: Microphone (Pink Rear)]
          + <- nid=25 [pin: Microphone (Pink Front)]
          + [DISABLED] <- nid=26 [pin: Line-in (Blue Rear)]
          + [DISABLED] <- nid=27 [pin: Headphones (Green Front)]
          + [DISABLED] <- nid=28 [pin: Speaker (None)] [DISABLED]
          + <- nid=29 [beep widget]
          + [DISABLED] <- nid=20 [pin: Line-out (Green Rear)]
          + [DISABLED] <- nid=21 [pin: Line-out (Black Rear)]
          + [DISABLED] <- nid=22 [pin: Line-out (Orange Rear)]
          + [DISABLED] <- nid=23 [pin: Line-out (None)] [DISABLED]
          + [DISABLED] <- nid=11 [audio mixer] [DISABLED]

            nid: 36
           Name: audio selector
     Widget cap: 0x00300101
                 STEREO
    Association: 1 (0x00000001)
            OSS: speaker, mic
    connections: 12 enabled 2
          |
          + <- nid=24 [pin: Microphone (Pink Rear)] (selected)
          + [DISABLED] <- nid=25 [pin: Microphone (Pink Front)]
          + [DISABLED] <- nid=26 [pin: Line-in (Blue Rear)]
          + [DISABLED] <- nid=27 [pin: Headphones (Green Front)]
          + [DISABLED] <- nid=28 [pin: Speaker (None)] [DISABLED]
          + <- nid=29 [beep widget]
          + [DISABLED] <- nid=20 [pin: Line-out (Green Rear)]
          + [DISABLED] <- nid=21 [pin: Line-out (Black Rear)]
          + [DISABLED] <- nid=22 [pin: Line-out (Orange Rear)]
          + [DISABLED] <- nid=23 [pin: Line-out (None)] [DISABLED]
          + [DISABLED] <- nid=11 [audio mixer] [DISABLED]
          + [DISABLED] <- nid=18 [pin: Speaker (None)] [DISABLED]

            nid: 37 [DISABLED]
           Name: audio output
     Widget cap: 0x00000411
                 PWR FORMAT_OVR STEREO
     Stream cap: 0x00000001
                 PCM
        PCM cap: 0x000e05e0
                 16 20 24 bits, 44 48 88 96 192 KHz

            nid: 38 [DISABLED]
           Name: audio mixer
     Widget cap: 0x0020010f
                 AMP_OVR OUT_AMP IN_AMP STEREO
     Output amp: 0x00025757
                 mute=0 step=87 size=2 offset=87
     Output val: [0x00 0x00]
      Input amp: 0x80000000
                 mute=1 step=0 size=0 offset=0
      Input val: [0x80 0x80] [0x80 0x80] 
    connections: 2 enabled 1
          |
          + <- nid=37 [audio output] [DISABLED]
          + [DISABLED] <- nid=11 [audio mixer] [DISABLED]
