00:00.0 Host bridge: Intel Corporation 2nd Generation Core Processor Family DRAM Controller (rev 09)
	Subsystem: CLEVO/KAPOK Computer Device 5102
	Flags: bus master, fast devsel, latency 0
	Capabilities: [e0] Vendor Specific Information: Len=0c <?>

00:01.0 PCI bridge: Intel Corporation Xeon E3-1200/2nd Generation Core Processor Family PCI Express Root Port (rev 09) (prog-if 00 [Normal decode])
	Flags: bus master, fast devsel, latency 0, IRQ 25
	Bus: primary=00, secondary=01, subordinate=01, sec-latency=0
	I/O behind bridge: 0000e000-0000efff
	Memory behind bridge: f7e00000-f7efffff
	Prefetchable memory behind bridge: 00000000e0000000-00000000efffffff
	Capabilities: [88] Subsystem: CLEVO/KAPOK Computer Device 5102
	Capabilities: [80] Power Management version 3
	Capabilities: [90] MSI: Enable+ Count=1/1 Maskable- 64bit-
	Capabilities: [a0] Express Root Port (Slot+), MSI 00
	Capabilities: [100] Virtual Channel
	Capabilities: [140] Root Complex Link
	Kernel driver in use: pcieport

00:16.0 Communication controller: Intel Corporation 6 Series/C200 Series Chipset Family MEI Controller #1 (rev 04)
	Subsystem: CLEVO/KAPOK Computer Device 5102
	Flags: bus master, fast devsel, latency 0, IRQ 11
	Memory at f7f0a000 (64-bit, non-prefetchable) [size=16]
	Capabilities: [50] Power Management version 3
	Capabilities: [8c] MSI: Enable- Count=1/1 Maskable- 64bit+

00:1a.0 USB controller: Intel Corporation 6 Series/C200 Series Chipset Family USB Enhanced Host Controller #2 (rev 05) (prog-if 20 [EHCI])
	Subsystem: CLEVO/KAPOK Computer Device 5102
	Flags: bus master, medium devsel, latency 0, IRQ 16
	Memory at f7f08000 (32-bit, non-prefetchable) [size=1K]
	Capabilities: [50] Power Management version 2
	Capabilities: [58] Debug port: BAR=1 offset=00a0
	Capabilities: [98] PCI Advanced Features
	Kernel driver in use: ehci-pci

00:1b.0 Audio device: Intel Corporation 6 Series/C200 Series Chipset Family High Definition Audio Controller (rev 05)
	Subsystem: CLEVO/KAPOK Computer Device 5102
	Flags: bus master, fast devsel, latency 0, IRQ 39
	Memory at f7f00000 (64-bit, non-prefetchable) [size=16K]
	Capabilities: [50] Power Management version 2
	Capabilities: [60] MSI: Enable+ Count=1/1 Maskable- 64bit+
	Capabilities: [70] Express Root Complex Integrated Endpoint, MSI 00
	Capabilities: [100] Virtual Channel
	Capabilities: [130] Root Complex Link
	Kernel driver in use: snd_hda_intel

00:1c.0 PCI bridge: Intel Corporation 6 Series/C200 Series Chipset Family PCI Express Root Port 1 (rev b5) (prog-if 00 [Normal decode])
	Flags: bus master, fast devsel, latency 0, IRQ 26
	Bus: primary=00, secondary=02, subordinate=02, sec-latency=0
	Memory behind bridge: f7d00000-f7dfffff
	Capabilities: [40] Express Root Port (Slot+), MSI 00
	Capabilities: [80] MSI: Enable+ Count=1/1 Maskable- 64bit-
	Capabilities: [90] Subsystem: CLEVO/KAPOK Computer Device 5102
	Capabilities: [a0] Power Management version 2
	Kernel driver in use: pcieport

00:1c.1 PCI bridge: Intel Corporation 6 Series/C200 Series Chipset Family PCI Express Root Port 2 (rev b5) (prog-if 00 [Normal decode])
	Flags: bus master, fast devsel, latency 0, IRQ 27
	Bus: primary=00, secondary=03, subordinate=03, sec-latency=0
	I/O behind bridge: 0000d000-0000dfff
	Memory behind bridge: f7c00000-f7cfffff
	Capabilities: [40] Express Root Port (Slot+), MSI 00
	Capabilities: [80] MSI: Enable+ Count=1/1 Maskable- 64bit-
	Capabilities: [90] Subsystem: CLEVO/KAPOK Computer Device 5102
	Capabilities: [a0] Power Management version 2
	Kernel driver in use: pcieport

00:1c.2 PCI bridge: Intel Corporation 6 Series/C200 Series Chipset Family PCI Express Root Port 3 (rev b5) (prog-if 00 [Normal decode])
	Flags: bus master, fast devsel, latency 0, IRQ 28
	Bus: primary=00, secondary=04, subordinate=04, sec-latency=0
	Memory behind bridge: f7b00000-f7bfffff
	Capabilities: [40] Express Root Port (Slot+), MSI 00
	Capabilities: [80] MSI: Enable+ Count=1/1 Maskable- 64bit-
	Capabilities: [90] Subsystem: CLEVO/KAPOK Computer Device 5102
	Capabilities: [a0] Power Management version 2
	Kernel driver in use: pcieport

00:1c.3 PCI bridge: Intel Corporation 6 Series/C200 Series Chipset Family PCI Express Root Port 4 (rev b5) (prog-if 00 [Normal decode])
	Flags: bus master, fast devsel, latency 0, IRQ 29
	Bus: primary=00, secondary=05, subordinate=05, sec-latency=0
	Memory behind bridge: f7a00000-f7afffff
	Capabilities: [40] Express Root Port (Slot+), MSI 00
	Capabilities: [80] MSI: Enable+ Count=1/1 Maskable- 64bit-
	Capabilities: [90] Subsystem: CLEVO/KAPOK Computer Device 5102
	Capabilities: [a0] Power Management version 2
	Kernel driver in use: pcieport

00:1d.0 USB controller: Intel Corporation 6 Series/C200 Series Chipset Family USB Enhanced Host Controller #1 (rev 05) (prog-if 20 [EHCI])
	Subsystem: CLEVO/KAPOK Computer Device 5102
	Flags: bus master, medium devsel, latency 0, IRQ 23
	Memory at f7f07000 (32-bit, non-prefetchable) [size=1K]
	Capabilities: [50] Power Management version 2
	Capabilities: [58] Debug port: BAR=1 offset=00a0
	Capabilities: [98] PCI Advanced Features
	Kernel driver in use: ehci-pci

00:1f.0 ISA bridge: Intel Corporation HM65 Express Chipset Family LPC Controller (rev 05)
	Subsystem: CLEVO/KAPOK Computer Device 5102
	Flags: bus master, medium devsel, latency 0
	Capabilities: [e0] Vendor Specific Information: Len=0c <?>
	Kernel driver in use: lpc_ich

00:1f.2 SATA controller: Intel Corporation 6 Series/C200 Series Chipset Family 6 port SATA AHCI Controller (rev 05) (prog-if 01 [AHCI 1.0])
	Subsystem: CLEVO/KAPOK Computer Device 5102
	Flags: bus master, 66MHz, medium devsel, latency 0, IRQ 30
	I/O ports at f070 [size=8]
	I/O ports at f060 [size=4]
	I/O ports at f050 [size=8]
	I/O ports at f040 [size=4]
	I/O ports at f020 [size=32]
	Memory at f7f06000 (32-bit, non-prefetchable) [size=2K]
	Capabilities: [80] MSI: Enable+ Count=1/1 Maskable- 64bit-
	Capabilities: [70] Power Management version 3
	Capabilities: [a8] SATA HBA v1.0
	Capabilities: [b0] PCI Advanced Features
	Kernel driver in use: ahci

00:1f.3 SMBus: Intel Corporation 6 Series/C200 Series Chipset Family SMBus Controller (rev 05)
	Subsystem: CLEVO/KAPOK Computer Device 5102
	Flags: medium devsel, IRQ 18
	Memory at f7f05000 (64-bit, non-prefetchable) [size=256]
	I/O ports at f000 [size=32]

01:00.0 VGA compatible controller: Advanced Micro Devices, Inc. [AMD/ATI] Blackcomb [Radeon HD 6970M/6990M] (prog-if 00 [VGA controller])
	Subsystem: CLEVO/KAPOK Computer Radeon HD 6970M
	Flags: bus master, fast devsel, latency 0, IRQ 42
	Memory at e0000000 (64-bit, prefetchable) [size=256M]
	Memory at f7e20000 (64-bit, non-prefetchable) [size=128K]
	I/O ports at e000 [size=256]
	Expansion ROM at f7e00000 [disabled] [size=128K]
	Capabilities: [50] Power Management version 3
	Capabilities: [58] Express Legacy Endpoint, MSI 00
	Capabilities: [a0] MSI: Enable+ Count=1/1 Maskable- 64bit+
	Capabilities: [100] Vendor Specific Information: ID=0001 Rev=1 Len=010 <?>
	Capabilities: [150] Advanced Error Reporting
	Kernel driver in use: radeon

01:00.1 Audio device: Advanced Micro Devices, Inc. [AMD/ATI] Barts HDMI Audio [Radeon HD 6800 Series]
	Subsystem: CLEVO/KAPOK Computer Device 5102
	Flags: bus master, fast devsel, latency 0, IRQ 40
	Memory at f7e40000 (64-bit, non-prefetchable) [size=16K]
	Capabilities: [50] Power Management version 3
	Capabilities: [58] Express Legacy Endpoint, MSI 00
	Capabilities: [a0] MSI: Enable+ Count=1/1 Maskable- 64bit+
	Capabilities: [100] Vendor Specific Information: ID=0001 Rev=1 Len=010 <?>
	Capabilities: [150] Advanced Error Reporting
	Kernel driver in use: snd_hda_intel

02:00.0 USB controller: NEC Corporation uPD720200 USB 3.0 Host Controller (rev 03) (prog-if 30 [XHCI])
	Subsystem: CLEVO/KAPOK Computer Device 5102
	Flags: bus master, fast devsel, latency 0, IRQ 16
	Memory at f7d00000 (64-bit, non-prefetchable) [size=8K]
	Capabilities: [50] Power Management version 3
	Capabilities: [70] MSI: Enable- Count=1/8 Maskable- 64bit+
	Capabilities: [90] MSI-X: Enable+ Count=8 Masked-
	Capabilities: [a0] Express Endpoint, MSI 00
	Capabilities: [100] Advanced Error Reporting
	Capabilities: [140] Device Serial Number ff-ff-ff-ff-ff-ff-ff-ff
	Capabilities: [150] Latency Tolerance Reporting
	Kernel driver in use: xhci_hcd

03:00.0 Ethernet controller: JMicron Technology Corp. JMC250 PCI Express Gigabit Ethernet Controller (rev 05)
	Subsystem: CLEVO/KAPOK Computer Device 5102
	Flags: bus master, fast devsel, latency 0, IRQ 43
	Memory at f7c20000 (32-bit, non-prefetchable) [size=16K]
	I/O ports at d100 [size=128]
	I/O ports at d000 [size=256]
	Memory at f7c10000 (32-bit, non-prefetchable) [size=64K]
	Expansion ROM at f7c00000 [disabled] [size=64K]
	Capabilities: [68] Power Management version 3
	Capabilities: [50] Express Legacy Endpoint, MSI 00
	Capabilities: [40] MSI-X: Enable- Count=8 Masked-
	Capabilities: [70] MSI: Enable+ Count=1/8 Maskable+ 64bit+
	Capabilities: [100] Device Serial Number 7e-6a-b7-ff-ff-f5-90-00
	Kernel driver in use: jme

03:00.1 System peripheral: JMicron Technology Corp. SD/MMC Host Controller (rev 90)
	Subsystem: CLEVO/KAPOK Computer Device 5102
	Flags: bus master, fast devsel, latency 0, IRQ 18
	Memory at f7c26000 (32-bit, non-prefetchable) [size=256]
	Capabilities: [a4] Power Management version 3
	Capabilities: [80] Express Endpoint, MSI 00
	Capabilities: [94] MSI: Enable- Count=1/1 Maskable- 64bit-
	Capabilities: [100] Device Serial Number 7e-6a-b7-ff-ff-f5-90-00
	Kernel driver in use: sdhci-pci

03:00.2 SD Host controller: JMicron Technology Corp. Standard SD Host Controller (rev 90) (prog-if 01)
	Subsystem: CLEVO/KAPOK Computer Device 5102
	Flags: fast devsel, IRQ 18
	Memory at f7c25000 (32-bit, non-prefetchable) [size=256]
	Capabilities: [a4] Power Management version 3
	Capabilities: [80] Express Endpoint, MSI 00
	Capabilities: [94] MSI: Enable- Count=1/1 Maskable- 64bit-
	Capabilities: [100] Device Serial Number 7e-6a-b7-ff-ff-f5-90-00

03:00.3 System peripheral: JMicron Technology Corp. MS Host Controller (rev 90)
	Subsystem: CLEVO/KAPOK Computer Device 5102
	Flags: bus master, fast devsel, latency 0, IRQ 18
	Memory at f7c24000 (32-bit, non-prefetchable) [size=256]
	Capabilities: [a4] Power Management version 3
	Capabilities: [80] Express Endpoint, MSI 00
	Capabilities: [94] MSI: Enable- Count=1/1 Maskable- 64bit-
	Capabilities: [100] Device Serial Number 7e-6a-b7-ff-ff-f5-90-00
	Kernel driver in use: jmb38x_ms

04:00.0 Network controller: Intel Corporation Centrino Advanced-N 6230 [Rainbow Peak] (rev 34)
	Subsystem: Intel Corporation Centrino Advanced-N 6230 AGN
	Flags: bus master, fast devsel, latency 0, IRQ 41
	Memory at f7b00000 (64-bit, non-prefetchable) [size=8K]
	Capabilities: [c8] Power Management version 3
	Capabilities: [d0] MSI: Enable+ Count=1/1 Maskable- 64bit+
	Capabilities: [e0] Express Endpoint, MSI 00
	Capabilities: [100] Advanced Error Reporting
	Capabilities: [140] Device Serial Number 88-53-2e-ff-ff-03-a2-5a
	Kernel driver in use: iwlwifi

05:00.0 FireWire (IEEE 1394): JMicron Technology Corp. IEEE 1394 Host Controller (rev 30) (prog-if 10 [OHCI])
	Subsystem: CLEVO/KAPOK Computer Device 5102
	Flags: bus master, fast devsel, latency 0, IRQ 19
	Memory at f7a01000 (32-bit, non-prefetchable) [size=2K]
	Memory at f7a00000 (32-bit, non-prefetchable) [size=256]
	Capabilities: [44] Power Management version 3
	Capabilities: [80] Express Endpoint, MSI 00
	Capabilities: [94] MSI: Enable- Count=1/1 Maskable- 64bit-
	Kernel driver in use: firewire_ohci

